Old version Thexder joystick patch for IIgs.




If you want to have a good joystick on the Thexder (old version), first make

a copy of the disk and use the backup disk, NOT the original disk.



Then make a patch as follows using the block editor:



Block $058D:  Byte $B9:9C 33 BC 78

              Byte $FD:9C 34 BC AF 70 C0 00 A0  30 AF 64 C0 00 10 03 EE

                       33 BC AF 65 C0 00 10 03  EE 34 BC 68 D0 EB 58

              Byte $CA:10

              Byte $D3:A8

              Byte $DF:10

              Byte $E6:A8

Block $059D:  Byte $28:02

              Byte $2C:33

              Byte $72:34

              Byte $77:23

              Byte $79:33

              Byte $7E:2C

              Byte $80:34



That's it!  Each time when you play the game, press J for joystick so you can

play the game smoothly.



Tom Beversdorf

  ______               __

    /                 /  )                     /       /)

 --/ __________      /--<  _ , __/> __  _   __/ __,_  // 

(_/ (_) / / / <_    /___/_</_\/ (__/ (_/_)_(_/_(_) (_//_

                                                    />

                                                   </ 

