KŠŠ BBS Hardware & Software

Hardware

- matična plošča: 486 DX2/66, 256kb cache
- 4Gb Quantum bigfoot HDD, EIDE
- 32 Mb RAM
- CD ROM IDE 8x
- Zyxel COM port card, UART 16550
- Zyxel 19.200 ext modem
- 3COM mrežna kartica 10Mb, Combo
- 1.44 FDD
- VLB Diamond Stelth 64 2 Mb DRAM

Software

- OS/2 WARP Connect 3.0
- FrontDoor 2.20c.mL/CS00023E; MultiLine
- RemoteAccess version 2.02/Professional (10 node)
- Communications driver: Ray Gwinn's double aught buckshot driver, VX00 1.35
  (Registered to: Uros Bizjak, KSS BBS)

Majan, v Škofji Loki dne 24/4/98