# Information

The mailbox is operated at present on a computer AMD K6/2-300 with 64 MT RAM. The used mailbox often commodity is NCB Mail . As a choice haven are available 2 ISDN connections. At these two USR Courier I, a USR Sportster Flash as well as a ZyXEL U-1496 E+ are attached. The box is under the following call numbers 24 hours on the day attainable:

Preselection | Call number | Modem/terminal adapter | Connecting kind | Standard | Speed
0341 | 4410685 | ZyXEL U-1496 E+ | similar | V.32 | 19200
0341 | 4410686 | USR Courier I | ISDN | X75 | 64000
0341 | 4410686 | USR Courier I | similar | V.90 | 56000
0341 | 4411737 | USR Sportster Flash | similar | V.34+ | 33600
0341 | 4411747 | USR Courier I | ISDN | X75 | 64000
0341 | 4411747 | USR Courier I | similar | V.90 | 56000

For the use one needs a terminal program, like e.g.. Terminate for DOS or Zoc for Windows. The entrance to the box takes place for the time being with the user name guest . For a problem-free use of all services a user request is necessary. Thus one keeps an adequate InterNet address in the form username@elektron.east to de and can immediately E-Mail and News use.

Are to the Usern over 14 GB Shareware, Freeware, driver, sound, demo, pictures and much more besides to the free Download at the disposal. The file lists of the box obtain an overview in addition.

The POINTS is available a large number of nets for reading and writing. A POINT mechanism is possible for at any time on-line in the mailbox. During the registration also a before-configured CROSS POINT is furnished to the Download. Thus an immediate start of the POINT enterprise is uncomplicatedly possible.

Subject to change | © 2000, electron BBS, Udo Bertholdt