--------------------------------------------------------------------------
Setup hints for using BGFAX with FD 2.11/SW                       11-14-93
B.J. Guillot
FidoNet 106/400                              InterNet: st1r8@jetson.uh.edu
--------------------------------------------------------------------------

Keep in mind that fax commands cannot be stored in NVRAM.

Here is the relevant information from FDSETUP ...

[FDSETUP] Modem -> Command Strings
  Init-1 ... atz|
  Init-2 ... at+fcr=1;+fdcc=1,5,0,2,0,0,0,0|
  Init-3 ... at+flid="713 555 1212"|

  +fcr=1                   enables fax receiption
  +flid="713 555 1212"     sets your FAX ID, up to 20 characters

  +fdcc=1,5,0,2,0,0,0,0    enable high resolution, 14400 fax
  +fdcc=1,3,0,2,0,0,0,0    enable high resolution, 9600 fax

Do not attempt to give a 9600 maximum speed send/receive fax modem the 1,5
string as it will cause unpredicable results.

[FDSETUP] Modem -> Answer control
  Manual answer    Yes
  Force answer ... at+faa=1;a|

The "at+faa=1;a" causes the modem to answer adaptively, i.e., to
automatically determine whether the incoming call is fax or data and return
the response to the modem.

[FDSETUP] Mailer -> Errorlevels
  Fax ... 255

==========================================================================

If you are using a modem such as a Supra that returns a "FAX" response
proceed with the following instructions ( METHOD #1 ) ...

[FDSETUP] Modem -> Default Settings -> Messages
   Fax ... FAX

FDRUN.BAT should contain something similar to ...

@echo off
c:
cd\fd
fd
if errorlevel 255 bgfax /fax c:\bgfax 1 z
if errorlevel 103 maint.bat
if errorlevel 102 toss.bat
if errorlevel 101 local.bat
if errorlevel 100 dobbs.bat

==========================================================================

If you are using a modem such as a PPI FXMT that returns a "+FCON" response
proceed with the following instructions ( METHOD #2 ) ...

[FDSETUP] Modem -> Messages
  Fax ... +FCON

FDRUN.BAT should contain something similar to ...

@echo off
c:
cd\fd
fd
if errorlevel 255 bgfax /fcon c:\bgfax 1 z
if errorlevel 103 maint.bat
if errorlevel 102 toss.bat
if errorlevel 101 local.bat
if errorlevel 100 dobbs.bat

If BGFAX fails to work properly, try using this line instead:

if errorlevel 255 bgfax /fast c:\bgfax 1 z

==========================================================================

Regards,
B.J. Guillot

