Released July 4th, 1993

ÕÍµ  4_Drive Utilities v1.0  ³  Multiple Port Address AT/IDE Drive Inquiry
³                                  ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿    ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³      Dustbowl Designs, Inc.      ³     0   MB     ³    ³     153 MB     ³
³    "Dedicated to enhancing the   ³ ðþðððððððððððð ³    ³ ð*ðððððððððððð ³
³    world's personal computers."  ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ    ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ
³       (405) 741-4705 Voice            Drive 0               Drive 1
³       (405) 741-2721 BBS              Port Address:  170 (secondary)
ÃÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³     Copyright 1993 by Dustbowl Designs, Inc. All rights reserved.       ³
³         12600 S.E. 38th Street, Choctaw, Oklahoma USA 73020-6107        ³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ

You are free to copy this software and distribute it to other users as
long as the archive file is distributed in its entirety with this text
file included in the archive.

ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³±±± Introduction ±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ
We've decided to release to the public a handy in-house AT/IDE inquiry
utility.  What's particularly useful about this rendition is that you
may talk to drives that are attached to either the Primary or
Secondary Port Addresses.  This ability dovetails nicely with our
3_Drives and DiskQwik shareware utilities. Also, we've emphasized the
newer Multiple Sectors, DMA and LBA transfer options that are soon to
be more generally available on AT/IDE drives.

The 4_Drive Utilities is designed to assist in the use of our
3/4_Drives and DiskQwik products by suggesting the command line
switches that these programs may use.  This utility also serves as a
basic AT/IDE Inquiry that can give you the Cylinder, Head, Sectors per
Track geometry used by your AT/IDE drive.

This inquiry is defined and works on AT/IDE  and ESDI interface
drives.

Plans for 4_Drive Utilities include MBR and Partition Record
preparation and analysis, Multiple Sectors transfer rate test and much
more.

ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³±±± Command Line Switches ±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ
This program will accept three basic command line switches.  If no
command line switches are placed, then the program will run
interactively, asking for which Port and which Drive:

 [P]rimary or [S]econdary:  s
         Drive [0] or [1]:  1

You can load this info up on the command line as: 4DRVUTIL s 1

Additionally, if you place the m on the command line, all hi-ASCII
bytes will be masked out of the hex data dump.  This is useful when
printing, as these characters can cause unpredictable results.

Example: 4DRVUTIL s 1 m >drive2-1.dat
(then hit the enter key a few times..) will create an ASCII file of
this program's output....

Drive/Controller Model:  My Drive MD-123A
Serial number:  00123456789000000000,   Controller firmware:  REV. AA
Cylinders:  969,    Heads:  9,    Sectors:  36
            DMA mode:  NOT AVAILABLE
            LBA mode:  NOT AVAILABLE
Multiple sector mode:  64 sector/interrupt max

switches: 3/4_Drives m0+ or m0 (either 64 or 32 sectors per interrupt)
            DiskQwik b064 rm0 wm0

Buffer size:  128 KBytes (256 sectors)
A dual ported multi-sectored buffer capable of simultaneous transfers with
a read caching capability.

Word Offset Data-----------------------------------  ASCII------------------
   0  0000  4A32 C903 0000 0900 9051 4402 2400 100C  J2 .. .. .. .Q D. $. ..
   8  0010  0B00 0F00 3030 3231 3433 3635 3837 3039  .. .. 00 21 43 65 87 09
  16  0020  3030 3030 3030 3030 0300 4000 0400 4552  00 00 00 00 .. @. .. ER
  24  0030  2E56 4120 2041 794D 4420 6972 6576 4D20  .V A   A yM D  ir ev M
  32  0040  2D44 3231 4133 2020 2020 2020 2020 2020  -D 21 A3

  40  0050  2020 2020 2020 2020 2020 2020 2020 0100                       ..
  48  0060  0000 0100 0000 0000 0000 0000 0000 0000  .. .. .. .. .. .. .. ..
  56  0070  0000 0000 0000 0000 0000 0000 0000 0000  .. .. .. .. .. .. .. ..
  64  0080  0000 0000 0000 0000 0000 0000 0000 0000  .. .. .. .. .. .. .. ..
etc.....etc

ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³±±± Outline ±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ
The structure of the 256 words (512 bytes) is as follows:

0   General configuration
1   cylinders (default xlat mode)
2   reserved... ESDI: Removables
3   heads (default xlat mode)
4   bytes per track (unformatted)
5   bytes per sector (unformatted)
6   sectors/track (default xlat mode) hi=reserved lo=SPT
7   IDE:vendor unique... ESDI: bytes intersector gap lo=ISG hi=index gap
8   IDE:vendor unique... ESDI: bytes in sync lo=PLO bytes hi=reserved
9   words unique status
10  serial number in ASCII 20 bytes
20  controller or buffer type
21  buffer size in 512 byte blocks
22  ECC bytes transferred in r/w long
23  firmware revision in ASCII 8 bytes
27  model number ID in ASCII 40 bytes
47  number of sectors/interrupt in multiple, 00h = not implemented
    bits 8-15 are vendor unique
48  double word transfer flag
49  capabilities...LBA and/or DMA
       0-7   vendor unique
       8     1=DMA supported
       9     1=LBA supported
       10-15 reserved
50  reserved...
51  PIO data xfer timing mode lo=vendor unique
52  DMA data xfer timing mode lo=vendor unique
53  translation mode valid for words 54-58, 1-15 is reserved
54  translation cylinders
55  translation heads
56  translation sectors/track
57  number of sectors - low
58  number of sectors - high
59  current multiple setting
       0-7  current SPT if multiple valid
       8    1=multiple sector valid
       9-15 reserved
60  LBA sectors - low
61  LBA sectors - high
62  single word DMA
63  multi word DMA
64  reserved
128 vendor unique data
160 to end= reserved

This section will be expanded in the next release!

ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³±±± Legal Disclaimer ±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ

                          LICENSE AGREEMENT

There is no registration requirement for this version of 4_Drive
Utilities.

4_Drive Utilities All versions.

Dustbowl Designs, Inc. provides  the accompanying object code software
("Software")  and nonexclusively  licenses  its  use on  the following
terms and conditions. The Software is copyrighted by Dustbowl Designs,
Inc. with all rights reserved.  YOU ASSUME FULL RESPONSIBILITY FOR THE
SELECTION OF THE  SOFTWARE TO ACHIEVE YOUR INTENDED  PURPOSES, FOR THE
PROPER INSTALLATION  AND USE. Dustbowl Designs,  Inc. DOES NOT WARRANT
THAT THE  SOFTWARE WILL MEET  YOUR REQUIREMENTS, THAT  THE SOFTWARE IS
FIT FOR ANY PARTICULAR PURPOSE OR THAT THE USE OF THE SOFTWARE WILL BE
ERROR FREE. Dustbowl Designs, Inc. EXPRESSLY DISCLAIMS ALL WARRANTIES,
WHETHER  ORAL  OR  WRITTEN,  EXPRESSED  OR  IMPLIED, INCLUDING WITHOUT
LIMITATION WARRANTIES  OF MERCHANTABILITY OR FITNESS  FOR A PARTICULAR
PURPOSE. IN  NO EVENT WILL  Dustbowl Designs, Inc.  BE LIABLE TO  YOU,
YOUR  CUSTOMERS   OR  OTHER  USERS   FOR  ANY  INDIRECT,   INCIDENTAL,
CONSEQUENTIAL,  SPECIAL  OR  EXEMPLARY  DAMAGES  ARISING  OUT OF OR IN
CONNECTION WITH THE USE OR INABILITY TO USE THE SOFTWARE.

3_Drives, 4_Drives and DiskQwik are a trademarks of Dustbowl  Designs,
Inc. The 4_Drive Utilities software and documentation are Copyright 1993 by
Dustbowl Designs with All Rights Reserved. The 3_Drives v3.0, 4_Drives
v3.0 and 4_Park v1.1 software programs ARE NOT shareware or freeware
and unauthorized redistribution is STRICTLY PROHIBITED.

End of License agreement.

*****************************************************************

ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³±±± Revision History ±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±±³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ

v1.0    07/93 - public release of Shareware 4_Drive Utilities v1.0.

Contents of the 4_Drives Utilities Distribution Set. 4DRVU100.ZIP
(4DRVU.ZIP on CompuServe (tm) go IBMHW forum Lib 1)

4DRVUTIL.EXE    An AT/IDE Identify Drive inquiry utility that shows
                which 3_Drive/4_Drive and DiskQwik command line
                switches work best. Designed to work on both Primary
                and Secondary Port Addresses.
4DRVUTIL.DOC    Auxiliary documentation.
DBOWLDEM.EXE    Simple demo that gives a look at registered
                4_Drives v3.0 and 4_Park v1.1, and our new DiskQwik
                programs.
VENDOR3.DOC     Shareware vendor distribution policy

All files dated 7-4-93 02:50:00.

========================

              ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
              ³              4_Drives and 3_Drives              ³
From the      ³  The Universal device driver that lets you add  ³
makers of:    ³  an additional 16-bit interface to your system. ³
              ³   Add up to two more MFM, RLL, ESDI, or AT/IDE  ³
              ³  Hard Disk Drives to a Secondary Port Address!  ³
              ³    Fast Disk I/O options registered versions.   ³
              ³                                                 ³
              ³                     DiskQwik                    ³
              ³   A utility that maximizes the speed potential  ³
              ³    of AT/IDE hard disk drives. Many newer IDE   ³
              ³   drives often have an untapped feature called  ³
              ³ "Multiple Sectors per Interrupt". By activating ³
              ³  this, you can increase the data transfer rate  ³
              ³       of your hard drive by up to 50% ....      ³
              ³                State of the Art!                ³
              ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ

Shareware versions of these programs are available at all better
BBS's!  If you can't find a copy locally, feel free to call our BBS.

Dustbowl Designs, Inc.          |
12300 S.E. 38th Street          |
Choctaw, Oklahoma  73020-6107   |
U.S.A.                          | CIS: 71062,2542

phone:
(405) 741-4705 ordering, tech support, general information
(405) 741-2721 BBS (9600 HST/v.everything) Tech Support, Hard disk
               drive shareware, drive specs, Online Shareware
               Registration/Download for VISA or MasterCard orders!

-= EOF 4DRVUTIL.DOC =-
