                                                     


Snooper, the system checker, version 3.10  Copyright 1989-93 John Vias         
+-----------------------------------------------+-----------------------------+
| Equipment                                     | Disk [abC]                  |
|                                               |                             |
| Computer Hexium compatible                    |        HAVIN SEX Label      |
|  CPU Hexium-12        Video VESA 1.2 SVGA 1.0M|         \COMMO\2 Directory  |
|  NDP internal         Ports S-Blaster         | Conner 120MB - C IDE model  |
|  Bus ISA               Serial 3F8 2F8         |       fixed disk Drive type |
| Memory                 Parallel 378           |               47 CMOS type  |
|  655,360 b Convl      BIOS  11/11/92          |            local Status     |
|  536,880 b Free        Exts C000              |                8 Heads      |
|  118,480 b Used       Mouse Microsoft 6.24    |               39 Sectrs/cyl |
|    3,072 K Extended    Port serial, COM1(3)   |              762 Cylinders  |
|          K Ext free   Keyboard 101 Support 101|              512 b Sectors  |
|    2,592 K XMS 3.0    Environment             |            2,048 b Clusters |
|     free HMA           Free 86    Total 256   |      121,131,008 b Total    |
|          K UMB        DOS MS-DOS 6.20a        |       30,398,464 b Free     |
|    2,480 K EMS 4.0     Shell VCPI 1.0         |       90,732,544 b Used 75% |
|    2,096 K EMS free    Files 8    Buffers 15  |  XXXXXXXXXXXXXXXXXXX______  |
| Drives                 Break off  Verify  off |  Empty      Half      Full  |
| 2 Floppy  3 Physical  Cache                   +-----------------------------+
| 1 Hard    3 Logical   Network                 | Message: Logging display    |
+-----------------------------------------------+-----------------------------+
Snooper running Sunday, February 26, 1995, at 3:23:18pm                        