
-----------------------------------------------------------------------------
***                Jolly Box v4.00 final Construction Plans               ***
***                      Latest revision: 1993-06-01                      ***
-----------------------------------------------------------------------------


                       THE CREATION OF THE
                ___  _                  _   _
                  | | | |   |   \_/ __ |_| | | \/
                \_| |_| |__ |__  |     |_| |_| /\

                           Created By:

                    ___          _
                      /_  //    /_)_  _  _  _
                   (_/(_)//(_/ / \(_)(_)(_'/
                            /       (_/


        Additional Programming and Hardware Improvements by:

                Zaphod Beeblebrox of Control Team/I.C.S.


                          Version  4.0 final


-----------------------------------------------------------------

    For Ideas Bugreports additional developements and changes
    we can be contacted on the following BBS's:

Eagles Nest:                               +46-18-262804
Nightbox:                                  +49-5861-8795

Jolly Roger understands both German and English, and I, Zaphod Beeblebrox
understands Swedish and English, and also a very little bit German. Just
feel free to contact any of us if you need help or just want to chat a bit!!
For ideas and Bugreports you can also contact [>SmEGmA<] at all well known
Amiga Elite-Boards

-----------------------------------------------------------------

                          General Info

The Jolly-Box is a hardware project realized by Jolly Roger. The first
version in release was v3.1, which I downloaded from a BBS. I started
thinking about making a more advanced version, and contacted Jolly Roger
about it, and here we are again, now with the German-Swedish Co product-
-ion of The Jolly-Box v4.0!!! All original hardware design was made by
Jolly Roger, as well as the main structures of the software for the 80C39
Intel CPU. The improvements to the hardware, and the programming for adding
all the new features to the v4.0 software was made by Zaphod Beeblebrox of
ICS/Control Team. The Jolly-Box is now the most advanced hardware box of
any kind, which plans are released to the public. We have included the
sourcecode for the CPU software, together with sources in GFA basic for
an assembler/dissassembler for 80C39, and software for calculating the
sine-wawe samples for the different tones. All of these GFA basic programs
were written by Jolly Roger on the Amiga, I only added some features for
compatibility with the Atari ST/STE series of computers. You'll find all
these sources in ASCII format also in this archive so that you can convert
them if you wanna use a Pc for example instead of an Atari or Amiga....
However, I must notify you of the fact that you'll have to find out what
trunk-frequencies you should use yourself, since we will only include the
standard CCITT #5 ones, so if you need anything special you'll have to code
them yourself!!!!

The  hardware  will  cosists  out  of  two single-sided boards, a
keypad and a phone speaker. Or, you might put a 3.5 mm phono jack on the box
and use a pair of freestyle headfones. I use that myself, with excellent
results.... Also, this looks more unsuspicious if you use it in a payfone...

Now, the rest is up to you. There is still some room left in the eprom for
additional routines, so you might add wahtever you want to the box....

-----------------------------------------------------------------

                          *** WARNING ***

The use of a bluebox is a crimminal offence, and it's *YOUR* problem if you
get caught using one. We will accept no responsibility for your actions, we
just show you the theory behind the construction of a CPU controlled bluebox
and the use of this device on any phoneline without permission is strictly
forbidden!!!!!!! Now it's all up to you...........


Building this box is not a simple task. If you do not have good experience of
soldering together complicated circuit, do not attempt the constyruction of
this device. Ask somebody who does have experience to do it for you!!!!

-----------------------------------------------------------------

                 Parts List for Jollybox v4.00:
                 ==============================

    No:        Description:             Elfa Order #:
    ===        ============             =============
     01        80C39 CPU                73-802-49
     01        27C64 EPROM              73-729-31
     01        27C010 EPROM             73-736-32
     01        74LS373                  73-726-00
     02        74LS393                  73-729-15
     01        741 OP.                  73-010-21
     01        8-PIN SOCKET, 7.62MM     48-135-49
     02        13-PIN SOCKET, 7.62MM    48-135-64
     01        20-PIN SOCKET, 7.62MM    48-136-22
     01        28 PIN SOCKET, 15.24MM   48-137-54
     01        32 PIN SOCKET, 15.24MM   48-137-62
     01        40 PIN SOCKET, 15.24MM   48-138-12
     01        12-KEY TELEPHONE KEYPAD  35-678-07
     01        1 POLE SPST SWITCH       35-355-31
     01        3.5MM PHONO JACK         42-700-88
     01        146*90*37MM PROJECT BOX  50-381-04
     01        7805 5V POS.V. REGULATOR 73-090-08
     01        10 MHZ CPU CRYSTAL       74-505-05
     01        RED LED, 3MM             75-037-09
     02        10 UF, ELECTROLYTIC      67-008-19
     02        15 PF, CERAMIC           65-691-23
     01        0.1 UF, CERAMIC          67-776-43
     01        0.33 UF, CERAMIC         67-777-18
     01        100 KOHM POT, LOG.       64-064-09
     01        270 OHM, 5%              60-104-25
     03        10 KOHM, 5%              60-106-15
     03        100 KOHM, 5%             60-107-30
     01        10 KOHM, 1%              60-734-23
     01        20 KOHM, 1%              60-737-46
     01        40.2 KOHM, 1%            60-741-08
     01        80.6 KOHM, 1%            60-744-54
     01        160 KOHM, 1%             60-747-77
     01        324 KOHM, 1%             60-751-21
     01        634 KOHM, 1%             60-754-85
     01        1.3 MOHM, 1%             60-757-33
     02        PCB'S /W PHOTORESIST     49-576-19
     01        16 LEAD RIBBON CABLE,1M  55-660-54

-----------------------------------------------------------------

                     Building the Main-Board


This will be the hardest part!  If you make one mistake, you will
not get any result, so if it doesn't work, check the Layout!

'8049BB1P.PCX' is the picture showing where on the PCB the components
should be placed. '8049BB1.PCX' and '8049BB1M.PCX' is the circuitboard as
seen from the back in normal and mirrored format. The same pictures exist
for the sample board too, but the they're called #2 instead of #1....
To get films for photo etching, either make your own layout from these pics,
or if you have a standard epson 9 or 24 pin printer, or a HP Laserjet
compatible laser, you can just print the files in the PCB_PRNT.ZIP archive.

     *.P9      Epson 9-Pin printer image files.
     *.P24     Epson 24-Pin printer image files.
     *.HPL     HP-Laserjet printer image files.
     *.HPD     HP-Deskjet printer image files.
     *.PCB     PCB Layout files for PCB Layout v1.x on Atari ST.

Power up the main circuit board and test it with a power supply of
9V, 500mA. A normal 9V battery will do fine, but we do recommend
a real 9V DC power supply when the box is to be used indoors, since
normal batteries tend to run out quite fast, all these chips consume
quite a lot of current when the box is being used a lot. Check
the "power in" pins at the main board and check if there are 5V
comming out on the power out pins. Check if the clock jumper
shows  a 666666 Hz signal on a meter or a scope based to ground.
If this is ok the power, processor, quarz is working.  Now check
if one of the keyboard  pins  (p2-p7) based to ground shows a
frequenz (far  under  666666  Hz). Congratulation: You did the
hardest part if it works. Now connect the keyboard with p2-p7
for lines and t0-t1 for the rows with the ribbon cable. See
KEYBOARD.IFF how the keys are connected to the boards. You can
check it, when the sample-board is done.

-----------------------------------------------------------------

                    Building the Sample Board


'8049BB2P.PCX' shows where the components should be put, and '8049BB2.PCX',
and '8049BB2M.PCX' shows the back of the PCB in normal and inverted mode.

Put on all jumpers and sockets first. Then put on all bigger parts and
at least the ICs! Take the '27010SPL.ROM' file and program it into an
27010 eprom.  Press the eprom into it's socket too.

Use a ribbon cable and connet both boards with s0-s4, +5v, +7-9V, gnd.
Connect the poty and speaker also.

Turn  the  poty  to 1/4 of its resistance or less!  Listen to the
telephone speaker, when you turn on the power.

Now  you can hear 3 short beeps, this is the normal mode.  If you
press keys 1-4 while turning on, you can hear all samples in the
selected sample-bank. This is the self test option. Now you have to
adjust the poti so that the sound of the speaker is loud enough but
not in a bad quality. Find  out  the right volume by testing it!

-----------------------------------------------------------------

                        Operating the BB

Manual for the ROM 4.0

If  you  turn on the power, you must here 3 short beeps.  Now you
have a variety of options for different calls:

Whitebox:

Press the number (#) symbol to switch to whitebox.  Now press any
key and the DTMF tone for that key will be hold until you release
it again.  To exit the whitebox, press # again. The keys 0-9 will
generate the normal DTMF tones like a touch tone dialer.

          *1=DTMF "*"
          *2=DTMF "#"
          *3=DTMF "A"
          *4=DTMF "B"
          *5=DTMF "C"
          *6=DTMF "D"

Bluebox dial:

Press 0 to  dial ram number #1, 1 to dial ram number #2. Press 20-27 to dial numbers
stored in phonebook #1. 30-37 is for dialing from fonebook #2...

Trunk and Seize:

To trunk locally in countries that use inband signalling use key 7 to send
an 1.5 second 2600 Hz tone. Key(s) 8 and 9 will generate international trunk
tones for boxing off other countries. 8 will send universal trunk #1, 9
will send universal trunk #2. If you should call by sattelite, press 4 to send
a DHLS clipping disable signal. This will give you better line quality....
Keys 5 and 6 generate Redbox tones for Dime and Quarter, works in US and most
likely in some other countries too. Press **0 to enter a new dialing prefix, the
default prefix is 2460 (KP2+460), end input with # key. The first digit should
be 1 or 2, standing for KP1 or KP2!! If you use 3 as the first digit, the number
will be outpulsed i DTMF instead of Mf or any other kind of bluebox tones.


Universal trunk #1 is 2400/2600 Hz for 130 ms, pause 1.75 sec, 2400 Hz for 300 ms.
Universal trunk #2 is 2400/2600 Hz for 130 ms, pause 2.00 sec, 2400 Hz for 130 ms.
The trunk tones may be reprogrammed at your convenience by alterin the labels named
TRUNK1N, TRUNK2N and LTRUNKN in the 8049 assembler source code.

Test-Mode for testing sample rom and volume:

If  you  press  1-4 while  turning  on, you get all the tones of the
sample bank you choosed...

Enter number:

Press **0 to enter a new dialling prefix.
Press **1 to enter ram resident number #1.
Press **2 to enter ram resident number #2.

While entering a number, use * to enter special tones like the DTMF *,
# and ABCD tones. For DTMF, *1=*, *2=#, *3-*6=ABCD. The same goes for bluebox
mode. The first digit entered is very important. A 0 means dial prefix, then
outpulse the rest of the number. A 1 means outpulse KP1 tone and then dial in
the bluebox tone mode currently in use. A 2 means the same as above, but
oupulse KP2 instead of KP1. To finish entering the number/prefix, press #.
In bluebox mode, the * key together with keys 1-6 also have important uses.


	In mode 0:		In mode 1 & 2:
	==========		==============
	*1 = DTMF "*"		*1 = Code 11
	*2 = DTMF "#"		*2 = Code 12
	*3 = DTMF "A"		*3 = KP1
	*4 = DTMF "B"		*4 = KP2
	*5 = DTMF "C"		*5 = ST
	*6 = DTMF "D"		*6 = 1850 Hz DHLS

Of course these keys also have special uses in CCITT #4, but as we do not
know very much about CCITT #4 you'll have to figure them out by yourself.
Anyway, according to the CCITT #4 documentation that I got the keys should be
defined as:

	*1 = Code 11
	*2 = Code 12
	*3 = Space Code I
	*4 = Incoming Half Echo Supressor
	*5 = Space Code II
	*6 = End of Pulsing (ST).

The KP1 and KP2 signals are not part of the binary coded digit signals in
CCITT #4, and can only be sent at the start of dialing.

Prefix:

Press **0 to enter a prefix.  Press 1 for KP1 and 2 for KP2, 3 for DTMF mode.
Enter the  full  prefix  and stop with #. If you have a phonebook with
numbers  of  austria,  you  have to dial b430....So just enter 0-XXXXXX-ST
in your phonebook.   When  you  dial a number with 0 at the begining, the
prefix  will  be added.  This is an additional function, which is
not necessary for normal calls. The prefix default is B460.

The  entered  numbers  including prefix will be erased and set to
default when turn off and on the BB.

Special Functions:

          *0 - Select Sample Bank 0. (DTMF, All 16 Tones).
          *1 - Select Sample Bank 1. (CCITT #5-R1).
          *2 - Select Sample Bank 2. (CCITT #5-R2).
          *3 - Select Sample Bank 3. (Break/Simulation Tones).
          *4 - Select CCITT #4 Mode.
          *# - Enter Special Tone Simulation Mode

In CCITT #4 mode, you can only dial the numbers stored in RAM position(s)
one and two, and the trunk keys 8 and 9 will send CCITT #4 clear forward and
xfer forward signals. These signals are coded according to the CCITT's own
specifications, buit has not yet been tested as of todays date. Hopefully
they'll work fine, but we haven't had any possibility of testing them yet.

-------------------------------------------------------------------------

                    Special Tone Simulation Mode:

        1 - Swedish Dialtone
        2 - Swedish Busy Tone
        3 - Swedish Ring-Tone
        4 - US Dialtone
        5 - US Busy Tone
        6 - US Ring-Tone
        7 - Swedish Reorder Tone
        8 - US Reorder Tone
        9 - Greenbox Ringback Tone, 1000 ms
        0 - Greenbox Coin Return Tone, 1000 ms
        * - 2600 Hz Wink, 90 ms
        # - Return to Main-Menu

-----------------------------------------------------------------

                    How to create a phonebook


Take the "8049vXX.rom".  this will be the file, which you have to
program  into the eprom for the CPU. Insert Phonebook 1 and 2 at
$300-$3ff in the binary rom file for the 8049 program eprom, and
after that, burn the program onto the 2764 eprom. Also, if you want
to have CCITT #4 capabilities in your box, do not forget to program
the 64 byte file "CCITT4.BIN" at $5C0 on the program rom. This file
contains the 16 binary coded CCITT #4 signals......

If you like modified this plan, I will give you an idea, how you
can create a phonebook by your own. The Rom for the CPU goes
from  $0000-$07ff. The Phonebook goes from $0300-$03ff for 10-17,
20-27.

An example is shown here:

$0300: 02 04 09 00 01 02 03 04 05 06 07 08 20 00 00 00 : b49012345678c... 10
$0310: 01 00 09 00 03 01 04 01 20 00 00 00 00 00 00 00 : a0903141c....... 11
$0320: 00 04 00 01 02 03 04 05 06 20 20 20 20 20 20 20 : 040123456c...... 12
$0330: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 13
$0340: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 14
$0350: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 15
$0360: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 16
$0370: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 17

$0380: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 20
$0390: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 21
$03a0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 22
$03b0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 23
$03c0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 24
$03d0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 25
$03e0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 26
$03f0: 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 20 : ................ 27

Each of the 16 Bytes are one phonenumber. On the Right are the
Digits to press, when you want to dial them. For the number at
$0300  press 1 folowed by 0! Enter the number like you would do,
when you  enter it directly. Use $01 for 'kp1' or $02 for 'kp2',
$00 for prefix and $03 for DTMF dialing.

Then enter the digits: $00 for '0'...$09 for '9'.  The last
digit has to be a $20. The bluebox will add the 'st'-code.
In this example the first number is 'B49012345678C'. It will call
Germany: 0123/45678. The second will call rout operator.
The third will call (prefix40123456).  Use as prefix b490 for
this example if this is a german number.

The maximum is 15 Digits and $20 for st. If you like numbers
with more than 16 digits, just go on and use the next line of the
next number. The compuer will dial until it gets a $20 code. If
this isn't still enough, use more and more.

-----------------------------------------------------------------

                         ASS80XX

        Written by Jolly Roger for the Jolly-Box

There is a short  descripion of the 8049 assembler for the Jolly-Box. It is
necessary because you need to modify the source to your own developing.
It includes all opcodes.

The format must be as followed:

-No case sensity

-Only one opcode in one line and one label

label:	clr	a
label2:

	jmp	label

-You can use Decimal, Hex or Binary for values

	mov	a,=128
	mov	a,=$80
	mov	a,=%10000000

-Characters after a semikolon will be ignored until the next line

	clr	a	;set accu to zero

-Use  space  as well as tab to seperate.  Seperations between label and opcode,
 opcode and semikolon are not necessary.

-Jumps must always jump to a label, numeric is not allowed

If you like to skip to a memory page:

	page	2

will skip to byte 512 of memory. If it is already passed an error will occure.
Remember  that  only  JMP and CALL can jump to an adress within a page of 256!
How the opcodes work refer to the 8049 manual.

------------------------------------------------------------------------------

                    published by a member of

         ___                             ____     _
           /_ _/_  _ _  ___/._  _  __ /   /_  //_/_ _  _
        (_// )/(_'/ / )(_///(_)/ )(_//   /(_)// // (_'(_'
                         ___
                        /_ /_  _  _   _  _
                       /  /(_ (_ (_'_) _) 

    - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
                        Downloaded from NIGHT-BOX
                      ----------------------------
        __  __   ___   _______   ___  __  ________  
       / /\/ /\ / //\ / ___  /\ / //\/ /\/__   __/\         
      /  \/ / // // // //_/_/ // //_/ / /\_/ //\_\/         The ACF-BBS
     /     / // // // //__\_\//  __  / /  / // /           -------------
    / /\  / // // // //_\ /\ / // / / /  / // /               SysOps
   /_/ /_/ //__/ //______/ //__/ /_/ /  /__/ /             Pooky & Jacky
   \_\/\_\/ \__\/ \______\/ \__\/\_\/   \__\/            
 
                       05861 8795 (new number!)      

                                                _______   _______   __   ___ 
                 -- 8N1 --                     / __   /\ / ___  /\ /  \_/  /\
           17-9h online Sa,So 24h             / /_/ _/ // // / / / \    __/ /
     14.4K/12K/9600/7200/4800/2400/1200      / ___ \_\// // / / /__/  // _\/
  -=====================================-   / //_/ /\ / //_/ / //  _   \ \
   V.32/V.32bis HST V.42/V.42bis MNP 1-5   /______/ //______/ //__/ \__/ /
                                           \______\/ \______\/ \__\/ \_\/
 
               ATARI/ AMIGA/ IBM comptbl./ SNES/ M.Drive
                                           
                                             .---.        .---.
                                            /     \  __  /     \ 
 Coming soon....                           / /     \(  )/     \ \ 
                                          //////   ' \/ `   \\\\\\
          JACKTRO                        //// / // :    : \\ \ \\\\ 
                                        // /   /  /`    '\  \   \ \\
              by the ACF Design Team!  //          //..\\          \\
                                              ====UU====UU====
                                                  '//||\\`
                                                     ''``
                          __        __ 
          ________ ______/ /_______/ /_________ _________ __   __ ________
         / ______// ____/ /_  ____/ /_  ____  //  ____  // /\ / // ______/\
      __/_/_____ / /\__/ / / /\__/ / / /\__/ / / /___/_// /_// // /\_____\/
     /_______  // / / / / / / / / / / / / / / / //________  __// //__/\
     \/ /___/ // /_/_/ / / /_/_/ /_/ /_/_/ /_/ /___/ /\__/ /\_/ /_\__\/
     /_______//_______/ /_______//________//________/ / /_/ //_______/\
     \_______\\_______\_\_______\\________\\________\/  \_\/ \_______\/

                 Thanx for calling this fine ACF BBS


Click...

-----------------------------------------------------------------------------

.                                                +             .
               _______ ____   ________    ___    _______ _____/|
       +      /  __  //    \ /  ______\  /  /   /  __  //  ____!
             /  /_ \//  /\  \\  \  ___  /  /   /  /_ \//  /___
            /  __/  /  /  \  \\  \ \  \/  /   /  __/   \____  \
            \  \__/\\  \  /  / \  \/  /\__\___\  \__/\.____/  /    '
   *         \_____/ \__\/  /   \____/    \__/ \_____/| _____/     |
                        /__/  .     /    _  /         |/       - --+- -
      USR HST Dual Standard 14400  /    / \/ 285 Megs :            |
          _____________________   /     \   ______________________ .
   .      \__ __ _ _           \_/       \_/            _ _ __ __/
   :        \___ __ _ _  Sysop: Zaphod Beeblebrox   _ _ __ ___/
   |           \___ __ _ _   Control Team EHQ    _ _ __ ___/
---+--- -         \___________    ICS SHQ    ___________/
   |                          \___   :   ___/
   :            +46-18-262804     \  |  /     24 Hours/Day.           ' 
   .      *                        \ | /    .
                   .______    _____/ | \___/|___________ 
                   |   _  \  /  _/ __|__ \__!  ______  /
       '           |  | \  \/  /_\| /  /|/_  \/ |  | \/
                   |  |  \  \  _/ ' \___'  \    |  |              +
                   |  |  /  /  \__/\____/  /    |  |
                   !__! /__/\______| _____/     !__!
                                   |/                             
                                   :

-----------------------------------------------------------------------------
