STATION ID - 7091/6.411

9x Datakit Network
FOR OFFICIAL USE ONLY

This is a 9x system, restricted to authorized persons and for
official 9x business only. Anyone using this system, network or data
is subject to being monitored at any time for system administration and
for identifying unauthorized users or system misuse. Anyone using this
system expressly consents to such monitoring and is advised that any
evidence of criminal activity revealed through such monitoring may be
provided to law enforcement for prosecution.


	   Flygu's (flygu=lordofpain) Cellular Phreaking Guide For 96'
	  ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

about flygu: well flyGu, is just my IRC nick, i am Lord Of Pain from 
	     San Diego <whatsup 619>..i wrote dis cause Substance wanted
	     me to write something cool about cellular for his group 9x.                      
	     dis file will be released as a 9x release. thank you very much.

disclaimer: read this for learning. knowledge is power over those whom
	    opress our mind and soul. however, do not get arrested for
	    doing this. if you are gonna go down, go down as a fighter for
	    free thinking and our pathetic species. they want us to go down
	    for shit like this, so watch yourself.


thankx to: most thanx to the old school 619 people. they were around
	   and ran boards and supported the scene. (cj, bones, kludge, 
	   doctor disector, mrfab, ,dr.who, g, tck, tem, iron reeper).
	   special thanx to : Vigilante,digitalorgasm,coolddude,mrfab,
	   bobdobbs,satan,emp,diabolus,sliver,and everyone else in 619. 
	   thanx guys
	   


NOW FOR THE MANUAL. .  Cellular Phreaking Manual By FlyGU (lordofpain)
		       ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^



	Cellular phones are great tools for any hacker/phreaker. 
They can NOT be traced, they are mobile, and you can easily modify them. 
Although CID for cellz is in the making (i am sure) al you have to do is
modify the cell over and over, and you wont get caught. 

	Before I teach you how to modify a cell phone. Let me teach you 
the basics of how it works. Cellular companies have stations which 
have honeycomb like structures called cells. Each cell is capable of 
having certain number of calls and usually handles an area. The phone
sends its into to the tower, and it gets acess so it can place the call.
The phone actually sends and recieves at the same time. So there are 2
channels involved. If you know one, you know the other because they are
45 appart. (simple math, if you gonna be a phreaker/hacker you can atleast
figure this out. :} )...


ESN- electronic serial number
MIN- mobile identification number
NAM- numeric assignment module
FOVC- forward voice channel 
FOCC- forward control channel
ROVC- reverse voice channel
RECC- reverse control channel


	Your phone also has software in it. IT has a chip with actuall
sofware written to control its functions. Each make and brand name has a 
different software. Software can be modified to your advantage. You will
learn more about this leater in this text. 


	Now that you know how it works you should know "how not to get
caught". Basically if you are doing a major hacking project, change 
your physical location and the esn.min pair every 2 hours or so. If you
just call some LD boardz, then you can change it like ATLEAST once a day.
This is because of 3 simple things. The 1st is that the cellular company
has clonning detection. For example you are 20 miles away from the actuall
owner of a cellular phone. If he makes a call, then you make a call within
5 minutes a clonning flag goes off, because they know where you are located!
and since there is no way for him to get to where you are in 5 minutes a 
security flag goes off on his account. Second reason is that they know 
approximately what area you are in when you use the phone, so if they want
to catch you thell use directional antena and catch you. Thats
why if you move around alot and change pairs alot they cant catch you! and
third reason is the owner of the phone might get charged for your calls, so
switch pairs around so that you dont ruin someones life! (have morals in all
that you do, your morals dont have to be what society wants them to be, just
set them for yourself.)

	The company that makes the cell puts a permanet ESN on your phone
which is not made to be changed. It is permanently burned into a chip. Your
phone also has software thats in it. Its kinda like a cellular operation 
system. Each type and brand of phone has different software. All phones
allow you to change the NAM and other features. So here lets assume you 
already got a pair you want to put into the phone (ill teach you how to
snag pairs later in this manual). There are several ways you can do that. 
On some phones you can make a cable and use software on your computer to
change the esn.min pair. This software is readily available to you on
the internet. There is a second way which is 100% better then the first.
You can burn new software into your phone that will alow you to change the
ESN and store it at a different location. You can make this software if
get the original software (you gonna have to read the chip, then work
your way to the origian software) and add some minor adjustments to it. 
If you do not have programming skills you can go to your web browser and 
go to www.l0pht.com and go to drwho's radiophone (its in archives) and
you will find what you need there. So now you that you have that, can 
now change the esn, and you can change the min. Thats it! you just now 
clonned a cellular phone. But dont think that is it, hundreds of other
fun things you can do with your cellular phone. 

	Ok. You now have a phone that allows you to change the ESN and the 
NAM. But what fucking good is that gonna do you if you cant get (snarf) the
ESN.MIN pair. There are alot of ways to get pairs i will present some 
methods to  you that already work and at the end of this manual i will 
include some ideas you can try that no one else has tried before.



Method 1
_____________________________________________________________________________
the simplest way is this. tzanger wrote this little segment on irc the other
day so method one is his

 three components make the hardware:
 
 comparator, PLL and XOR gate.  take the discriminator's output from the
 scanner tuned on ROVC and feed it to the op amp, tune the PLL for 10khz and
 run its output and the incoming datastream thrugh the xor.  dats it, after
 you do this you should have a bunch of ddi info. SIMPLE!
______________________________________________________________________________



Method 2
_____________________________________________________________________________

	There is software available that you can use with your modified
scanner to recieve pairs using your computer. look for it on the net. 
i suggest trying all the web search engines. i have seen that stuff on
alot of pages i visited...i used tzanger's text that he wrote it in a way
that you guys can easily understand.
____________________________________________________________________________


Thats it. Its that simple. This works very easily, your scanner picks up the
RECC (reverse channels where the pairs are transmitted) then you just convert
them to readable format. simple!


	But clonning is not all you can do with your cellular phone. 
You can monitor other calls with your cellular phone also. The only 
problem is handoffs. They occur because a person moves out of range from
a cell, and a handoff occurs. He gets transported to another cell. 
But this can also be easily conquered. If you have a Motorola all you have
to do is put it into test mode, and unmute the audio, and go to a channel
and listen! So your cellular phone can also be a tracking and spying device.
The posibilities are unlimmited. have lots of cellular phun!


---experimental ideaz for your hungry mind to munch on----------------


 i have personally seen with my own eyes a cellular phone pick up the 
 channel where ESN.MIN's are transmited (yes i heard it, the transmition
 of the pairs makes the most annoying noise i have ever heard. hehehe).
 so now all you gotz to do is convert them and store them.. i believe
 that someday someone will create a phone that can do that. you can also
 convert somehow (think hard, i wont give you this one) and store in
 your computer.......i even heard rumors that someone had a phone that
 works like this: you put the number you want to call, push send, then
 the phone snarfs a pair, and uses it just for that one call! i also 
 heard rumors of phones having 1000 esn.min's in them, and they use them
 up slowly. I AM NOT SURE IF THESE RUMORS ARE TRUE, THEY CAN BE LIES..
 but we can make them true. cause H/P is all about learning and trying.

__________________________________________________________________________

# end. i made this manual short and complete. i am lazy. if you want to learn
  more i suggest asking someone who cares because i do not. i wrote this to
  help those who are motivated enough to get off there ass and learn more. 
   
_____________________________________________________________________________
				     _
				    |*|
Author: flygu (a.k.a Lord Of Pain)  |*|               
			     _______|*|
			    /*12345678#\ <---- :-)                  
			    |__________|                                          
			    |          |
    FLYGU thinks that OKI   | 1  2  3  |                              
	  is da SHITZ!      | 4  5  6  |   
			    | 7  8  9  | <--------- hail da oki!             
			    | *  0  #  |
			    |RclStoAlMe|
btw: did i forget to        |Snd Cl End|
     say that oki's rule!   |-+oki900__|
			    |__________|   <---oki900. da best phone!

find me on IRC as flygu, or on a BBS as Lord Of Pain..talk to me if you wish 
______________________________________________________________________________
