

                            HME/HM Electronics, Inc.

                              Frequency Selections


 I. Wireless Microphones
    A. General:   Churches, theatres, universities, entertainment centers, 
                  personal business users may operate under FCC Part 90.217 
                  using the following:

 Channel  Frequency (MHz)   Channel  Frequency (MHz)   Channel  Frequency (MHz)
   B1          169.445        B4         170.305         B7         171.845
   B2          169.505        B5         171.045         B8         171.905
   B3          170.245        B6         171.105

 B. Export:  The following are for export use:

 Channel  Frequency (MHz)   Channel  Frequency (MHz)   Channel  Frequency (MHz)
   A1          169.425        A7         170.825         C5         217.980
   A2          170.325        C1         216.000         C6         218.450
   A4          171.925        C2         216.400         C7         218.870
   A5          169.625        C3         216.900         C8         220.377
   A6          169.925        C4         217.525

 C. Broadcast:    Broadcasters, cable television operators, motion picture 
                  industry, and video production studios may operate under FCC 
                  Part 74.  Select from the following channels on a non-
                  interference basis:   

 Channel  Frequency (MHz)   Channel  Frequency (MHz)   Channel  Frequency (MHz)
   7A          174.800        9C         187.800         11E        202.000
   7B          175.400        9D         189.400         11F        202.800
   7C          175.800        9E         190.000         12A        204.800
   7D          177.000        9F         190.800         12B        205.400
   7E          178.000        10A        192.800         12C        205.800
   7F          178.800        10B        193.400         12D        207.400
   8A          180.800        10C        193.800         12E        208.000
   8B          181.400        10D        195.400         12F        208.800
   8C          181.800        10E        196.000         13A        210.800
   8D          183.400        10F        196.800         13B        211.400
   8E          184.000        11A        198.800         13C        211.800
   8F          184.800        11B        199.400         13D        213.400
   9A          186.800        11C        199.800         13E        214.000
   9B          187.400        11D        201.400         13F        214.800



HME  -2-


II. Wireless Intercom
    The IC150 Series Wireless Intercom is available on three frequency bands.  
    The "A" version is for export use, the "B" band is type accepted under FCC 
    Part 90 for general purpose use, and the "C" version is for broadcast use 
    under FCC Part 74. 

Channel  Frequency (MHz)   Channel  Frequency (MHz)   Channel  Frequency (MHz)
A) IC150 -     173.225      B) IC150 -   154.570      C) IC150 -    161.655
   MT1000-      72.020         MT1000-    30.840         MT1000-     26.150
                72.800                    33.140                     26.250
                75.420                    33.400                     26.300
                75.980                    35.020                     26.450



          This listing is supplied courtesy of HM Electronics and:
  
                      AV-Sync Atlanta (404) 320-6202



Downloaded From P-80 International Information Systems 304-744-2253

