Author : Regel                                                Date : 11/07/93
                          ÚÄ
                          ³ Ú¿  ÚÄÚÄ¿\ÚÄÚÄÚ¿³ÚÄ
                          À¿³³³³Ã ÃÂÙ³Ã ³¿³³³À¿
                           ³ÀÙÀÙÀÄ³À ³ÀÄÀÙ³ÀÙÄÙ
                          ÄÙ
                                   OF
                                  ÜÜÜÜ
                              ÜÜßß    ßßÜÜ
                            Üß   ÜßßßßÜ   ßÜ
                           ÞÝ   ÞÝ    ÞÝ   ÞÝ
                           Û   Üß      ßÜ   Û
                           ÞÝ ÞÝ        ÞÝ ÞÝ
                            ßÜ ßßßßÛÛßßßß Üß
                              ßßÜÜ    ÜÜßß
                                  ßßßß

                Soveriegns Of Bell Issue #1 - The InterBox
------------------------------------------------------------------------------

         OK. My purpose for writing this file is to shut people up about how
they are sick of putting a speaker from their SB, etc. up to their fone reciver.
This box will enable you to detect when the line is ringing, when the called
party has hung up, will allow you to hear what is on the line when it is both
on and off hook <allowing for line monitoring>, and applying a signal to the
fone line. Pretty cool, huh? I thought so.
         Now, first, I have to clear my ass. If you continue reading, I, nor any
body else is responsible for you fucking up, getting busted, and embarrasing
your mother, me, and the entire H/P scene. You are on your own. No one else but
you is held liable for your dumb ass phucking something up. There. Now, onto
the box.
         Instead of giving you some lame instructions, I will show what to do
in the form of schematics. If you can't figure them out, check out a book on
them at the good 'ol local library. Here goes...
                                 2 ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿ 5
<ÄÄÄÄÄÄÄÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄ´(ÄÄÄÄÄÄÄÄÄÄÅÄÂÄ¿         /ÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
            ÚÁ¿      <C1>          ³ Á     _³ÄÄ/  ³              |_Ring Det.
       <MOV>ÀÂÙ <C4>               ³  Â    ³³Ä-  ³              |
<ÄÄÂÄÄÄÄÄÄÄÄÄÅÄ)³Ä¿    ÚÄÄÄÄÄÄÄÄÄÄÄÅÄÁÄÙ    ³    \ÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
   ³         ³    ³    >         1 ÀÄÄÄÄÄÄÄÄÅÄÄÄÄÄÄÙ 4
 ÚÄÙ         ³    ³   <  <R1>       <IC2>
 ³        _______ ³ ___>
 ³    --0        ÃÄ¿  ÚÄÄÄÄÄÄÂÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
 ³ *  --0ÄÄÄÙ    ³ )³³(      Á   ³              ³                |
 ³ R  --0ÄÄÄÄÄÄÄÄÙ )³³( <D1>     <D2>        ÄÁÄ  <C2>         |-Audio I/O
 ³ Y      __        )³³(      ³   Â             ÄÂÄ               |
 ³ 1  --0        ÂÄÙ  ÀÄÄÄÄÄÄÁÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
 ³ *  --0ÄÄÄ¿    ³  <T1>
 ³    --0ÄÄÄÄÄÄÄÄ´
 ³  ________ ³ __ ³ ______________________________________________0 +
 ³ <Ú¿ <C3> ÄÁÄ   ³                                               |_ Line
 ³  ³³>     ÄÂÄ   ³                                               |  Seize
 ³ <ÀÙÄÄÄÄÄÄ ³ ÄÄ ³ ÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0 -
 ³           ÃÄÄÄÄÙ
 ³           >
 ³          <  <R2>
 ³           >                   1 ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿ 5
 ³          ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÅÄÂÄ¿         /ÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
 ³                                 ³  Á    _³ÄÄ/  ³              |_Party
 ³                                 ³ Â     ³³Ä-  ³              | HangUp
 ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÅÄÁÄÙ    ³    \ÄÅÄÄÄÄÄÄÄÄÄÄÄÄÄÄ0
                                 2 ÀÄÄÄÄÄÄÄÄÅÄÄÄÄÄÄÙ 4
                                  <IC1>     ³

R1------22,000 Ohm
R2------1000 Ohm
C1------.56 uF 250volt Mylar
C2------.01 uF 50volt Ceramic
C3, C4--.1 uF 250volt Mylar
IC1,IC2-H11AA1 AC input optoisolator
D1, D2--1N270 Germainium Diodes
T1------Telco 1:1 isolation transformer
MOV-----300 volt Metal Oxide Varistor <can be removed, but not recomended>
RY1-----12 volt DPDT Relay


        OK, so you have the beast wired. Now, let me tell you how to connect
it. The ring detect lines will close and conduct when the line rings. It
functions almost like a switch. Also, the party hangup lines function like
switches, except that when the party you called hangs up, this will pulse.
The line seize lines connect your sound input and output to the line. When
12 volts is not applied to these lines, the box goes into monitor mode, and
all audio will be passed to the audio I/O channel, and in effect, bugging the
line. When 12 volts is present at these lines, however, you can connect a 1/8"
plug to the audio I/O channel, and either connect it to an audio source, or to
the input of a recordng device to record what is said or heard on the fone.
I suppose that wrapps it up. If you have questions regarding this box, leave
me mail or something, and I'll be glad to help out. <part II will be released
shortly after this first release, where I will show you different tricks with
this box>. Also note that this interface complies FULLY with the FCC type 68
fone device, and, in itself is perfectly legal.

 ----------------------------------------------------------------------------
|                       Soveriegns Of Bell Issue # 1                         |
| Call these 3l33+ BBS:                                    Or Mail Us At :   |
| The Truth Sayer's Domain - 210-493-9975 - SoB WHQ          lmb@tenet.edu   |
| Red Dawn-2               - 410-263-2258 - Affiliated Board                 |
 ----------------------------------------------------------------------------
EOF : 5498 Bytes
