 tried chopping my
bootlist down to the bare minimums with the same result.

      -- john

There is 1 Reply.

#: 19117 S9/Utilities
    14-Oct-93  23:16:56
Sb: #19115-#AR
Fm: Carl Kreider 71076,76
To: John L. Wilkerson Jr. 71140,77 (X)

Are you using shell+?  If so, try it using shell from Microware.  You may (I am
not the expert here) have to rename shell and patch the binary, but you should
be able to use 'mw_shell ar -u foo *' from the shell+ prompt.

There is 1 Reply.

#: 19122 S9/Utilities
    15-Oct-93  22:03:51
Sb: #19117-#AR
Fm: John L. Wilkerson Jr. 71140,77
To: Carl Kreider 71076,76

    YES, as a matter of fact I do use shellpluss.  I was reading the other
messges on how to repair shellplus' memory bug.  I installed tha patch, and
BINGO, all aspects of the new ar. work flawlessly!

      -- john

There is 1 Reply.

#: 19125 S9/Utilities
    16-Oct-93  17:31:53
Sb: #19122-AR
Fm: Steve Wegert 76703,4255
To: John L. Wilkerson Jr. 71140,77

 > YES, as a matter of fact I do use shellpluss.  I was reading the
 > other messges on how to repair shellplus' memory bug.  I installed tha
 > patch, and BINGO, all aspects of the new ar. work flawlessly!
 >

Hmmm ..... did I miss the patch? Where did you find it?


*- Steve -*


#: 19124 S10/OS9/6809 (CoCo)
    16-Oct-93  11:40:41
Sb: #18919-3.5 drive query
Fm: Bob Palmer 74646,2156
To: David Breeding 72330,2051

Hayes might help but I hasten to add that although my old 1200 baud unit has
been ultra reliable (and No I didn't buy it new - wadda ya think - I'm made of
money |-) ) BUT! the new 2400 baud which I borrowed from work folded up in
short order. The pulse dialing relay went intermittent and we have had one
other of these do the same. That is why the question about pulse dialing.  This
is the same relay which does the off hook function so you could still have
trouble there. }iUSR sporsters are not expensive. - in fact they are one of the
lowest priced name brands I have seen. Bob.


#: 19116 S12/OS9/68000 (OSK)
    14-Oct-93  20:54:42
Sb: #19109-ultra 'C' installation
Fm: Zack Sessions 71532,1555
To: SCOTT HOWELL 70270,641

 > I did that, but that did not work. I still get the 'F' line instruction
 > error when I start to compile a program The instructions for the Ultra 'C'
 > compiler says to add 'fpu' to the bootlist, os9gen a new os9boot AND add
 > 'fpu' to the extension module of the Init module.

Oh, I forgot about that one. :-) You also need to make a special init module.
Just make a copy of the one you are using now and edit it with moded. Move down
to the item called "customization module list". It should have the value OS9P2.
Change it to "fpu  " without the quotes. I use the quotes to make the point
that you need to blank out the last two characters of OS9P2. Verify and write
the module and include it in your next gen.

------------------------------------
 Zack C Sessions
 ColorSystems

 via InfoXpress/OSK by Bill Dickhaus

#: 19119 S12/OS9/68000 (OSK)
    15-Oct-93  07:12:53
Sb: #19102-#ultra 'C' installation
Fm: Ed Gresick 76576,3312
To: SCOTT HOWELL 70270,641

 Scott,

 Look in your SYSMODS directory for 'init.a'.  You'll find the following
 code way down in the file -

          ifndef Extens
         Extens dc.b "OS9P2",0
          endc

 Change that as follows -

           ifndef Extens
          Extens dc.b "OS9P2 FPU",0
           endc

 Using the 'make' file provided, assemble the code.  This will generate a
 new 'init' module.  Make a new bootfile - don't forget to include 'FPU'.

 Ed Gresick - DELMAR CO


There is 1 Reply.

#: 19123 S12/OS9/68000 (OSK)
    15-Oct-93  22:50:14
Sb: #19119-ultra 'C' installation
Fm: Zack Sessions 71532,1555
To: Ed Gresick 76576,3312 (X)

Ed,

That is the proper way to do that, but unforch, init.a was not distributed with
the MM/1 for some reason.

------------------------------------
 Zack C Sessions
 ColorSystems

 via InfoXpress/OSK by Bill Dickhaus

Press <CR> !>