

#: 9637 S7/Telecommunications
    27-Feb-91  22:27:19
Sb: #tsrun/tsmon
Fm: Hugo Bueno 71211,3662
To:  76625,2273 (X)

Bruce,

I'm trying to get your tsrun/tsmon package to work on my
system. My config is as follows:

512K Coco
B&B Hard Disk
SACIA driver (multipak version)
RS232 pak on slot 1

I have set up the following init file called init.t2 in /dd/sys:

ATZ
ATM0Q0V1X1&D2&C1S0=2E0
Unsupported baud rate on this phone line.
"CONNECT 2400":04
"CONNECT 1200":03
"CONNECT":01

When I call the programs like so: tsrun tsmon /t2 /dd/sys/init.t2 &
the system crashes with horizontal lines flashing on the screen upon
access to the disk.

If I run just "tsmon /t2 /dd/sys/init/t2 &", the modem is 
initialized just fine.

Do I need to do any special xmode to /t2 or set the modem kill bit?
If so, could you tell me how?

Hugo
71211,3662
Delphi: MRGOOD


There is 1 Reply.

#: 9663 S7/Telecommunications
    02-Mar-91  17:51:24
Sb: #9637-#tsrun/tsmon
Fm: Bruce Isted (UG VP) 76625,2273
To: Hugo Bueno 71211,3662 (X)

Hugo,
  I've tried tsrun, and it doesn't crash my system.  I don't know what is
wrong, but I'll get back to you if I figure it out.  If possible, don't use
tsrun... it is only really useful if you have set the "modem kill bit" (see
xmode in your OS-9 manual) anyway.
  Bruce



There is 1 Reply.

#: 9667 S7/Telecommunications
    03-Mar-91  08:17:08
Sb: #9663-#tsrun/tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted (UG VP) 76625,2273 (X)

Just for the sake of science, could you give me an xmode of your /t2?

By the way, when I use your xmode on window devices, it doesn't work. (i.e.,
window parameters not shown, and cannot be changed). Is this correct?

Finally, could you explain swapped DSR DCD? Why would I implement it, what is
it supposed to do? How do I do it?

(Sorry for all the questions!)

Hugo

There is 1 Reply.

#: 9677 S7/Telecommunications
    03-Mar-91  21:25:36
Sb: #9667-#tsrun/tsmon
Fm: Bruce Isted (UG VP) 76625,2273
To: Hugo Bueno 71211,3662 (X)

~ Hugo,
  OK, here's an XMODE listing of my /T3 port (I don't have a /T2 port in
memory):

 nam=T3 mgr=SCF ddr=DACIA hpn=07 hpa=FF60 upc=00 bso=01
 dlo=00 eko=01 alf=01 nul=00 pau=00 pag=18 bsp=08 del=18
 eor=0D eof=1B rpr=09 dup=19 psc=17 int=03 qut=05 bse=08
 ovf=07 par=02 bau=06 xon=11 xof=13 col=50 row=18 xtp=45
 wnd=45 val= sty= cpx= cpy= fgc= bgc= bdc=

  It sounds like you're referring to the "wnd= val= sty= ..." stuff near the
end of the XMODE listing of a window descriptor.  As you will see in the
following listing, they can be changed, but only if the window descriptor's
option table size includes them.  Get my "WINVDG.AR" package if you want window
descriptors that are already set up that way, or you can modify your own window
descriptors by changing the byte at offset $0011 to $24.

 nam=W1 mgr=SCF ddr=CC3IO hpn=07 hpa=FFA1 upc=00 bso=00
 dlo=00 eko=01 alf=01 nul=00 pau=00 pag=18 bsp=08 del=18
 eor=0D eof=1B rpr=09 dup=19 psc=17 int=03 qut=05 bse=08
 ovf=07 par=80 bau=00 xon=00 xof=00 col=50 row=18 xtp=01
 wnd=01 val=01 sty=02 cpx=00 cpy=00 fgc=00 bgc=01 bdc=02

  Finally, swapped DSR+DCD is useful if you want your 6551 ACIA based serial
port to be able to receive characters even when DCD is not valid.  This is of
most interest to BBS SysOps, who want their BBS to be able to recognize when a
caller hangs up (DCD would go from valid to invalid) and reset itself, rather
than going through the hassle of the modem kill bit killing their BBS program
and then having to use a program like TSRUN to restart the whole thing.  The
easiest way to implement it is to simply swap the two lines on your serial
cable and then set the appropriate bit in the XTP byte.
  And don't worry about the questions, there hasn't been too much mail for me
here lately, so this is a nice change!
  Bruce

There are 2 Replies.

#: 9680 S7/Telecommunications
    04-Mar-91  19:39:28
Sb: #9677-tsrun/tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted (UG VP) 76625,2273 (X)

OK, I'll read your response offline.

Ah, so swapping involves some actual wire crossing, YUCK! By the way, what
would that do to telecom programs? Could I still call out?

I've been having nothing but frustration with your tsmon :-(.

I've had a friend calling in for testing, and tsmon never seems to recognize
when he presses ENTER.  I tried the Developer's pak tsmon, and it worked fine.
The only problem is when people hangup unexpectedly, which is something I'd
like to protect against!

I'll upload a summary of my efforts in another message.

Hugo

#: 9681 S7/Telecommunications
    04-Mar-91  19:59:54
Sb: #9677-#tsrun/tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted (UG VP) 76625,2273 (X)

Bruce,

As I said, I've had problems with your tsmon/tsrun combo. Anyway,
here's the init file that I send to the modem via the tsmon command
line: TSMON /t2 /dd/sys/init.t2 &

ATZ
ATM0Q0V0X1&D2&C1S0=2E0S25=100
Unsupported baud rate on this phone line.
"CONNECT 2400":04
"10":04
"CONNECT 1200":03
"5":03

Is there anything obviously wrong with it? When a caller calls, the modem
answers, carrier detect gets established but pressing return (I can see
the RD light flashing) yields nothing except a series of dots (SOMETIMES).

Here is an xmode of /t2 as I have it set up when I run TSMON:
 nam=T2 mgr=SCF ddr=SACIA hpn=07 hpa=FF68 upc=00 bso=01
 dlo=00 eko=01 alf=01 nul=00 pau=00 pag=00 bsp=08 del=18
 eor=0D eof=1B rpr=09 dup=19 psc=17 int=03 qut=05 bse=08
 ovf=07 par=0C bau=04 xon=11 xof=13 col=50 row=18 xtp=05
 wnd=05 val= sty= cpx= cpy= fgc= bgc= bdc=

Anything visibly wrong?

When I run the stock developer's pak tsmon, everything works peachy,
except if a caller hangs up without typing "ex", things get messy.
What possible difference can there be between the two where the stock
TSMON sees the CR and your TSMON doesn't???? I'm pulling my hair out
on this one.
I wonder if it's a problem of your tsmon never getting the CONNECT
string and running at the wrong baud rate???

HELP HELP HELP     SOS!
Hugo Bueno    CIS:71211,3662
              Delphi: MRGOOD


There is 1 Reply.

#: 9707 S7/Telecommunications
    06-Mar-91  22:14:45
Sb: #9681-tsrun/tsmon
Fm: Bruce Isted (UG VP) 76625,2273
To: Hugo Bueno 71211,3662 (X)

~ Hugo,
  I'm afraid I don't know what is wrong, but I can pass along a couple ideas
that others have given to me when they had solved their tsmon/modem problems.
The first is from Rich Mailer, who found that his "Zoom" type modem hung up too
quickly when DTR dropped momentarily.  What happened was someone called in, the
modem connected, and then hung up on the caller.  The solution was to increase
the amount of time allowed before a DTR interruption causes the modem to hang
up.  Sorry, but I can't remember exactly which S register controls that... and
I can't find an equivalent S register in my modem manual.
  The other thing is related to exactly when the modem sets DCD enabled.  On my
modem, the CONNECT message comes in first, and then after that the DCD line is
enabled.  If your modem does this then you'll have to do the DSR+DCD swap to
get it to work with a 6551 ACIA.  Check your modem manual for info regarding
the DCD signal, you may be able to set it so DCD is enabled before the modem
sends result codes and CONNECT messages.  You can check if DCD is enabled too
late by getting someone to call in at the default baud rate, and then manually
typing in the CONNECT message after the modems have connected. Remember, when
my TSMON is given an "init" file parameter it doesn't respond to just a CR,
unless there's a line in the init file that has a CR connect message in it. 
You could do this with a file editor such as dEd, BTW.
  I can't see anything wrong with the sample "init" files you've posted.  As a
matter of fact, I used the first one you posted in a test and had no problems
with it.
  Bruce

#: 9639 S10/OS9/6809 (CoCo)
    28-Feb-91  16:31:26
Sb: #9625-#Write IBM Disks?
Fm: JIM HICKLE 76672,602
To: Bill Henderson 72215,341 (X)

Bill, somewhere, (here or Delphi) is an IPATCH for cc3disk, if you don't have
Sdisk.  PCDos transfers great, but I can't figure out hou to format a pcdos
disk.
    -jim

There is 1 Reply.

#: 9658 S10/OS9/6809 (CoCo)
    01-Mar-91  19:03:06
Sb: #9639-Write IBM Disks?
Fm: Lee Veal 74726,1752
To: JIM HICKLE 76672,602

For formatting a PC-DOS diskette, there's a couple of utilities in the
commercial arena. As I recall D.P. Johnson (author of SDISK3) has or had some
OS-9 Utilities that formatted a PC-DOS diskette.  Also, I think that Clearbrook
Software Group has some similar utilities.

Lee



#: 9640 S1/General Interest
    28-Feb-91  22:59:31
Sb: #clibt.ar library
Fm: Bernie 74076,1215
To: all

HELP! Some time ago I downloaded a file named clibt.ar, which contained
relocatable library code and documentation for additional "C" library routines.
The routines included trig functions, time functions, getopt(), and various
other goodies.  Due to a disk problem, I can no longer read the AR file and
have therefore lost the doco. Can anyone tell me where I can find the original
file (or documentation for it) that I can download?

There are 2 Replies.

#: 9649 S1/General Interest
    01-Mar-91  07:39:13
Sb: #9640-clibt.ar library
Fm: Steve Wegert 76703,4255
To: Bernie 74076,1215

Bernie,

As mentioned over in COCO, it's LIB 3 ... and should be close to the top.

Whatcha got going?

Steve

#: 9650 S1/General Interest
    01-Mar-91  08:47:29
Sb: #9640-clibt.ar library
Fm: Pete Lyall 76703,4230
To: Bernie 74076,1215

Bernie -

That should be here in DL3.

Pete

#: 9641 S10/OS9/6809 (CoCo)
    28-Feb-91  23:36:11
Sb: #9363-#OS9 to MSDOS
Fm: Ralph Fehringer 76200,1045
To: Paul Rinear 73757,1413 (X)


Does anyone know of an OS-9 program that will format msdos floppies (I have
tried Marty's RS-DOS utility and can't get pcdos to read them. 

There are 2 Replies.

#: 9651 S10/OS9/6809 (CoCo)
    01-Mar-91  08:48:30
Sb: #9641-OS9 to MSDOS
Fm: Pete Lyall 76703,4230
To: Ralph Fehringer 76200,1045 (X)

Ralph -

I don't know of any functional PC/MSDOS floppy formatters for the coco.

Pete

#: 9657 S10/OS9/6809 (CoCo)
    01-Mar-91  18:51:25
Sb: #9641-OS9 to MSDOS
Fm: Lee Veal 74726,1752
To: Ralph Fehringer 76200,1045 (X)

I think the D.P. Johnson (company) had some cross-system utilities.  Seems like
I remember, too, that Clearbrook Software Group use to have PC-DOS formatter
that ran under OS-9. Lee



#: 9642 S7/Telecommunications
    28-Feb-91  23:53:00
Sb: #9568-Sterm 1.3 bug found
Fm: PaulSeniura 76476,464
To: Ed Gresick 76576,3312 (X)

Wow!  Uploads are free - wonder what CIS thinks of that!  *-)

I use a Courier 9600 HST (real USRobotics but before they upgraded 'em to 14.4k
& 19.2k).  It "defaults" with MNP5 & ARQ mode on CIS and Delphi both, but with
B+ and QB I'm getting 75% thruput as well (local DTE set to 4800 even tho the
line & CIS runs at 2400).  Compression on top of AR'd files are not suppose to
be that good according to the USR book!  Might want to do some research into
the Acia drivers being used cuz I'm using something like 2100 bytes each for
send & receive buffering (read my  ACPDS7.TXT article for more info on that -
still waiting on how to program the undocumented Stat calls!).

-- Thx, Paul Seniura (76476,464)

#: 9643 S7/Telecommunications
    28-Feb-91  23:55:46
Sb: #9569-Sterm 1.3 bug found
Fm: PaulSeniura 76476,464
To: Mark Griffith 76070,41 (X)

Thanks Mark!  It's "the" only thing to use on CIS here!  (Kinda wish Delphi
would ask around for ideas on improving their d/l support, but then again their
20/20 package cannot be beat no matter how slow their I/O gets!)

-- Thx again, Paul Seniura (76476,464).

#: 9644 S10/OS9/6809 (CoCo)
    01-Mar-91  00:00:38
Sb: #9566-speed-up kit for CoCo3?
Fm: PaulSeniura 76476,464
To: Bob van der Poel 76510,2203 (X)

Ooops ... sorry ... I wasn't sure so that's why I said "I thought" it were U. I
see I'm getting Bobs mixed up.  And now I remember Mr. Puppo was the one who
invented the PC-AT interface for "us".  Sorry about that, y'all.

I know what you say about hardware mods, and that's probably why they don't
sell too well.  I myself, however, will do anything to oooch more zip into this
tired machine, cuz I can't even begin to find any way this year whatsoever to
buy them 68k models coming out (as I said earlier here!).

Thx for getting me straight there ... -- Paul Seniura (76476,464).

#: 9645 S10/OS9/6809 (CoCo)
    01-Mar-91  00:19:20
Sb: #9599-Level 2 upgrade?
Fm: PaulSeniura 76476,464
To: Kevin Darling 76703,4227 (X)

Ok I see that the Grfdrv article is not here - I guess back then I only had an
account on GEnie - I'll get it up by the weekend then.  It was sparked by the
25-line text zap found in SuperComm's docs and all due respects paid therein.
I've had a few gripes about my copyrighting these articles - well the record
shows on Delphi that way too many things are plagerized and the patches are
never recorded in the database themselves, which makes other users ask the very
same questions every time the subject comes up around the world.  (Well here on
CIS, too, it's that way but more organized.  :-)  So to stop the abuse, I wrote
up everything we had, did all my own research (again credit is "paid" where it
was due - I do own all of y'all's books, not a photocopied one!), thought up
how to get those other modes working (yep a rewrite was needed) and I spit the
article out in hopes y'all would read it before the upgrades were finalized -
1.5 years ago!  So that's why I do them seemingly legal-sleeze things.  If I
mention something as specific as "I hope the authors of the L-II upgrade will
read this", well that's kinda giving y'all the authority to use it right then &
there - or so I thought!  :-)

As for the stat calls - the ACPDS7.TXT file mushes thru what we've been able to
accomplish so far with our Acia driver - I have been told by Ron Bihler that
Bill Brady will let us share it now.  I'm still waiting for the responses cuz
what we still need help on is already explained in that article (CIS and Delphi
both have it).  Again it's <C>'d cuz of the willful plagerizing that goes on
and I need to keep track of what we are all talking about when the help (e.g.
you & whomever) does come.  In order to support this driver, there is a
customization pgm to set the size of the send & recv buffers (separately). It
is *known* to cure all RiBBS ills, the y-reg problem with C-language pgms, and
the like, plus I can pretty darn well keep up with 9600 uncompressed I/O so
long as the host pauses at a full screen.  It still won't do 1k Xmodem

#: 9646 S10/OS9/6809 (CoCo)
    01-Mar-91  00:28:20
Sb: #9599-Level 2 upgrade?
Fm: PaulSeniura 76476,464
To: Kevin Darling 76703,4227 (X)

uh got cut off ... This ACPDS7.TXT file might shed some light on the subjects
we're needing help on.  Might show something "hidden" that messes up our 1k
Xmodem at 9600.  I actually stated in it that maybe there's a long-term timing
problem between the Acia & modem at 9600 or greater speeds, otherwise I dunno
why 1k Xmodem can't keep up while a whole 1920-byte 80x24 text screen will look
perfect.

I do have the L-I docs that R.S. sold way back then, around when 1.1.0 was
available.  Got the 2.0.0 docs also (they actually had my name on the mailing
list, kin U beleev?!).  So the ACPDS7.TXT shows what we're after and where
we've already been.

This time around, if the cost of an upgrade for L-II becomes such that the
manuals get editted, please consider an "optional" set of manuals for the
people who'd need the "complete" docs on everything.  Even big blue sells their
software/manuals that way: most users simply don't need a Diagnostics book or
example! - that's for the systems pgmrs!

-- Thx, Paul Seniura (76476,464).

#: 9647 S15/Hot Topics
    01-Mar-91  00:45:06
Sb: #9601-High Sierra CDROM fmts
Fm: PaulSeniura 76476,464
To: Kevin Darling 76703,4227 (X)

Our local PBS station just broadcasted this week's "Computer Chronicles" and
the subject was CDROMs!  The companies are finally sending the same CD for both
PCs and Macs with the machine accessing the appropriate application pgms.  So
one hopes those of us who want to hook a drive up, can call or write the
software co. to get the poop on their database formats (as opposed to the ISO
sector & directory formats which *should* be standard, and OS9 would need the
file mgr for).

I called our local CDROM expert - my goodness he didn't want "us" to be able to
read these critters.  He even went so far to wonder whether what we're wanting
to do is a copyright violation.  I said - Listen, if I go down there to plunk
down $895.00 for Compton's Encyclopedia, is THAT a legal copy OR WHAT?

So ... y'all see the flack I'm getting ... bunch of crap if you ask me ... this
might embroil me enough to do some serious letter writing to those govmt
agencies that handle this kind of stuff, from anti-trust to freedom of
information in the case of those NASA CDs being shared (and Library of Congress
etc.).  Wonder if the Supreme Court would want to decide whether an "empire"
like CDROM is turning out to be, if it's unruly to force people to buy
particular kinds of computers instead of providing the format in order to
access a legally-bought CD's information.

IBM publishes their standards!  You can find out how RFT documents work and any
company can write their pgms to support that format (an idea I was hoping would
encroach on the people who write OS9 word processors).  It might be that
Compton's, for example, *does* share its database formats with those who've
bought the CD, and how to uncompress the pictures & animation.  That'd be okay!

Well I babbled on long enough - thx for helping & listening!  -- Paul S.

#: 9648 S4/MIDI and Music
    01-Mar-91  00:50:32
Sb: #9602-#MIDI File code
Fm: PaulSeniura 76476,464
To: Pete Lyall 76703,4230 (X)

Thank you & Tim both!  Yes we will share his stuff for free - never intended to
do otherwise (didn't I make it clear? sorry if not).  Want to make sure Mike
Knudsen & others get his sources at least, for the obvious reasons!

Did Tim want to talk in person or write/email him somehow?  If so let me know
and I'll do what we need to do.

Btw also let me know if the phone tolls need to be reimbursed!

-- Thx, Paul Seniura (76476,464).

There is 1 Reply.

#: 9652 S4/MIDI and Music
    01-Mar-91  08:51:20
Sb: #9648-MIDI File code
Fm: Pete Lyall 76703,4230
To: PaulSeniura 76476,464 (X)

Nope... no further comms are required, and the Internet bore the expense. Just
go ahead with the coding.. and good luck.

Pete

#: 9653 S14/misc/info/Soapbox
    01-Mar-91  13:53:06
Sb: Cheap Tandy Equipment
Fm: Randy Moore 76672,1700
To: Everyone


I have some equipment that MUST GO SOON!  My fiancee says she is tired of
looking at a closet full of computer stuff.  On the block is a MODEL 1000
pc-compatible with 20 meg hard drive, CGA monitor, 640k ram, internal
clock/calendar, 1200 baud modem, and a joystick. Also, I have a CoCo 2 with
Floppy drive, 'Smart' controller, Graphics, Speech, and Assembly cartridges. 
Oh, I almost forgot, there are two printers; a linePrinter V and a DMP110; both
Radio Shack models.

Here's the package deals:
  The model 1000 and both printers for $400.
    or
  The CoCo and both printers for $200.
    or
  All of the above for $500.

If you want just some of these, let me know and we'll work something out.  I
have to get married on April 6 so you know I need the cash!  Thanks,
                                    Randy Moore
                                    76672,1700



#: 9654 S1/General Interest
    01-Mar-91  16:13:57
Sb: #9397-OS9 to MSDOS
Fm: Curtis Veit 76067,3225
To: Rodney Harper 75130,1321 (X)

Hi, There is source for a utility to do this on UNIX systems in the UNIXFORUM
here on Compuserve. It is called M-16 or MT16 I think (sorry about the fuzzy
memory). I'd love to see someone port it to OS9 and OSK!!! (this is one of
those projects I've thought of doing but haven't even had time to look at the
code to see if it would be ugly...  There are others here on the forum that
seem to have lots of experience porting from Unix (any of you guys want to try
your hand at this?)

- Curtis
        ps. that source is probably in the utilities or tools section
        of the Unixforum.

#: 9655 S1/General Interest
    01-Mar-91  16:29:44
Sb: #9503-OS9 -> Mac Hard disk
Fm: Curtis Veit 76067,3225
To: Steve Bliss 75716,117

This could be done a couple of ways. 1. write a clone of the mac file system
for OS9 so your system can read
        the directories and files as they are. 2. Write a utility for both the
Mac and OS9 to read and write using
        some arbitrary simple format (perhaps something already written
        would work, such as tar). You would need to set aside a partition
        on the hard disk for this shared area. (Yes the Mac can partition
        hard drives with third party software like silver lining, (from
        LaCie I think). This can be done by bit diddling on the hard disk
        IF ... 1. You have the info telling how? (I've seen it but I don't
        know where). 2. You are brave and like to risk all the data on your
        disk. 3. Write a utility to pass info from the Mac to OS9 directly over
the SCSI
        port. (this is probably the easy choice (comparatively)). After
choseing one of the above be sure to set up your SCSI IDs so they don't
conflict (I believe the Mac is ID=7, not adjustable). The Mac hard disk is
usually ID=1 and is adjustable directly on the drive if nowhere else.

If you actually attempt this I'd love to hear about it. As you might guess from
the above there might be alot of pitfalls along the road to any of these
solutions.

- Curtis

[D/exit



#: 9656 S6/Applications
    01-Mar-91  18:38:51
Sb: #Unit Help
Fm: JC Hoit 73127,2213
To:  76703,4230 (X)

I just downloaded UNIT.AR. Seems it only wants to run under a VDG 32-column
screen. However, the menus are set up for a larger screen. What's the deal
here?

There are 2 Replies.

#: 9659 S6/Applications
    01-Mar-91  21:30:54
Sb: #9656-#Unit Help
Fm: Pete Lyall 76703,4230
To: JC Hoit 73127,2213 (X)

I doubt it's wired to a 32 character screen.... It was ported from Unix onto a
Gimix 6809 system.....

Why don't we start with some symptoms?

Pete

There is 1 Reply.

#: 9684 S6/Applications
    04-Mar-91  22:10:34
Sb: #9659-Unit Help
Fm: JC Hoit 73127,2213
To: Pete Lyall 76703,4230 (X)

It definitely isn't wired for 32 column. It runs there but doesn't fit.

I think Bob may have a handle on the problem (msg.#9676) and I am going to try
his suggestion. The main symptom (as Bob mentioned) is that the screen just
simply doesn't show up. If I press the proper keys in response to the program's
menu, things happen but no characters ever show up.

Thanks bunches,
 -John-

#: 9676 S6/Applications
    03-Mar-91  20:59:36
Sb: #9656-#Unit Help
Fm: Bob van der Poel 76510,2203
To: JC Hoit 73127,2213 (X)

I recall the same problem with UNIT a long time ago. As I recall was real
simple to fix...the program has a string to clear the screen and the CoCo
doesn't like it. Just change the string to a 0x0c and all should work fine. \ex
post

There is 1 Reply.

#: 9685 S6/Applications
    04-Mar-91  22:12:12
Sb: #9676-Unit Help
Fm: JC Hoit 73127,2213
To: Bob van der Poel 76510,2203 (X)

I think you have something there! Will give it a try. Looks like a very useful
program.

-John-

#: 9660 S5/OS9 Users Group
    02-Mar-91  11:11:05
Sb: #9611-go.ar
Fm: Ken Drexler 75126,3427
To: Steve Wegert 76703,4255 (X)

Thanks.

Ken

#: 9661 S5/OS9 Users Group
    02-Mar-91  11:11:42
Sb: #9620-go.ar
Fm: Ken Drexler 75126,3427
To: Mike Ward 76703,2013 (X)

Thanks, Mike.  I will go grab it.

Ken

#: 9662 S8/BBS Systems/TSMon
    02-Mar-91  17:22:41
Sb: TSMON
Fm: Bob Archambault 76506,3544
To: ALL

Has anyone used the file "TZMON1.AR" from Lib 8. I de-arc'ed itand have it all
on a system disk (level 2). Now I need to know HOW to use it :-)

Is it the same as the TSMON on level 1? Also, how do I go about assigning
passwords (if any)?

Any help greatly appreciated!

Thanx!

 Bob



#: 9664 S10/OS9/6809 (CoCo)
    03-Mar-91  00:23:44
Sb: #Hires Joystick Interface
Fm: NAM PUI 73347,3324
To: all

I  have  encountered  a  couple of problems with  both  my  hires joystick
interface. Both of them seems to get "stuck" half of the time  after starting
up MV and can be freed if I use the keyboard mouse  to get to CONTROL and get
out again. I replaced the IC  in both  of  them. One seems to be fixed for a
few days and back  to the same problem again.

The other problem I encountered with one of them is that when the cursor 
reached about one inch from the right edge or the  bottom edge  of the screen
it "jump" to the edge of the screen. There is nothing  in between. I tried to
fix the problem by replacing  all the   component  on the board. Is there
anybody out there with  a service  manual  covering the part list of the  hires
interface? What  is the value of C1. I replaced all the other components and
the problem presists.

Thank for any help.

               Nam




There is 1 Reply.

#: 9665 S10/OS9/6809 (CoCo)
    03-Mar-91  02:18:11
Sb: #9664-#Hires Joystick Interface
Fm: Kevin Darling 76703,4227
To: NAM PUI 73347,3324 (X)

Nam - define "stuck".  Does it just stay in one place?  Or only move half way
across the screen?  Or?

Added any other hardware lately?  Cleaned off the GIME, too?  best - kev

There are 3 Replies.

#: 9666 S10/OS9/6809 (CoCo)
    03-Mar-91  05:58:23
Sb: #9665-#Hires Joystick Interface
Fm: James Jones 76257,562
To: Kevin Darling 76703,4227 (X)

I think I've seen the behavior Nam Pui describes.  There's a strip down the
right hand side of the screen such that if you enter it, the mouse cursor is
immediately dragged over to the far right side of the screen, making it almost
impossible to position the mouse within that strip.

The problem I've more recently had is jittery mouse, with the mouse cursor
jumping back and forth even when the mouse is stationary.

What this probably *really* means is it's time to seriously look at smouse.ar.

There are 2 Replies.

#: 9668 S10/OS9/6809 (CoCo)
    03-Mar-91  08:20:40
Sb: #9666-#Hires Joystick Interface
Fm: John R. Wainwright 72517,676
To: James Jones 76257,562 (X)

Hey James, I also have a mouse that is very sensitive on the right edge of the
screen.  I can position it, but verrrry carefully.

For your jumpy cursor, try moving the mouse cables around a little. I had the
same thing and it turned out that my (extra long, homemade) cables from the
hires adaptor to the coco were picking up some stray signals.

There are 2 Replies.

#: 9672 S10/OS9/6809 (CoCo)
    03-Mar-91  15:11:49
Sb: #9668-Hires Joystick Interface
Fm: Kevin Darling 76703,4227
To: John R. Wainwright 72517,676 (X)

John - yah, I had to move my mouse cables away from my monitor... got real
jumpy on me.  Also, sometimes I had to remove my joystick for the mouse to work
right... but that went away for some reason.

#: 9678 S10/OS9/6809 (CoCo)
    03-Mar-91  23:40:21
Sb: #9668-Hires Joystick Interface
Fm: James Jones 76257,562
To: John R. Wainwright 72517,676 (X)

Aha!  Thanks for the advice.  Alas, the cartridge port position means that for
right-handed folks, the ergonomically best place for the mouse maximizes the
problem you describe.  I may just try it southpaw to see what happens.

#: 9693 S10/OS9/6809 (CoCo)
    05-Mar-91  20:18:19
Sb: #9666-Hires Joystick Interface
Fm: NAM PUI 73347,3324
To: James Jones 76257,562 (X)

I have looked at smouse.ar and got a serial mouse. (It is currently with my AT)
But, with all the 68K systems arround the corner and all the possible 386's for
OS9000. I am just keeping the COCO the way it it.

Try my best to keep it working until I can afford one of the nice machines.

Nam

#: 9692 S10/OS9/6809 (CoCo)
    05-Mar-91  20:12:08
Sb: #9665-Hires Joystick Interface
Fm: NAM PUI 73347,3324
To: Kevin Darling 76703,4227 (X)

Kevin

I behaves erratically. It moves in the opposite direction about 1/3 of the way
from the bottom of the screen or at the left most of the screen in a straight
line only. Almost as if I have defined the wrong type of interface i.e. defined
low res with the hires interface in.

Nam

#: 9694 S10/OS9/6809 (CoCo)
    05-Mar-91  20:29:54
Sb: #9665-Hires Joystick Interface
Fm: NAM PUI 73347,3324
To: Kevin Darling 76703,4227 (X)

Kevin: Haven't add any hardware recently. Will try cleaning the GIME. The "over
sensitive" right and bottom edge is hires interface dependent and not COCO
deppendent. Could the GIME be the one causing my COCO to hang as I exist
SCULPTOR? This is very strange one I am trying to figure out. I got Sculptor
setup on one COCO. It runs fine. I transported the setup to the other COCO. It
hangs everytimes I exist the main menu.

Nam



#: 9669 S10/OS9/6809 (CoCo)
    03-Mar-91  11:18:50
Sb: #9633-GFX2
Fm: Brother Jeremy, CSJW 76477,142
To: Kevin Darling 76703,4227 (X)

I seem to have gotten it working by ending with a WnSet 0,0 command. As soon as
I get a chance to play with it some more, I will post the results. Tank you,
Br. Jeremy

#: 9670 S12/OS9/68000 (OSK)
    03-Mar-91  12:25:28
Sb: Need 'C' Programmer- MA
Fm: Scott Stingel 73260,3123
To: ALL

Need 'C' programmer/consultant in the Boston metro area to develop radio
communications software.   Must be experienced in writing "embedded"
EPROM-based 'C' code to run on a 68000-family CPU.  Math or engineering
background and standalone (ie: no operating system) programming experience
desirable.   Please send me an EasyPlex. Thanks, Scott Stingel   73260,3123

#: 9671 S10/OS9/6809 (CoCo)
    03-Mar-91  14:54:47
Sb: #Memory
Fm: DAVID DE FEO 71630,721
To: All

I'm trying to slim down my memory requirements to give me more ram, but I've r
run into a problem.  I have a 512k Coco, OS9 level II.  Once I boot up and get
my shell running, mdir says I have 392k ram free.  However, I checked all my
modules in memory, taking into account the 8k minimum block size and all the
merged files and I come up short 48k. OS9boot takes up 32k, shell+ 8k, all the
rest of my loaded utils 16k, and grfdrv 8k.  My term is patched to come up as a
type 2 window and uses 8k. Thats it...72k.  This means I should have 440k free
mem. Where is the other 48k?? Thanks in advance...Dave

There is 1 Reply.

#: 9673 S10/OS9/6809 (CoCo)
    03-Mar-91  15:15:14
Sb: #9671-#Memory
Fm: Kevin Darling 76703,4227
To: DAVID DE FEO 71630,721 (X)

Dave -

Shell itself would need a block for it's data.  The kernel itself may add
another block, plus one for it's data (process descs, path descs, etc).

With MMap and PMap, you should be able to see exactly where all the blocks have
gone.  Got those?

There is 1 Reply.

#: 9675 S10/OS9/6809 (CoCo)
    03-Mar-91  20:27:52
Sb: #9673-Memory
Fm: DAVID DE FEO 71630,721
To: Kevin Darling 76703,4227 (X)



Kevin,

I do have MMap and PMap, but this my first real forage into the heavy duty,
behind the scenes OS9 works so I've been getting "slightly" confused and
disoriented of late :-).  I read in The Complete Rainbow Guide to OS9 that OS9
Level II needs 64K for the operating system (pg 10).  Does this mean that even
if OS9Boot needs only 32K of memory, an additional 32K is still put aside by
the OS?  Are the Boot, OS9P1, and REL part of OS9P2 or are they already in the
system (ROM)?  I've been doing my calculations assuming that they are part of
OS9P2 and take up part of OS9Boot's 32K.  If they are not merged in with OS9P2
then they take up a separate 8K block.  Or do they each take up a separate 8K
block (which comes to 24K).  Even if thats the case, I'm still short 24K
somewhere.  Shell+ is already linked in memory so Term should just take up an
additional 8K for the term-window itself.

I'll try using MMap and PMap again and see if I can get this figured out down
to the BYTE (yeah, right).

Thanks,

Dave

#: 9679 S10/OS9/6809 (CoCo)
    04-Mar-91  03:24:02
Sb: #Memory at 3am
Fm: DAVID DE FEO 71630,721
To: Kevin Darling

With no help from the Tandy OS9 LII manual (man, is it confusing) and with the
help of your pmap and smap utilities, I've come to few conclusions about memory
use under OS9 LII.  Is any of this right or am I way off base??:

When a module is loaded into memory, only its module size uses up memory(at the
top of free RAM).  When a module becomes an active process, its data then uses
up memory(at the bottom of free RAM).  These memory requirements can be found
with ident==>Module size and Data size.

Everything in OS9Boot is considered active and takes up memory in both code
(top) and data(bottom) RAM areas.  All these modules together, along with Boot,
REL, and OS9P1 are known collectively as "System".

If modules are merged, as in OS9Boot, they load without leaving 8K block gaps
between them.  Therefore, if a merged file has modules needing altogether 25K,
then you actually use 32K of RAM or 4 blocks.

Code blocks and data blocks are separate and use up 8K blocks individually of
eachother.

EVEN if the total System memory requirement is less than 64K, 64K is still
reserved and whatever the difference is not useable.

Now for some questions :-) ==>

1) Why doesn't PMap show the memory blocks for active windows?

2) If you iniz or wcreate two 4K windows, do they use up only 8K together, or
do they each use 8K(through my fumblings I've seem to come to the conclusion
that they both wind up in the same 8K block)?

3)Why does SLED use up 16K of data RAM when ident shows it to need only 8K==>
data size: #4101 ??

4) Why do I invariably never get my memory back when I deiniz or display 1b 24
a window?  The window disappears and so does the memory!!!

Hey, who knows...5, 10 more years of this and I might even be able to write a
decent program ;-).

Thanks...Dave

There is 1 Reply.

#: 9686 S10/OS9/6809 (CoCo)
    05-Mar-91  00:53:44
Sb: #9679-#Memory at 3am
Fm: Kevin Darling 76703,4227
To: DAVID DE FEO 71630,721 (X)

Dave - you're right on target, with the sole exception that: the System process
doesn't go ahead and allocate 64K of RAM, but will get more if it needs to.  If
your PMAP shows the system map to be all full up, then that happened.

PMap only shows what "64K images" have been assigned to process descriptors
(it's a Process Map).  It's to help you visualize how block numbers are shared
if they hold a module, and to show that code is mapped in high and data mapped
in at lower addresses, and to help debug memory requirements, etc.

MMap kinda shows the window RAM usage... the window memory comes from the
highest block numbers (with the kernel taking up block 3F at the very top).
WDir (in the libs) will actually tell you the block number(s) being used for
each window, if that'll help.  Each little tool tells a piece <grin>.

The SLED answer: I dunno, but any program can ask for more RAM after it starts
up, which could be what's happening there.

Yes, two 4K windows will try to use the same 8K block if possible. Use DDir to
make sure that the deiniz actually gave up the window.  There is a bug with the
text windows tho... what happens is this: if the window was visible when it's
given up, it is CLS'd.  Unfortunately that happens AFTER a "this block is free"
flag ($FF) was stored in the first byte of that 4K section when the RAM was
given back :-(  So the memory effectively disappears from use. Ouch.  I'll see
if I have a patch.  Fast grfdrv?  - kev

There is 1 Reply.

#: 9687 S10/OS9/6809 (CoCo)
    05-Mar-91  03:22:51
Sb: #9686-#Memory at 3am
Fm: DAVID DE FEO 71630,721
To: Kevin Darling 76703,4227 (X)

Kev...

Thanks so much for the explanations!!!!

Ok..when I did PMap, System used only 48k.  I was still missing 16K somewhere.

Then it kinda dawned on me...I had two immortal shells running.  Since Shell is
loaded in memory, it takes up 8K. When it comes alive in /term, it needs to
take an additional 8K for data.  When the second shell came up, it also needed
an additional 8K for data, but lived in the same 8K code block as the original
shell.  I had counted only 16K for both shells when in reality it was 24K. 
That accounted for 8 of the 16k still missing.  Now, even though mfree is
loaded into memory, when it is called it takes up an 8k block of RAM for ITS
data.  Therefore, when you do an mfree, you actually have an extra 8K that will
be given back once mfree is finished (ie  mfree=48K + 8K for mfree data which
will be returned = 56K).  Did I find my missing 16k or am I reaching for
straws(or bytes)????:-)

As for losing memory with my windows...usually the window is visible when I
deiniz or display 1b 24.  This is because I run basic09 in one window and Sled
in another (sled/basic09<>>>/w#).  If I quit B09 and sled, the window remains
(dead of course).  I use wcreate to make my windows...does this make a
difference?? Actually, I do iniz one window right away and merge stdfonts,etc
to it.

I just download fstgrf today...as a matter of fact I just finished making a
bootable shellplus with alot of the patches I'v been living without(gfx2,
fstgrf,cc3disk.ipc,scffix,new copy and list, and ls).  Iwas able to give myself
an extra 16k of ram(64k total now) with everything either loaded or in an
/r0/cmds/file.  Which comes to my final :-) question.

When I try to format a disk with my newly booted shell+ and patches, I get an
error 237...insufficient Ram.  Mfree says I have 64k free.  Did the CC3Disk
patch cause this??? All other cmds seem to work fine.

CRC of patched CC3IO: $E11F29, Edition #11

Once again, thanks for your patience and help.  I'll get Wdir and see if I can
figure out these windows....does fstgrf fix this???...I didn't check it on the
new boot...hm...

Dave

There is 1 Reply.

#: 9688 S10/OS9/6809 (CoCo)
    05-Mar-91  05:45:06
Sb: #9687-#Memory at 3am
Fm: Kevin Darling 76703,4227
To: DAVID DE FEO 71630,721 (X)

Dave - gee, you sound like an expert <grin>!  Yes, I think you found your
missing memory.

The 237 is different from 207.  207 means not enuf RAM left in the whole
system.  237 means there's no room left in the system 64K map.

In the case of format, that meant there was not enuf system ram (SMap) left to
allocate for the necessary 6K+ track format data buffer.

That's a toughie, there, and I think we all run into it... especially with the
large bootfiles we now have.  Only solution: either kill off some shells, or do
formatting when you first boot up ;-).

PS: is /r0 inside your 512K?  If so, it makes more sense to merge and preload
any commands, instead of storing them on internal ramdisk... as loading and
executing them means you're using twice the RAM!  Ramdisks make more sense for
data only under OS9.  best - kev

There is 1 Reply.

#: 9696 S10/OS9/6809 (CoCo)
    05-Mar-91  21:50:46
Sb: #9688-#Memory at 3am
Fm: DAVID DE FEO 71630,721
To: Kevin Darling 76703,4227 (X)

Kev,

I could've kicked myself when I read about /r0.  I was so enchanted with the
speed, that I totally forgot/didn't realize that I would use up twice the ram.
Oh well, time to write a new OS9Boot :-)!

About error 237...I understand the part about not having enuf system ram left..
SMap does show it using up the full 64K.  But, I don't understand what killing
Shells will do.  I don't have shell in my OS9Boot.  It loads separately with
other merged files and then I link it in the stsrtup file.  OR...does it load
into System ram???  But PMap shows each shell (2 altogether) to occupy a
different 64k block. I'll kill one of the Shells and see if it works, and if it
does I'll be da*ned if I'll know why >:-| !!!

As always, THANKS!!!!

Dave

There is 1 Reply.

#: 9698 S10/OS9/6809 (CoCo)
    06-Mar-91  00:16:34
Sb: #9696-#Memory at 3am
Fm: Kevin Darling 76703,4227
To: DAVID DE FEO 71630,721 (X)

Dave - ok, the part about killing off shells, windows or other programs (last
first) to carve out some system map space for format is because:

OS9 uses up that system space for process and path descriptors, and window
device variables, etc.  Check your SMap, start a new shell, then check SMap
again.  Anywhere from two to four or more pages are used up for each new
process.

So.. by getting rid of the lastmost-setup devices/processes, you can sometimes
regain enough free system map space for the format buffer.
 - kev



There is 1 Reply.

#: 9702 S10/OS9/6809 (CoCo)
    06-Mar-91  12:03:05
Sb: #9698-#Memory at 3am
Fm: DAVID DE FEO 71630,721
To: Kevin Darling 76703,4227 (X)

Kev,

Got it about the system map space!

I finally got up and running with commands loaded into mem instead of /r0 and
patched shell+ so it would only reserve 1 page of mem when it chained/forked a
process instead of 31 pages (thanx Paul Seniura!).  This now leaves me with a
whopping 112K free,  including a 77K ramdisk :-)!! Takes a while to load, but I
think I can live with it (he he!).

Thanks for the help....I really learned a GREAT deal!!!!

Dave

There is 1 Reply.

#: 9710 S10/OS9/6809 (CoCo)
    07-Mar-91  03:10:57
Sb: #9702-Memory at 3am
Fm: Kevin Darling 76703,4227
To: DAVID DE FEO 71630,721 (X)

Dave - heck, I didn't do much... you learned it all yourself!

PS: a secret -- I wrote those utils so *I* could learn it myself, too <grin>.

#: 9682 S1/General Interest
    04-Mar-91  21:26:22
Sb: #OS-9/OS-9000 Features
Fm: William Verthein 76557,3623
To: ALL

I am new to the forum and new to OS-9.  I have been looking into different
operating systems for use in a real time embedded system for my company.  I
have heard a lot of good things about OS-9/OS-9000 and I'd appreciate any help
you forum members can give me.  Some questions I have are:

1)      What company distributes an 80386 version of OS-9000?
2)      Is OS-9000 a real time system (priorities, pre-emption...)?
3)      Does anyone out there use OS-9000 in a real time environment?
4)      Does anyone out there run OS-9000 on an 80386?

Thanx for any help you can give me...

wgv
  

There is 1 Reply.

#: 9781 S1/General Interest
    13-Mar-91  19:46:10
Sb: #9682-OS-9/OS-9000 Features
Fm: David L. Kaleita 72657,2775
To: William Verthein 76557,3623

William, although I can't answer your questions quite yet, give me a couple of
weeks and I might be able to give you a bit of insight. You see, I have OS-9000
on order (it should arrive within the next few days), complete with the RAVE
graphics system. I have been using OS-9 for years and if OS-9000 is even 3/4 of
what OS-9 is, then I predict it is EXACTLY what you are looking for. I decided
to move to OS-9000 after studying a set of OS-9000 and Rave manuals for a
couple of months and finding that Microware has apparently not left anything
out from the OS-9 product, and actually added a few nifty new things.

I'll report back here as soon as I have a chance to play with it for awhile.

By the way, I am the Engineering Manager for a company who designs industrial
controls (primarily for resistance welding robots), hence my interest in real
time control systems. Besides, computers are one of my hobbies and I just HAD
to have the most powerful operating system you can get for a home computer
<grin>!

One last comment (for the benefit of you UG guys that are reading this
message): I'll get back into the OS-9/68000 game when CD-I FINALLY SHOWS UP AT
THE CES IN JUNE!!! In the meantime, I've bought myself a PC.

MS-DOS does indeed suck, and Windows ain't much better. Give me GEM or MAC any
day. I hope I can do some good stuff with Rave.

<Dave Kaleita>

#: 9689 S4/MIDI and Music
    05-Mar-91  06:46:58
Sb: #Rhapso Query
Fm: Ches Looney 73016,1336
To: Denise Tomlinson 71021,3274 (X)

Denise, I had listened to a bit of Rhapsody earlier, but last night I had time
to listen to the whole thing and found that it doesn't quite get to the end.  I
think the last note was an eighth-note chord after bar 230 or 231.  Using DED
to examine the .ar file shows a string of nulls at the end which doesn't look
normal.  Did you have any indication that the upload was unsuccessful?  Have
you downloaded it yourself to check its condition? Perhaps you should chat with
the sysop and maybe upload it again??  Sounds good, and I would like to hear
the proper ending.  There's always the possibility that the problem is on my
end somehow, so please let me know what you find out.  A vagrant thought; you
did end the last measure with a bar, didn't you?  Thanks and regards, Ches.

There is 1 Reply.

#: 9780 S4/MIDI and Music
    13-Mar-91  19:01:04
Sb: #9689-Rhapso Query
Fm: Denise Tomlinson 71021,3274
To: Ches Looney 73016,1336 (X)

Thanks Ches, I'll check it out Huggs, Denise

#: 9691 S10/OS9/6809 (CoCo)
    05-Mar-91  14:44:04
Sb: #SALT problems??
Fm: Dan Charrois 70721,1506
To: all







c/0.1/0.1/ I have a problem with communications on my Coco.  I have used the
serial port for quite some time, both under RSDOS and with OS9 using the
"build-your-own internal RS232 chip" featured in Rainbow several years ago. (I
believe it was called "The forgotten chip".  At any rate, it has just decided
to stop working.  Even using thbitbanger method of communicating with the port
under RSDOS doesn't seem to do the job. I have disconnected my modification
from the SALT chip and the computer is able to communicate with the printer
just fine (I re-installed the trace that needed to be removed as well..) 
Things should be back to normal, but although communication with the printer
through the bitbanger is possible, it is not with the modem. (It seems as
though the modem must be a little more fussy with voltage levels than the
printer is.)  Digging a little deeper, I found that sending a 0 to the port
gave 0.1V at pin6 of the SALT and a 1 ives 4.7V.  This seems fine enough.  But
pin 12, which seems to be connected to the output port (and hence the
peripherals) outputs a 4.1V on a 0, and 1.2V on a 1.  I thought the standard
was in the 12V range..?? At any rate, this subtle difference dsn't make fr
great logic levels, and I think this is why the modem can't figure out what's
going on.
  So, what I'm asking is, is this response to be expected for a SALT chip, or
should I look into installing a new one?  This is rather frustrating since I
operate a BBS under OS9 and it'll have to be down until I fix this.
 Thanks for your reply....Dan

There is 1 Reply.

#: 9697 S10/OS9/6809 (CoCo)
    06-Mar-91  00:06:38
Sb: #9691-#SALT problems??
Fm: Kevin Darling 76703,4227
To: Dan Charrois 70721,1506 (X)

Haven't checked it on my machine, but I believe the output should be around +/-
5 volts... they define RS232 as +/- 3 to 12 volts, I think.

Sounds like no negative regulation going on.  The input at pin 15 should be a
negative voltage (unregulated) of at least -10v.   If not, check those large
diodes at the pwr  supply.

There is 1 Reply.

#: 9708 S10/OS9/6809 (CoCo)
    07-Mar-91  00:23:02
Sb: #9697-SALT problems??
Fm: Dan Charrois 70721,1506
To: Kevin Darling 76703,4227 (X)

Thanks a lot for your reply, Kevin.  I will check out the voltage levels and
see what is going on.  Hopefully I can come up with something productive.
  Thanks....Dan

#: 9695 S14/misc/info/Soapbox
    05-Mar-91  20:55:08
Sb: Tomcat DL15 stuff?
Fm: James Jones 76257,562
To: All

Anyone know what happened to the past weekend's Tomcat status report?  I was
kind of looking forward to seeing what's happening.

#: 9699 S4/MIDI and Music
    06-Mar-91  03:56:10
Sb: #Mfplay
Fm: Ches Looney 73016,1336
To: Paul Seniura 76476,464 (X)

Paul, congrats and encouragement on MFPLAY et al.  Please keep up the good
work.  Ches.

There is 1 Reply.

#: 9720 S4/MIDI and Music
    08-Mar-91  00:03:23
Sb: #9699-#Mfplay
Fm: PaulSeniura 76476,464
To: Ches Looney 73016,1336 (X)

Well thank you!  I'm about to upload a mess of CMFs for the Roland MT32 I found
on CIS' MIDI SIG.  PolySoft shared some demos of their commercial "jukebox"
library.  They sound so good, as soon as I get the MFConverter 100% right, I'm
going to order their libraries!  And then I found four Impromptus (piano
concerts) on IEMUG some time back, so I'll upload those, too.

Once the MFConv utility comes out, I highly discourage uploading and sharing
the CMFs since everyone's MIDI systems are different.  The MFConv util will
have lots of options to selectively NOT output those special MIDI controls.
This means someone could convert then upload an EDITTED PIECE!  That's a no-no
in several of the "permissions" I have seen over at the MIDI SIG, whereby they
want to share their pieces but in their entireity (regardless of the converted
form), which is what these CMFs are that I've uploaded. Let a user convert &
modify his own version, that's okay, but don't upload it.

These are just to get everyone's mouth watering.  I suspect once we can get
into/out-of UME format, we'll ask to delete these versions.  That is, if Mike
Knudsen will start supporting the extra MIDI controls (he knows which ones I
mean :-).

Let me get busy uploading ... -- Thx, Paul Seniura (76476,464).

There is 1 Reply.

#: 9769 S4/MIDI and Music
    11-Mar-91  20:36:25
Sb: #9720-#Mfplay
Fm: Ches Looney 73016,1336
To: PaulSeniura 76476,464 (X)

Paul, I just pulled down your mfconv et al and noted your mention of UnZip v3.0
for OS9.  Where is it?  I can find a couple of versions of unzip for msdos and
C sources, but here I sit without a C compiler.  Any help??  Ches.

There is 1 Reply.

#: 9785 S4/MIDI and Music
    13-Mar-91  23:29:21
Sb: #9769-#Mfplay
Fm: PaulSeniura 76476,464
To: Ches Looney 73016,1336 (X)

Hi.  Unzip 3.0 I found on Delphi and/or the RiBBS HQ BBS.  They kept putting
out a really bad-working version from Sam Smith's Tools BBS (who makes/ports
things to Amiga I think; I forget).  3.0 is the first one that has held up
across different Zip files.  Ported to OS9 by Vaughn Cato.  If somehow we can
get permission, I think I have the complete package as distributed.

-- Paul Seniura.

There is 1 Reply.

#: 9787 S4/MIDI and Music
    14-Mar-91  06:54:25
Sb: #9785-#Mfplay
Fm: Ches Looney 73016,1336
To: PaulSeniura 76476,464 (X)

Oh.  I guess I'm out of luck for a while then since I'm not on Delphi and don't
recognize RiBBS HQ.  Suggestions?  Ches.

There is 1 Reply.

#: 9814 S4/MIDI and Music
    15-Mar-91  20:18:13
Sb: #9787-#Mfplay
Fm: PaulSeniura 76476,464
To: Ches Looney 73016,1336 (X)

Oh lemme peek inside his original file here ... (dontcha love true multitasking
windows so I don't hafta logoff to do it?!).

It seems that Vaughn made this version of UnZip "from the general UnZip that is
provided as source code and is available anywhere".  But he went on to say he
couldn't share the sources for OS9 as modified *because* of a restriction for
sharing modified sources.  He only shared the executable and the short readme
that says this.  I'll post it and let the Sysop decide.

Btw Sam Smith (I *think* it *is* Amiga software he ports things to) is the main
dude to ask for the sources, in fact I've called his BBS up a few times in the
past.  Get a '-?' listing when ya get it runnable, and it'll mention his BBS
phone # etc.  :-)

Frankly I don't like the Zip format -- smells of a copyright violation with the
U.S. Post Office if you ask me.  Plus this is the format that Phil Katz
invented after getting sued by (and lost to) the SEA folks (ARC people), if you
remember that broo-ha-ha.  Katz changes this format, too, more drastically than
any other format I know of (even IBM's mainframe stuff!).

Come to think of it, the PC people with their "software distribution networks"
over the Fido system, has been (still are) using a PAK extension to all of
their compressed files -- AND THIS IS *NOT* COMPATIBLE WITH G.B.Janssen's OS9
Pak utility that is found here.  Moreover, Janssen's PAK is copyrighted a at
least a whole year EARLIER than the earliest copyright for the PC "version". I
promptly reported this to the Fido officials and *boy* did they yell back at
me.  If they do it it's okay, but if we can PROVE we were "first" with a naming
convention and how it can cause confusion, we get our faces slapped.  I mean
this is exactly what SEA/PKWARE were feuding over minus the source-code
stealing.  That slap in my face got me so frustrated (we can't unpak their
goodies etc., plus it IS NOT in a form usable by DeArc no matter what they
say).  I've not kept up with Fido and haven't been hooked up for two or more
months now (mainly getting the MIDI & hardware mods going but the Pak issue

There is 1 Reply.

#: 9819 S4/MIDI and Music
    16-Mar-91  06:54:10
Sb: #9814-Mfplay
Fm: Ches Looney 73016,1336
To: PaulSeniura 76476,464

Paul, that's an interesting list of incompatibles.  I had suspected some of it
without having any details, since I had run into the PAK difference before.
Your aside remark about the pleasure of multi processing allowing a quick look
into another process touches a familiar feeling of mine; ain't it great?  I
trust you know your message was too long and was truncated?  I saw on the MIDI
forum that you had been promised a converter from MFF1 to MFF0; please keep us
posted on that development.  I've used MFCONV to look a bit at the way the
music is encoded and I find it interesting, but I don't have the time (and
probably not the tools/skill) to be of much help other than to send you
encouraging words.  Your work in this area is much appreciated. Regards, Ches.

#: 9703 S6/Applications
    06-Mar-91  12:44:40
Sb: #9585-#Phbook11
Fm: Brian Stretch 76176,1216
To: Tony Cappellini 76370,2104 (X)

Got your check the other day.. thanks!  (Will send you a registered copy as
soon as I can find a proper envelope..)

Edit the modem prefix and add a 1 to the end for long-distance numbers. The 1
is not added automatically to accomodate calling cards, etc.

(You're the third person to register PBook.. nice to know people are enjoying
the program.)

There is 1 Reply.

#: 9852 S6/Applications
    17-Mar-91  23:19:47
Sb: #9703-Phbook11
Fm: Tony Cappellini 76370,2104
To: Brian Stretch 76176,1216

Brian I just finished calling your BBS before I logged into CIS. I forgot that
I left you this message here. Disregard the meesage on your BBS, as it is a
duplicate of the message I left you here. What is different about the
registered copy of Pbook ? Aare there more features, or is it just official.
Any chance of sneding me the source so I can customize my version ? Tony

#: 9704 S10/OS9/6809 (CoCo)
    06-Mar-91  18:20:38
Sb: TSMON
Fm: Bob Archambault 76506,3544
To: ALL

Has anyone used  the program TZMON.AR in lib 8 ? If so could someone please
tell me how to use it :-), is it anything like TSMON under level 1 ? Since it
comes with no docs, I am totally in the dark!!

Any help would be GREATLY appreciated!!!!!

Thanx,

Bob



#: 9705 S10/OS9/6809 (CoCo)
    06-Mar-91  18:35:41
Sb: #DeskMate3
Fm: Floyd Resler 72500,2572
To: all

Deskmate 3 won't run with the 1 meg upgrade.  Is there a patch that will allow
it to run?

There is 1 Reply.

#: 9711 S10/OS9/6809 (CoCo)
    07-Mar-91  03:12:40
Sb: #9705-DeskMate3
Fm: Kevin Darling 76703,4227
To: Floyd Resler 72500,2572 (X)

Hmmm. It must assume that memory block numbers don't go that high.  You're
using the patched VDGInt, right?

Can't recall if I ever tried DM3 under 1 meg... probably not.  You'd have to
just about disasm it to figure out where it was playing games.

#: 9709 S12/OS9/68000 (OSK)
    07-Mar-91  00:39:42
Sb: #ar68.bin problem
Fm: Scott Tegtmeyer 72560,1503
To: All

Dear Forum Members,

I have been trying to run ar68.bin on my 68030 VME computer for several weeks. 
I have contacted several Forum members and Microware customer support, but I
still have problems.

The problem I am having is that when I try to run ar68.bin, OS-9 thinks it is a
procedure file and prints 'Can't execute "J" ...'.
When I do an IDENT on the file I get the message 'incomplete module'. 

When I looked at the file size in the file itself, I found that it was larger
than what the dir command showed.  I think this indicates that the file was
truncated, but I am not sure how this happened.

If anyone has the source to ar68.bin, or knows how to fix the problem, I would
like to hear from you.

Sincerely,

Scott Tegtmeyer 

There is 1 Reply.

#: 9712 S12/OS9/68000 (OSK)
    07-Mar-91  03:18:58
Sb: #9709-#ar68.bin problem
Fm: Kevin Darling 76703,4227
To: Scott Tegtmeyer 72560,1503 (X)

Hi Scott - the source to AR should be in DL9... unfortunately, it's in AR
format :-).

Can you load AR?  If so, then you can Save it back out and that should fix
things up.  Ooops.  Wait.  You say part of it is missing?  You may have to
download it again.

PS: the "can't execute J" thing.... always confuses people.  What that means is
that you have the command in the wrong place.  Try moving it to your commands
directory, and be sure to set execution attributes on it.

Here's the deal.  As you know, OS9 searches memory first, then the exec dir,
and then looks in the data dir for a *shell procedure* text file.  GRIN. Guess
what the first byte of an OS9 module is in ASCII?   If you guessed "J", you're
correct!   The shell tried to run it as a shell script, and got terribly
confused.   best - kev

There is 1 Reply.

#: 9722 S12/OS9/68000 (OSK)
    08-Mar-91  00:57:45
Sb: #9712-#ar68.bin problem
Fm: Scott Tegtmeyer 72560,1503
To: Kevin Darling 76703,4227 (X)

Kevin,

Thanks for responding to my request.

Unfortunately, since the AR program source is in AR format, I can't unpack it
until I get AR running.

I tried downloading the file 3 times, twice on Compuserve and once on a
friend's PC using the Bit-Com communications program.  All three files compared
the same and produced the same result ... 'incomplete module' when I ran the
IDENT program.

I was hoping you might have a copy of AR unpacked which you could send to me or
upload onto Compuserve.

If you can't upload or send the source of AR, maybe you could suggest some
other approach to this problem. 

Thanks,


There is 1 Reply.

#: 9730 S12/OS9/68000 (OSK)
    08-Mar-91  14:09:58
Sb: #9722-ar68.bin problem
Fm: Kevin Darling 76703,4227
To: Scott Tegtmeyer 72560,1503 (X)

Scott - I wonder what's going on?  I just downloaded AR68.BIN (with the B
protocol), and Ident said all was okay.  It was 21,106 bytes long.

What happens when you try to load it?  "load -d ar"  Does OS9 refuse?

I've asked that a copy of a merged text version of the AR source be placed into
DL9 for you... should show up within a coupla days.  Worst case, you can edit
that out into separate files and compile it.  Keep us informed.
  best - kev

#: 9713 S10/OS9/6809 (CoCo)
    07-Mar-91  05:30:16
Sb: #8925-CoCo 3 Emulator?
Fm: MOTD Editor..Bill Brady 70126,267
To: John M Semler 74020,736

I am using the Dove. 30% speed-up is just about right. Makes the SE seem like a
snail.

#: 9714 S10/OS9/6809 (CoCo)
    07-Mar-91  05:32:45
Sb: #9385-LISP for CoCo3
Fm: MOTD Editor..Bill Brady 70126,267
To: Mike Knudsen 72467,1111

Yup, I know all about Wiz Pro, <grin>, and Dales col. I'm glad that *someone*
followed suit. No 64k limit eh? ;)

#: 9715 S9/Utilities
    07-Mar-91  08:38:22
Sb: SCCS/what
Fm: Mark Wuest 74030,332
To: all

I am not sure if anyone else out there does source code version control. We use
something called Software Management System (SMS) from Intesoft in UK. It did
not come with a "what" command like Unix SCCS (with which it is loosely
compatible) so I wrote it. If anyone wants it (other than to just see what it
does), respond and I'll upload it.
 If you just want to know what it does, here it is:
 You put a line in each source code file like this:
 static char *smsid = "$Header$";
 sms does substitution in $Header$ of a string identifying the source code
name, version, and date. "what" displays these strings in a binary (or .r, or
c for that matter) and you can see what versions of what files are linked into
your module. Now you know. If you have no source code control, it will be of
little use.
 Mark

#: 9716 S10/OS9/6809 (CoCo)
    07-Mar-91  12:40:21
Sb: #gfx problem
Fm: Tom Napolitano 70215,1130
To: all


 A friend has found a strange problem with Basic09 and we both would like
 to hear your ideas. From a VDG screen, run a GFX("mode",1,2) GFX("quit").
 Try to rerun the program. I keep getting errors which only clear up with a
 $display # where # can be anything. If I replace the "quit" with a print or
 put #1 chr$($12), I still get the same error. However, if I shell "display 12"
 then the program works just fine.  GFX is just doing a write $12 to CC3IO as
 is the print and put. So why do I need a shell intermediary?
   The error varies from 246 to 207 to others, but is based on problems with
 screen deallocation. Even a $display 0 clears up the problem. Any ideas?

 It sounds like what I experience when io is blocked to a screen.  Instead of
 "display #" if I just do a dir or procs or any command that generates io
 on the current screen it fixes the error.  This also happens when I abort
 a command that uses pipes and so I attributed it to io that doesn't get
 flushed to the stdout (maybe because its buffered?) until you do something
 like running another command that flushes the buffer.

 Is this just another "feature" of os9?



There is 1 Reply.

#: 9719 S10/OS9/6809 (CoCo)
    07-Mar-91  23:00:47
Sb: #9716-#gfx problem
Fm: Kevin Darling 76703,4227
To: Tom Napolitano 70215,1130 (X)

Tom - I can't duplicate the problem here, but then I'm patched a bit.

I wrote a two line basic09 program: run gfx("mode",1,2) and run gfx("quit"),
and it worked over and over.

My GFX brain is rusty tho.  What kind of screens have you used before this is
done, etc?  Also, is a progam always alive on that VDG window?

There is 1 Reply.

#: 9725 S10/OS9/6809 (CoCo)
    08-Mar-91  07:01:24
Sb: #9719-gfx problem
Fm: Tom Napolitano 70215,1130
To: Kevin Darling 76703,4227 (X)

Kevin,
    yes, a program is always running in the window, but I think the vdg screen
was the only one up at the time.
   Thanks,
     tom

#: 9717 S7/Telecommunications
    07-Mar-91  20:17:22
Sb: #more tsmon
Fm: Hugo Bueno 71211,3662
To:  76625,2273 (X)

Bruce,

I've built myself an rs232 cable with swapped DSR/DCD so now there shouldn't be
a problem with the serial port not receiving connect messages from the modem. 
With the swapped DSR/DCD, I now xmode /t2 XTP=85 instead of XTP=05 that I used
previously. Is TSMOn smart enough to deal with the "OK" messages sent back from
the modem?

As far as modem connect, that part is fine. The connection is made, but TSMON
just doesn't recognize the caller's carriage returns. After a call-in attempt,
a PROC command shows that TSMON is suspended.

Variables: 1. I use Dennis Skala's clock driver for the B&B. That driver is
supposed to be compatible with the clock you provide in the Eliminator software
package.

2. My multipak is not upgraded. Before I used the hardware clock driver, the
system time would advance at an exceptional rate during serial port
transmissions.  I notice the keyboard repeat is "enhanced" during serial
transmissions also.  Could it be tha the non-upgraded multipak can be causing
me grief??

Someday this will be behind me, but right now it's tough to keep a smile on my
face!

Hugo



There are 2 Replies.

#: 9718 S7/Telecommunications
    07-Mar-91  22:22:49
Sb: #9717-#more tsmon
Fm: Kevin Darling 76703,4227
To: Hugo Bueno 71211,3662 (X)

Hugo - definitely yes: the non-upgraded MPI is causing your clock/keybd
problems.  It's because when the cpu reads the GIME irq register, your MPI is
turning on and overwhelming the data bus with false info.  The upgraded MPI
doesn't do that.  best - kev

There is 1 Reply.

#: 9726 S7/Telecommunications
    08-Mar-91  11:17:51
Sb: #9718-#more tsmon
Fm: Hugo Bueno 71211,3662
To: Kevin Darling 76703,4227 (X)

My only question is, why do term programs run ok in spite of the "super speed".

Hugo

There is 1 Reply.

#: 9727 S7/Telecommunications
    08-Mar-91  11:22:45
Sb: #9726-#more tsmon
Fm: Kevin Darling 76703,4227
To: Hugo Bueno 71211,3662 (X)

Umm. The term programs only require that the characters incoming are found, and
the extra fake interrupt flags (caused by the MPI) actually would help there,
perhaps... altho causing some cpu time to be wasted checking for irqs that
didn't really exist.

There is 1 Reply.

#: 9732 S7/Telecommunications
    08-Mar-91  16:55:00
Sb: #9727-more tsmon
Fm: Hugo Bueno 71211,3662
To: Kevin Darling 76703,4227 (X)

OK, I've been testing again with my friend today and things were especially
bad. I would start any tsmon (microware's, Bruce's, Bruce's patched by my
friend, etc) and every time, your proc command would show Tsmon suspended.

I've ordered the satellite board upgrade for my mpak from Howard Medical.
Should arrive next week sometime. Hopefully, upgrading will solve the problem
because I just don't see where I'm doing anything wrong. And I want to get UUCP
up and running so bad now!

What's weird is that my friends Mpak isn't upgraded either, and he has no
problems. Such is life.

Hugo

#: 9735 S7/Telecommunications
    08-Mar-91  22:52:02
Sb: #9717-#more tsmon
Fm: Bruce Isted (UG VP) 76625,2273
To: Hugo Bueno 71211,3662 (X)

~ Hugo,
  As Kevin said, the un-upgraded MPI is probably causing some of your problems,
so get it upgraded ASAP.  As for the B&B clock, it should be OK. Actually, it
really wouldn't matter if it had the GIME IRQ toggle or not, except Rx
characters might be lost more often.  But I doubt it'd cause the total lack of
response you're seeing.
  A couple more things to check.  If your modem has LED status lights, can you
see if the Tx and Rx lights come on (virtually) solid as soon as the connection
is made?  If so, your modem echo isn't being turned off by the "initialization"
string properly, although it looked fine in your example "init" file.  Also,
your serial port's echo isn't being turned off by TSMon, though it's supposed
to do that whether or not it was enabled in the first place.
  Also, try enabling "forced DTR".  That'd be "xtp=C5" with swapped DCD+DSR, or
"xtp=45" with regular DSR+DCD.  That should prevent any small period of time
where DTR is dropped when TSMon forks LogIn, though it really shouldn't happen
at all.
  Speaking of LogIn, what happens when you try "TSMon" in a window.  No "init"
file, just start TSMon all by itself.  Does LogIn work properly then, finding
the password file (./SYS/password or /DD/SYS/password, or whatever your LogIn
wants) and so on?
  One other thing is you said "... caller's carriage returns.", but you didn't
say whether the caller tried typing in the full "CONNECT" message followed by a
carriage return.  Please try that and let me know the results.
  I'm sorry I can't be more help, but I only use the TSMon program's most basic
(original) capabilities.  I did have a terrible time writing it (as Pete Lyall
said, and auto-baud TSMon is among the most difficult trivial programs to
write) and getting it to work decently.  And it does work for me, when I test
the auto-baud stuff... though as you've found out some people have no luck with
it at all.
  Bruce

There is 1 Reply.

#: 9749 S7/Telecommunications
    10-Mar-91  08:32:30
Sb: #9735-#more tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted (UG VP) 76625,2273 (X)

Bruce,

The other day I tried the stock tsmon, and immediately upon initialization, a
PROC command would show the process as suspended. The other day it worked fine.

Then I tried your tsmon with and without the initialization file.  Sometimes it
works, sometimes it doesn't (set up corectly). However, sometimes it seems to
set up just fine. Then a caller calls in, and the PROC command shows the
program as suspended with an AGE of 255.

So either with or without an initialization file, your tsmon does absolutely
nothing except get suspended once someone calls in.

By serial port echo, does that mean I should set eko=0 ?

TSMon works fine in windows.

Hugo

There is 1 Reply.

#: 9826 S7/Telecommunications
    16-Mar-91  18:50:28
Sb: #9749-#more tsmon
Fm: Bruce Isted (UG VP) 76625,2273
To: Hugo Bueno 71211,3662 (X)

~ Hugo,
  I don't think being suspended is the problem, but maybe it is a clue.  The
serial driver must be suspending TSMON because it tried to read when there was
no data available, which is normal.  The problem appears to be with either the
hardware or driver for the serial port.
  You need to be using a driver that supports the get/set status calls required
by TSMON, such as SACIA.  ACIAPAK will not do the job, unless it is a
customized version, and even then if there are problems I can't help you at
all.  If the driver isn't at fault, then you need to ensure that DCD is valid
for the 6551 ACIA to receive data.  If you have swapped the DCD+DSR lines, make
sure that your modem forces DSR valid (which is then swapped and hooked up to
the 6551's DCD input).  If you haven't swapped DCD+DSR, then make sure your
modem enables DCD before transmitting any data to the 6551 ACIA.  Also, make
sure that the /T2 descriptor's "swap DCD+DSR" bit in the XTP byte matches the
serial cable.
  I think you mentioned once that you've done the DCD+DSR swap, so the first
thing to do is ensure that the modem forces DSR enabled all the time.
  Bruce

There is 1 Reply.

#: 9835 S7/Telecommunications
    17-Mar-91  09:56:54
Sb: #9826-#more tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted (UG VP) 76625,2273 (X)

Bruce, I'm doing one last ditch effort. On the software end, everything is in
order. I have a swapped DCD/DSR cable, I have set XTP=85, and I'm using the
SACIA.mpi driver.  I'll let you know what happens once I install the satellite
upgrade board in my multipak. Kevin Darling recommended that I perform the
upgrade since it may be possible that my problems are MPI related.

Hugo

There is 1 Reply.

#: 9847 S7/Telecommunications
    17-Mar-91  21:15:00
Sb: #9835-#more tsmon
Fm: Bruce Isted 76625,2273
To: Hugo Bueno 71211,3662 (X)

~
Hugo,
  Yes, by all means do the MPI upgrade.  It could be the problem, I've seen
stranger things!  Anyway, did you check to ensure that your modem forces DSR
(now hooked to the 6551 ACIA's DCD input) enabled?  Also, I assume SACIA has
been set up for the appropriate MPI select code...?  By default the sacia.mpi
driver sets the MPI for floppy controller in slot 4 and RS-232 Pak in slot 1.
  Bruce

There is 1 Reply.

#: 9859 S7/Telecommunications
    18-Mar-91  19:24:44
Sb: #9847-more tsmon
Fm: Hugo Bueno 71211,3662
To: Bruce Isted 76625,2273

As of yesterday, the MPI upgrade board is installed. (My first hardware
soldering project!) .

Now, I need to have someone call in to test that %&$#* TSMON.  If it doesn't
work, I'll scream.

By the way, I was meaning to ask you about that slot select stuff mentioned in
the eliminator manual.  It says something about setting a byte at some offset
in SACIA. I don't quite understand what you were trying to explain.  Right now,
my floppy controller (Disto DC-7) is in Slot 4, B&B controller is in slot 3,
and rs232 pak is in slot 1. Is this the definitely the default that SACIA.mpi
is set for?

I'll let you know how the tsmon stuff goes once I can get Bob Billson to call
in. (He was working with Rich Mailer, if you remember).

Hugo

#: 9723 S1/General Interest
    08-Mar-91  01:57:12
Sb: #Help with ar
Fm: Dale Toyne 76304,2104
To: all









Help!  I download aro9.bin and sr.doc using xmodem, then used DOSOR9.bas on
tyhem to make them readable under os9 [D, then I copied them onto an os9
formated disk along with sterm.bin Sterm.ar but I cannot get AR to work.  What
am I doing wrong?  Maybe I ned something called "Instructions for the complete
idiot." or somet thanks , Dale A. Toyne

There is 1 Reply.

#: 9731 S1/General Interest
    08-Mar-91  15:16:48
Sb: #9723-#Help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Hi Dale.  You already got the hard part done.  Now set the file permissions on
Ar, so that OS-9 will let you load, run, and/or delete it:

 attr /d1/ar e pe w

You might also want to copy it to your CMDS dir.  Or just load it with a full
pathname, like

 load /d1/ar

Okay, once you get it loadable, then you need to know how to use it... which is
the semi-complicated part.  Basically, you CHD to the directory where you want
the broken-out files to end up.  For example, let's say you downloaded sterm.ar
to drive 0.  First, make sure it has the ".ar" extension on the filename.  Now,
if you wanted to break it out to drive 1, you'd say:

 chd /d1               <== where files will go
 ar -x /d0/sterm       <== where sterm.ar is now

All the files will be de-archived to /d1. Ignore any "archive" errors; they're
probably due to xmodem padding adding junk to the file and confusing ar.  You
can also do an "ar -t /d0/sterm" and check what files are in an archive first,
if you wish.  Yell if need help.
 - kev

There is 1 Reply.

#: 9737 S1/General Interest
    09-Mar-91  01:02:40
Sb: #9731-#Help with ar
Fm: Dale Toyne 76304,2104
To: Kevin Darling 76703,4227 (X)

Thanks I'll give it a try an let you know how it works out, Appreciate the
help. Thanks, Dale

There is 1 Reply.

#: 9738 S1/General Interest
    09-Mar-91  02:58:18
Sb: #9737-#Help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Okey-doe.  Let us know if it works.  Oh.  Have you downloaded anything else,
and did those work before?   We'll figure it out (actually, more likely YOU
will figure out, and let us know :-).  cheers - kev

There is 1 Reply.

#: 9739 S1/General Interest
    09-Mar-91  03:10:03
Sb: #9738-#Help with ar
Fm: Dale Toyne 76304,2104
To: Kevin Darling 76703,4227 (X)

I downloaded pacman and your instructions worked great.  But I still can't get
STERM1.ar busted I get the message "ar cannot find sterm1.ar

There is 1 Reply.

#: 9742 S1/General Interest
    09-Mar-91  13:02:56
Sb: #9739-#Help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Hmm. Does "sterm1.ar" really have the ".ar" extension?  Did you give a full
path to it? (assuming you didn't break it out in the same disk/dir)

Better do this: tell us which disk it's on, how many drives you have, etc.
 - kev

There is 1 Reply.

#: 9747 S1/General Interest
    10-Mar-91  05:36:19
Sb: #9742-#Help with ar
Fm: Dale Toyne 76304,2104
To: Kevin Darling 76703,4227 (X)

It has the ar extension.  Its on /d1 and ar is on /d0/cmds. I try to bustt it
and ar says it can't find it.  I try to copy  it and I get "n

There is 1 Reply.

#: 9748 S1/General Interest
    10-Mar-91  05:39:37
Sb: #9747-#Help with ar
Fm: Dale Toyne 76304,2104
To: Dale Toyne 76304,2104 (X)

Half of my message got cut off. I get no permission when i try to copy the file
sterm1.ar the attr's are set for public read, write, and ex

There is 1 Reply.

#: 9752 S1/General Interest
    10-Mar-91  13:29:31
Sb: #9748-#Help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Hmm. Has sterm.ar been copied to a real OS9 disk, like you did with Pacman? You
should be able to
  chd /d1
  ar -x sterm

A "dir e /d1" shows sterm.ar, right?  Ah, maybe you need to take off the
execution permission?  (I haven't checked to see if ar cares about that).

There is 1 Reply.

#: 9758 S1/General Interest
    11-Mar-91  02:33:14
Sb: #9752-#Help with ar
Fm: Dale Toyne 76304,2104
To: Kevin Darling 76703,4227 (X)

I can't get sterm1.ar copied to a real os9 disk. I was able to with Pacman but
not with sterm.  Sterm is still on the dosor9 disk.

There is 1 Reply.

#: 9759 S1/General Interest
    11-Mar-91  02:36:36
Sb: #9758-Help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Ouch. What kind of error do you get when you try to copy sterm.ar to an os9
disk?  Also, what happens if you do an "ar -t /d1/sterm1"  even with the dosor9
disk?

#: 9733 S12/OS9/68000 (OSK)
    08-Mar-91  17:08:15
Sb: #question
Fm: Kevin L. 71521,2723
To: all

 Has anyone heard of a profesinal 68000 based computer made by TBL, or Foxmyer?
I can get one for next to nothing! I would first like to know if I can get any
software for it, especialy OSK. Kevin

There is 1 Reply.

#: 9734 S12/OS9/68000 (OSK)
    08-Mar-91  19:15:46
Sb: #9733-#question
Fm: James Jones 76257,562
To: Kevin L. 71521,2723 (X)

Will the seller let you take a gander at the manuals before you buy?  I think
I'd ask about that.

I've never heard of TBL or Foxmyer.

There is 1 Reply.

#: 9736 S12/OS9/68000 (OSK)
    09-Mar-91  00:09:31
Sb: #9734-question
Fm: Kevin L. 71521,2723
To: James Jones 76257,562 (X)

I may get it free! and I'm not sure about the manuals. If he has any or not but
Why didn't I think about that ? Prety stupid huh? Thanks Kevin



#: 9741 S4/MIDI and Music
    09-Mar-91  05:55:57
Sb: MFConverter.AR
Fm: PaulSeniura 76476,464
To: all


About the MFConverter.AR package I uploaded.  You need to read the
documentation, especially the RULES section, before using the program.
Basically, it's like this:

I'm going to ask that all the Sysops to not accept CMF files (output from the
MFConv program).  In fact I'm asking you not to share any such output on any
system whatsoever.

If the original SMF file can be shared, THEN SHARE IT INSTEAD, and it *should*
be placed on the MIDI SIGs rather than the CoCo or OS9 SIGs.

Once the MFConv and MFPlay programs have been on the OS9 SIGs for a sufficient
amount of time, I will delete the CMFs I have posted myself.  I'll make a new
archive with the two programs and new documentation sans CMF files.  There will
be plenty of SMFs to download and use in the MIDI SIGs everywhere.

I feel by providing some sample CMFs will help in getting a firm grip on how to
use the MFConv program.  These samples can be used as a comparison to see if
you are running MFConv correctly.  After a while, even myself will succumb to
these rules and won't be sharing CMFs anymore.

You're whining "Why the restrictions?" I bet.  If you need reasons, they are
explained in the readme file.  So please read it before commencing.

I'm posting the same rules on every network I have accounts on.

-- Thx, Paul Seniura



#: 9743 S1/General Interest
    09-Mar-91  21:59:06
Sb: #Erase
Fm: Ian Hodgson 72177,1762
To: All

Is there a utility available that will erase a file by writing zeros (or
whatever) over the data before deleting it? Would be useful for security
reasons.

There is 1 Reply.

#: 9744 S1/General Interest
    09-Mar-91  23:12:16
Sb: #9743-#Erase
Fm: James Jones 76257,562
To: Ian Hodgson 72177,1762 (X)

I think I have indeed seen one--it is in the UG library, if memory serves. It
wouldn't be hard to write one, for that matter; just get the file size, and
write out that many zeroes, preferably a sector size or multiple thereof at a
time (save for the last hunk, of course).

There is 1 Reply.

#: 9745 S1/General Interest
    10-Mar-91  00:43:20
Sb: #9744-Erase
Fm: Ian Hodgson 72177,1762
To: James Jones 76257,562 (X)

I'll take a look in the UG library, but hope someone can remember the file name
so I don't have to BROwse for too long! Maybe I should take the time to write
one, but I'm usually too busy writing text instead of programs. Thanks for the
suggestion.

#: 9750 S7/Telecommunications
    10-Mar-91  08:35:18
Sb: #shell+/mail
Fm: Hugo Bueno 71211,3662
To: All

My friend Bob asked me to post this question of his here on CIS:

sg#: 6342 ** Private Mail **
03/09/91 13:45:35
From: BOB BILLSON

Can you ask anyone who might be able to help, how to get 
Shell+ v2.1 NOT to strip the '%' from a command line?
 
I am attempting to write a smart mailer to be used with both of current OS-9 
UUCP programs out there.  In order to be able to handle Internet-style 
addresses properly such as:  bob%kc2wz.uucp@fdurt1.fdu.edu
 
When Shell+ gets done with the address it becomes: bobkc2wz.uucp@fdurt1.fdu 
.edu  definitely not the same thing.
 
Quoting the address like you can do with '!' to protect it from the shell 
doesn't help.  Shell+ still removes the '%'.  I guess no matter what it treats 
the % as a shell variable.
 
Seems like a bug in Shell+.  Does anyone have a way to fix this? 


There is 1 Reply.

#: 9807 S7/Telecommunications
    15-Mar-91  16:47:03
Sb: #9750-#shell+/mail
Fm: Lee Veal 74726,1752
To: Hugo Bueno 71211,3662 (X)

You have to preface any command that has a percent sign (%) in it with a SHELL+
2.1 command to turn off the shell variable feature.

 OS9:-v
 OS9:{command with a % in it}
 OS9:v

 The -v and v turn the variable feature off and on, respectively.


I ran into the same problem with RSB commands which use a % to point to an
drive containing in RS-DOS diskette.

Lee



There is 1 Reply.

#: 9809 S7/Telecommunications
    15-Mar-91  18:45:02
Sb: #9807-#shell+/mail
Fm: Hugo Bueno 71211,3662
To: Lee Veal 74726,1752 (X)

Thanks Lee. I'll send Bob your response to his question!

Hugo Bueno

There is 1 Reply.

#: 9824 S7/Telecommunications
    16-Mar-91  16:09:26
Sb: #9809-shell+/mail
Fm: Lee Veal 74726,1752
To: Hugo Bueno 71211,3662 (X)

No problem.  Glad I could help.

Have a "bueno" day!!!!!

Lee

#: 9751 S12/OS9/68000 (OSK)
    10-Mar-91  12:54:13
Sb: #9560-#OSK Clib.l Order
Fm: Robert Heller 71450,3432
To: Carl Kreider 71076,76

*I* have a working version of LHArc - I ported it from the UNIX version from
unix.sources (ftp'ed from uunet.uu.net).
                Robert

There is 1 Reply.

#: 9761 S12/OS9/68000 (OSK)
    11-Mar-91  04:29:17
Sb: #9751-#OSK Clib.l Order
Fm: Mike Haaland 72300,1433
To: Robert Heller 71450,3432 (X)

This could be interesting, we've been playing with a ported version of LHArc
now for about 6, maybe 8 months!  Did you define a new extended header for OSK
file info? (Store the attributtes, etc...)  This version does, and I'd hate to
see multiple/different versions around for OSK.  We've have been creating and
extracting data with LHArc for some time now.  So we need to keep something
like this standardized.  Know what I mean?

Mike Haaland



There is 1 Reply.

#: 9766 S12/OS9/68000 (OSK)
    11-Mar-91  06:10:45
Sb: #9761-OSK Clib.l Order
Fm: Robert Heller 71450,3432
To: Mike Haaland 72300,1433 (X)

Mike:
   I just did a quick and dirty port of the UNIX version.  I needed it in a
hurry - the PTB on FidoNet decided to change the archive method for FidoNews
from ARC 5.12 to LHArc without warning anyone.  My only other choise would have
been to find someone with a Mess-dos machine to unpack the FidoNews files for
me.  So I FTP'ed the UNIX port of lharc and ported it.  I only use it to unpack
FidoNews issues (a minor pain since the files arrrive on my CP/M-68K machine
and I have to ship the file to my OSK machine to unpack and repack as an .ARC
file for processing on my CP/M-68K machine).  I also ported the UNIX version of
UNZIP too (a simular quick and dirty done in "self-defense").

It seems that the mess-dos world seems to be insisting on using these
non-portable archiving methods...  And seem to have little interest in
supporting people with other operating systems (as if such people are some
oddball minority or something).

               Robert

#: 9753 S1/General Interest
    10-Mar-91  15:15:05
Sb: #Packet Radio
Fm: John Baer 71615,1175
To: ALL

 Hello all.

 I don't know if this question was asked before but, here goes.  I was
 wondering if someone can give the information needed on the hardware/
 software needed to connect OS-9 to "packit" radio?

 I know a cupple of "ham's" in my area, but they are using clone systems
 so that don't help any!  If someone could point me in the right direction,
 any and all info you could give is GREATLY appreciated!!!

 Thanks in advance.

 John Baer 71615,1175

 J

There is 1 Reply.

#: 9757 S1/General Interest
    10-Mar-91  23:18:27
Sb: #9753-Packet Radio
Fm: Wayne Day 76703,376
To: John Baer 71615,1175

John,

"Packet" (not 'Packit') radio is a general term that doesn't always tell
exactly what you're going to be doing.

If you're merely wanting to hook up your computer to a TNC and do real-time
control of the TNC, to talk on the air, do the TNC controlling, etc, then any
terminal program should work... as long as you are NOT using a standard RS-232
ROMPack (which requires that the Carrier Detect be held hi in order for
incoming data to be passed along back to the computer).

Since OS-9 is an operating system that operates on several different, very
divergant, computer systems, you'll have to specify your hardware before we can
tell you much more.

Wayne

#: 9754 S10/OS9/6809 (CoCo)
    10-Mar-91  15:53:42
Sb: Tetris
Fm: Al Fleagle 72527,1354
To: all

Does anyone know where I can get a copy of Tetris for OS9? I lost my copy when
my drive crashed.

#: 9756 S9/Utilities
    10-Mar-91  16:16:12
Sb: #OSK HELP needed
Fm: Brett Wynkoop 72057,3720
To: all

Greeting-
     I have uploaded a modified version of Pete's uptime utility to the utility
lib.  It can be found in uptime2.ar. The mod consists of putting the date and
time in the uptime display. Works great under os9 and under Coherent (the $99
unix clone) My question is why does it bomb out under OSK?!  someone with more
OSK experience please fix it and point the errors out to me as I have been
having no luck with anything involving time under OSK!

      Thanks for any help, and to those folks who use the prog under OS9 enjoy!

-Brett




There are 4 Replies.

#: 9762 S9/Utilities
    11-Mar-91  04:34:02
Sb: #9756-OSK HELP needed
Fm: Mike Haaland 72300,1433
To: Brett Wynkoop 72057,3720 (X)

Brett,

I took a look at your code and found a couple of things you might have missed
in the manual.  First, the 'tm' time structure is defined under 'mktime()' in
the MW C manual.  tm_mon is the number of months AFTER january, so in order to
get the correct month add 1.  The code was also failing to compile cause there
is no headers 'utime.h' or 'lowio.h'. In order to get around that I used an
#ifdef OSK preprocessor directive to include the proper defines and headers for
OSK.  Also I changed the variable 'clock' to 'clck', cause clock is an OSK
function.  All the long's in the code I changed to 'time_t' and added a typedef
long time_t to the OS9 ifdef switch, mainly cause that's what the OSK time
functions return and are defined as in the header 'time.h'.  (Plus it made it
easier for me! It works fine now.  One more thing, If you really meant
/R0/SYS/uptime to be the filename, I assume you're iniz'ing the Ramdisk and
making the SYS directory on /R0 before running the util, right?

New Code in the NEXT MESSAGE

#: 9763 S9/Utilities
    11-Mar-91  04:41:10
Sb: #9756-OSK HELP needed
Fm: Mike Haaland 72300,1433
To: Brett Wynkoop 72057,3720 (X)

/* Uptime - reports how long the system has been up since
**          last reboot. Requires that an 'uptime -' command be
**          placed in the system startup file. The 'uptime -' syntax
**          may only be used by the superuser to initialize the 'uptime'
**          file in /DD/SYS. Using 'uptime' by itself will yield
**          a report of how long it has been since the 'uptime -' 
**          command was run.
**          
**          Note: for speed, it may be better to redefine FNAME
**                to use the RAMDISK, if you have one.
**          
**          by Pete Lyall 76703,4230
**          4/19/89
*/

#include <stdio.h>
#ifdef OSK
#include <time.h>

#define WRITE 0x02
#define READ  0x01
extern int errno;
#else 
#include <utime.h>
typedef long time_t
#endif OSK
/* #include <lowio.h> */

#define FNAME "/DD/SYS/uptime"

time_t time();
time_t clck;     /* changed from 'clock' which is an osk function */
time_t future;
struct tm *tm;

Continued in next message

#: 9764 S9/Utilities
    11-Mar-91  04:42:14
Sb: #9756-OSK HELP needed
Fm: Mike Haaland 72300,1433
To: Brett Wynkoop 72057,3720 (X)


main(argc,argv)
int argc;
char **argv;
{
     int days, hours, minutes, seconds;
     time_t boottime,nowtime, delta;
     int tpath;

     if((argc >1) && (*argv[1] == '-'))
     {
          if(getuid())
               exit(_errmsg(214,"only root user may initialize uptime\n"));
               
          nowtime = time(NULL);

          if((tpath = open(FNAME,WRITE)) == -1)
               if((tpath = creat(FNAME, WRITE | READ)) == -1)
                    exit(_errmsg(errno,"cannot open %s\n", FNAME));

          write(tpath, &nowtime, sizeof(time_t));
          close(tpath);
          exit(0);
     }
     else
     {
          nowtime = time(NULL);
          if((tpath = open(FNAME,READ)) == -1)
               exit(_errmsg(errno,"cannot open %s\n", FNAME));
          read(tpath, &boottime,sizeof(time_t));
          close(tpath);

          delta = nowtime-boottime;
          days = (int)(delta/86400L);
          delta -= (time_t)days * 86400L;
          hours = (int)(delta/3600L);
          delta -= (time_t)hours * 3600L;
          minutes = (int)(delta/60L);
          delta -= (time_t)minutes * 60L;
          seconds = delta;

          time (&clck);
          tm=localtime(&clck);
          fprintf(stdout," %02.02d/%02.02d/%02.02d %02.02d:%02.02d:%02.02d
  up for:  %d days  %d hours  %d minutes %d seconds\n", \
                          tm->tm_year, tm->tm_mon + 1, tm->tm_mday, tm->tm_hour, \
                  tm->tm_min, tm->tm_sec,days, hours, minutes, seconds);

     }
}


#: 9765 S9/Utilities
    11-Mar-91  04:45:44
Sb: #9756-#OSK HELP needed
Fm: Mike Haaland 72300,1433
To: Brett Wynkoop 72057,3720 (X)

All in all it looks like you have a pretty good handle on the time fucntions.
If I can help with anything just holler,

Mike

There is 1 Reply.

#: 9817 S9/Utilities
    15-Mar-91  23:52:17
Sb: #9765-OSK HELP needed
Fm: Brett Wynkoop 72057,3720
To: Mike Haaland 72300,1433 (X)

Greeting-
     Thanks for the help.  I am going to look at the code off line to see where
my errors were.  With luck I will have some of my 6809 stuff moved to OSK by
the fest!

-Brett

#: 9760 S1/General Interest
    11-Mar-91  04:13:46
Sb: #help with ar
Fm: Dale Toyne 76304,2104
To:  76703,4227 (X)

I think I've found the problem.  But I still don't have the solution.  Dosor9
didn't finish with the disk, it was ending with an FC error in 2330.  I think
it only wrote the directory and then ended because sterm1.ar was too long. 
When I tried to us it on sterm.ar it said "too fragmented" and ended.  What now
??




There is 1 Reply.

#: 9767 S1/General Interest
    11-Mar-91  17:02:19
Sb: #9760-#help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Dale - okay, that makes sense.  Under rsdos, try copying the file to a fresh
rsdos disk, so that it's not so broken up.  Also, there's a newer dosor9 in the
libs which handles files larger than 64K... that's the main prob.

There is 1 Reply.

#: 9770 S1/General Interest
    12-Mar-91  01:42:03
Sb: #9767-help with ar
Fm: Dale Toyne 76304,2104
To: Kevin Darling 76703,4227 (X)

Thanks I'll get the newer dosor9 program and try that.  I've already tried
recop recopying to a brand new formatted disk and still too fragmented. thanks
again,
           Dale

#: 9771 S1/General Interest
    12-Mar-91  03:25:02
Sb: #help with ar
Fm: Dale Toyne 76304,2104
To:  76703,4227 (X)

Success !!!!! The newer dosor9 program did the trick. Thanks a lot for all the
help, I really appreciate it. Dale

There is 1 Reply.

#: 9773 S1/General Interest
    12-Mar-91  14:55:23
Sb: #9771-help with ar
Fm: Kevin Darling 76703,4227
To: Dale Toyne 76304,2104 (X)

Excellent!!  You did all the hard work tho.  Thx for keeping at it!
  cheers - kev

#: 9772 S10/OS9/6809 (CoCo)
    12-Mar-91  07:04:11
Sb: RAINBOW Mags forsale
Fm: Bill Henderson 72215,341
To: All

I have for sale a complete set of RAINBOW magazine from December 1982 to
January 1990. If you are interested in purchasing these magazines (all 84 of
them), please leave me a message. I will gladly part with them for the best
offer.

Bill Henderson

#: 9774 S10/OS9/6809 (CoCo)
    12-Mar-91  16:33:43
Sb: Addresses needed
Fm: Floyd Resler 72500,2572
To: All

Many of you have sent me money for the games I have written.  Many thanks! A
However, my database file got scrambled and I lost everyones' addresses. I need
the addresses for two reasons:  so I can send out upgrades and source code
requests and so I can send everyone a copy of my upcoming game for beta
testing.  So, anyone who has sent money for one of my programs, please leave
email with your addresses.  Thanks!

#: 9775 S10/OS9/6809 (CoCo)
    12-Mar-91  20:34:20
Sb: #WD1002 controller
Fm: JOERG SATTLER 74016,631
To: Bruce Isted

Bruce.
 I have been ofered a WD 1002-HDO controller.
 The person that has them has told me that they are a
 direct replacement for the WD 1002-05.
 The instruction set in the WD1002-HDO is more extensive
 but otherwise the same as the WD1002-HDO. Now I have no
 real way to check this out so I am hoping that you may
 know something about these controllers and will be able
 to solve this dillema for me.

 BTW thanks or the repair of the ELIMINATOR board.
                               Joerg Sattler, 74016,631

There are 2 Replies.

#: 9777 S10/OS9/6809 (CoCo)
    13-Mar-91  11:31:40
Sb: #9775-#WD1002 controller
Fm: Pete Lyall 76703,4230
To: JOERG SATTLER 74016,631 (X)

Joerg -

I believe the only difference between the WD-1002-05 and the WD-1002-HDO is
that the latter is HARD DISK ONLY, and has no onboard WD2797 floppy disk
controller.

Pete

There is 1 Reply.

#: 9784 S10/OS9/6809 (CoCo)
    13-Mar-91  22:46:06
Sb: #9777-#WD1002 controller
Fm: JOERG SATTLER 74016,631
To: Pete Lyall 76703,4230 (X)

I was led to believe that the HDO version has both lfloppy as well as hard disk
support.    Did I get it wrong ??    Joerg

There is 1 Reply.

#: 9789 S10/OS9/6809 (CoCo)
    14-Mar-91  13:08:34
Sb: #9784-#WD1002 controller
Fm: Pete Lyall 76703,4230
To: JOERG SATTLER 74016,631 (X)

When I was last paying attention to the WD-1005-xxx series, I was told by Kent
Meyers that the HDO was hard disk only (or was it Steve Odneal, who put out the
predecessor to the Isted system?) That's my only reference to the HDO unit, as
all of mine (3) have been -05's. If you can't get a response from Bruce, try
calling Computer Surplus listed in the Computer Shopper. They were selling
WD-1005's for long time (may still have them) and could probably tell you.

Pete

There is 1 Reply.

#: 9790 S10/OS9/6809 (CoCo)
    14-Mar-91  15:41:40
Sb: #9789-WD1002 controller
Fm: JOERG SATTLER 74016,631
To: Pete Lyall 76703,4230 (X)

Thanks I will do that.   Joerg



#: 9827 S10/OS9/6809 (CoCo)
    16-Mar-91  18:50:31
Sb: #9775-#WD1002 controller
Fm: Bruce Isted (UG VP) 76625,2273
To: JOERG SATTLER 74016,631 (X)

~ Joerg,
  As I said in EMAIL, the WD 1002-HDO is a "Hard Drive Only" version of the WD
1002-05.  It supports hard drives exactly the same as the -05, but can't be
used to control floppy drives.  This is more for others than for you, since I
see you've already seen my EMAIL.
  Bruce

There is 1 Reply.

#: 9836 S10/OS9/6809 (CoCo)
    17-Mar-91  10:34:47
Sb: #9827-WD1002 controller
Fm: JOERG SATTLER 74016,631
To: Bruce Isted (UG VP) 76625,2273 (X)

So the problem of locating a WD 1002-05 still remains.    Joerg

#: 9860 S10/OS9/6809 (CoCo)
    18-Mar-91  22:11:44
Sb: WD1002 controller
Fm: JOERG SATTLER 74016,631
To: Bruce Isted 76625,2273

Well Frank (Hogg) gave me a number to call for RMT. 800 243 6922 but when I
tried it there was no answer. I tried sveral times but had no luck. So I'm not
sure the number is still valid .     Joerg. Ex 1

#: 9782 S10/OS9/6809 (CoCo)
    13-Mar-91  19:59:09
Sb: #Ldgr45.pak
Fm: Denise Tomlinson 71021,3274
To:  76264,142

Tried to use ldgr45.pak, got an error, "module not found". What is Gshell+?
Will the program run as is under runb? Or does it need Gshell+? Is Gshell+ the
same as multiview? I got that if I need it. One other thing, is it an arcd file
(ldgr45)? Thanks, Denise

There is 1 Reply.

#: 9802 S10/OS9/6809 (CoCo)
    14-Mar-91  23:28:04
Sb: #9782-Ldgr45.pak
Fm: DAVID DE FEO 71630,721
To: Denise Tomlinson 71021,3274 (X)

Denise....
      GShell+ is an enhanced GShell for Multivue.  It should be in the Apps lib
but I'm not sure.
       -Dave

#: 9792 S4/MIDI and Music
    14-Mar-91  18:46:40
Sb: #Rhapsody
Fm: Denise Tomlinson 71021,3274
To:  73016,1336 (X)

Ches, you got the whole score. I forgot to add a Fine to the end and put a bar
in. The eigth notes at the end are supposed to be a "stinger". Denise

There is 1 Reply.

#: 9804 S4/MIDI and Music
    15-Mar-91  10:06:00
Sb: #9792-Rhapsody
Fm: Ches Looney 73016,1336
To: Denise Tomlinson 71021,3274 (X)

Thanks for the info Denise - that's an easy fix.  Regards, Ches.

#: 9794 S11/OS9/6809 (Non-CoCo)
    14-Mar-91  18:50:36
Sb: #Non Coco os9
Fm: Denise Tomlinson 71021,3274
To: Sysop (X)

Are there modules that will run under a Coco in Lib 11? Same microprossessor it
looks like?

There is 1 Reply.

#: 9798 S11/OS9/6809 (Non-CoCo)
    14-Mar-91  19:24:02
Sb: #9794-Non Coco os9
Fm: Kevin Darling 76703,4227
To: Denise Tomlinson 71021,3274 (X)

Denise - yah, non-coco OS9 programs should run fine on the CoCo (6809 ones,
that is).  best - kev

#: 9795 S10/OS9/6809 (CoCo)
    14-Mar-91  18:52:26
Sb: #LDGR45.PAK
Fm: Denise Tomlinson 71021,3274
To: Sysop (X)

Is the file "LDGR45.PAK" in library 10, a arced file? I can't get it to run on
my Coco 3 512k using runb Thanks, Denise

There are 2 Replies.

#: 9796 S10/OS9/6809 (CoCo)
    14-Mar-91  18:56:59
Sb: #9795-#LDGR45.PAK
Fm: Pete Lyall 76703,4230
To: Denise Tomlinson 71021,3274 (X)

Denise -

There's yet another archiver/packer/cruncher/compressor floating about called
PAK. Anything with a .pak extension needs that in order to be unPAKed. Check
DL9 for PAK (i.e. BRO/KEY: PAK or BRO PAK*).

Pete

There is 1 Reply.

#: 9811 S10/OS9/6809 (CoCo)
    15-Mar-91  19:01:24
Sb: #9796-#LDGR45.PAK
Fm: Denise Tomlinson 71021,3274
To: Pete Lyall 76703,4230 (X)

Thanks Pete, for the much needed info Huggs, Denise

There is 1 Reply.

#: 9816 S10/OS9/6809 (CoCo)
    15-Mar-91  22:52:30
Sb: #9811-LDGR45.PAK
Fm: Pete Lyall 76703,4230
To: Denise Tomlinson 71021,3274 (X)

De nada, De nise. (g)

Pete

#: 9797 S10/OS9/6809 (CoCo)
    14-Mar-91  18:58:27
Sb: #9795-LDGR45.PAK
Fm: Pete Lyall 76703,4230
To: Denise Tomlinson 71021,3274 (X)

Denise -

Found it... nab PAK.BIN in DL10. That should do it.

Pete

#: 9799 S10/OS9/6809 (CoCo)
    14-Mar-91  20:01:15
Sb: #Voltage level
Fm: Chris Bergerson 72227,127
To: All

I'm looking for some suggestions...

I'm running OS9 level II on my Coco, and would like to monitor the status of a
voltage level as a background task, and periodically record the value of the
(binary) level to a log file.  I've written a program that almost works, but
there is a problem.  I have wired the signal to the left joystick X input.
Apparently, though, the returned value is valid only if I am in the calling
window.

Wiring the signal to the fire button won't work, of course, since if the signal
is true, the keyboard will be locked out for all other processes.

Most of my available ports are tied up.  I've got a hi-res interface tying up
the right joystick input and the casette I/O. The printer, of course, is
hogging T1.  I've got a MultiPak with slot 1 being a dual RS232 pak, slot 3 is
the HD adapter and slot 4 is the floppy controller.  I'd prefer to keep slot 2
open.

What can I wire my signal to, such that it will not conflict/ interfere with
other processes?  The output of my device is either 0.7V or about 5 volts.

There is 1 Reply.

#: 9805 S10/OS9/6809 (CoCo)
    15-Mar-91  11:41:37
Sb: #9799-#Voltage level
Fm: Pete Lyall 76703,4230
To: Chris Bergerson 72227,127 (X)

What about using a bit of buffering circuitry (and possibly level reducing) and
using that cassette data input line? That's certainly unused under os9.

Also - you could get 'dirty' and write a program that interrogates the other
joystick input (using your OWN low level routines to manipulate the joystick
selector MUX and comparator - using the system's would obviously create the
problem you've encountered). Other possibilities include using unused lines on
one of the PIA's and hanging a wire out the back.

Pete

P.S. You could get some joystick tweaking code from the color basic rom
disassemblies, if you have the "UNRAVELLED" series. You'll need to be careful
to lock interrupts while you're manipulating any control registers and restore
things as you found them.

There is 1 Reply.

#: 9831 S10/OS9/6809 (CoCo)
    16-Mar-91  23:18:13
Sb: #9805-Voltage level
Fm: Chris Bergerson 72227,127
To: Pete Lyall 76703,4230 (X)

Thanks for the good suggestions, Pete.  Seems to me that there's also an unused
input to be found on the RGB connector.  I do like the idea, though, of writing
a non-system routine to look at one of the joystick buttons.

#: 9800 S10/OS9/6809 (CoCo)
    14-Mar-91  21:22:50
Sb: #NEED OS9 Term Prog
Fm: Charles L. Mallory 76447,166
To: [F] All

T0: OS9 SYSOP FROM: 76447,166 Charles L. Mallory Looking for: Communications
software compatible w/OS9
    Requirements:
    1. Can be used with Hard drive
    2. has built in or can access wordprocessor while in term mode
    3. Can access OS9 files for uploading while on-line at the terminal screen
    4. Can direct incomming data to /D0 /D1 or /H0 /H1
    5. Ccan be used with auto dial auto answer modem
    7. Compatible with 300-9600 baud modem
    8. several xmit and receive protocols
    9. If possible, can send incomming data to /P as it is received

We are currently using the listed Hdwr

        CoCo 3  512K
        Multipak interfface
        Segate ST251-1 80 meg Hd Ddrive; /H0 and /H1
        Burke & Burke CcoCo XT & XT-RTC Controller Ver. 2.4B
        Tandy 501 Disc Drive /D0 & /D1
        Tandy 300 Baud Direct Connect Modem Pak (Slot )

Tandy CM8 Moniter


        Tandy DMP 130 A Printer

        If you know of software which may conform to the above, or close to
those specs, please leave a message for us. Wwe We also need a more so

Thank you very Much: 76447,166 Charles L. Mallory



There is 1 Reply.

#: 9806 S10/OS9/6809 (CoCo)
    15-Mar-91  11:45:16
Sb: #9800-NEED OS9 Term Prog
Fm: Pete Lyall 76703,4230
To: Charles L. Mallory 76447,166 (X)

Best for use with Compuserve is Sterm version 1.3. Handles BPlus protocol,
which is optimal for file xfers here. Also manages X modem, and possibly
another.

For the minimalist, Xcom9 is best. Fast, small, and handles Xmodem.

I doubt you'll get more than 2400 baud service out of a coco3 running os9/LII.
Interrupt response time, buffering problems, and inherent limitations of the
hardware require special attention and adjustment to get any faster.

Pete

#: 9801 S10/OS9/6809 (CoCo)
    14-Mar-91  22:40:31
Sb: #9793-#Ultimusic os9
Fm: Wayne Day 76703,376
To: Denise Tomlinson 71021,3274 (X)

Uh... well, you can CHAnge the description of the file yourself, Denise.


Just BROWse the file, and at the download prompt, enter: CHA (for CHAnge).

If it's not too much trouble, though, the easiest thing might be just to
re-upload the file as it should have been.

Wayne

There is 1 Reply.

#: 9812 S10/OS9/6809 (CoCo)
    15-Mar-91  19:04:26
Sb: #9801-#Ultimusic os9
Fm: Denise Tomlinson 71021,3274
To: Wayne Day 76703,376 (X)

Thanks, Actually the file is intact, just missing the bar at the end for good
vus visual effects is all. All of my access to Compuserve is long distance, so
I pay "dearly" for the privelege of using it. All access numbers close by are.
Even tynet and such. Im not sure if the Compuserve 1-800 number is cheaper or
not?

There is 1 Reply.

#: 9820 S10/OS9/6809 (CoCo)
    16-Mar-91  06:56:53
Sb: #9812-#Ultimusic os9
Fm: Ches Looney 73016,1336
To: Denise Tomlinson 71021,3274 (X)

Denise, the end bar is not just visual; without it the note(s) in the last
measure do not play.  Perhaps just a change in the description could be added
(or is this what you were asking Wayne to do?).  Ches.

There is 1 Reply.

#: 9822 S10/OS9/6809 (CoCo)
    16-Mar-91  11:25:16
Sb: #9820-Ultimusic os9
Fm: Denise Tomlinson 71021,3274
To: Ches Looney 73016,1336 (X)


The last measure has only the first eigth note showing. After that, there is
only rests to fill the last measure. All you need to do is add a end bar. Yes,
I was asking Wayne to change the message to read that the entire score was
there, only the bar was missing. He replied to me that all I need to do is do a
Bro to the file and reply CHA to change the descript message. Interesting,
Compuserve dosen't tell us how to change a file message once it's uploaded, but
Wayne did. Might make note of this if you want to change file upload messages.
Later, Denise

#: 9803 S1/General Interest
    15-Mar-91  01:09:09
Sb: CoCoPRO!/Alpha Software
Fm: Dave Myers 71750,210
To: all

Mar. 14, 1991 For Immediate Release

   CoCoPRO! Products is pleased to announce the acquisition of Alpha Software
Technologies and their fine line of OS-9/6809 software products. Included in
the new lineup are Data Windows (full-featured database), Data Merger
(mail-merger for use with Data Windows and/or your favorite wordprocessor),
Presto Partner (RAM-resident desktop accessory package), Disk Manager Tree
(complete control over directory structures), Multi-Menu (easily creates
pop-down menus for Multivue), OS-9 Level 2 BBS (complete, ready-to-use bulletin
board system),  The Zapper (disk zapper for OS-9 lv. 1 or 2), and Level II
Tools (25 useful tools to make your computing life easier).
   We are also pleased to announce the planned introduction (at the Chicago
Rainbowfest) of a new OS-9/6809 product, II Tools II. This product will consist
of a SECOND set of 25 useful tools and utilities for OS-9 lv 2, written by
Keith Alphonso with the user's computing convenience in mind. This package will
offer a great amount of flexibility to the OS-9 user, at an exceptional price
for the value
 recieved.
   In other related announcements, we are excited to announce that in addition
to our OS-9/6809 line (the abovementioned products, plus those of Burke & Burke
and other vendors), we will be introducing a line of OS-9/68000 software in the
very near future. Planned introductions include OSk versions of several of the
Alpha Software products mentioned above, as well as a special OSk Tools
package. For those users who own and are comfortable with the OS-9 versions of
these products, the OSk versions will provide familiar software on a hardware
platform which may be somewhat new to the user...and for those who do not own
the OS-9 versions, this product line will offer time-tested utility to the
relatively uncluttered OSk landscape.
   For product and purchasing information, as well as OSk product availibility,
feel free to contact CoCoPRO! Products at (313) 481-3283 1-9 PM EST Mon-Fri,
1-7 PM Sat.     a

#: 9810 S10/OS9/6809 (CoCo)
    15-Mar-91  18:49:03
Sb: #satellite upgrade
Fm: Hugo Bueno 71211,3662
To: All

Hello all, I have a hardware/soldering type question. I just acquired the
satellite upgrade baord for the multipak. The wires on that thing are really
thin.  Question is, do I have to strip the ends a bit before soldering? If yes,
is there a recommended procedure other than wire cutters/strippers? I think
wire strippers would just break the wires since they're so delicate.

This will be my first hardware "hacking" other than creating myself an rs232
cable and installing the 512K upgrade.

Hugo

There are 2 Replies.

#: 9815 S10/OS9/6809 (CoCo)
    15-Mar-91  22:52:01
Sb: #9810-#satellite upgrade
Fm: Pete Lyall 76703,4230
To: Hugo Bueno 71211,3662 (X)

Hugo -

You could just use the blades of a pair of dikes (diagonal cutters) or even a
knife. For really thin wires, I sometimes use the stripper built into those
little wire wrap tools.

Pete

There is 1 Reply.

#: 9833 S10/OS9/6809 (CoCo)
    17-Mar-91  09:53:20
Sb: #9815-satellite upgrade
Fm: Hugo Bueno 71211,3662
To: Pete Lyall 76703,4230 (X)

Thanks for the reply Pete! (re: wire stripping)

Hugo

#: 9821 S10/OS9/6809 (CoCo)
    16-Mar-91  10:06:58
Sb: #9810-#satellite upgrade
Fm: LARRY OLSON 72227,3467
To: Hugo Bueno 71211,3662 (X)

Hugo,
   If you have an enamel coated wire, one way to strip them is with some
sandpaper. You could use a knife too scrape a little test spot on one of the
ends, too see if it is just an enamel coating or not.

Larry

There is 1 Reply.

#: 9834 S10/OS9/6809 (CoCo)
    17-Mar-91  09:54:11
Sb: #9821-#satellite upgrade
Fm: Hugo Bueno 71211,3662
To: LARRY OLSON 72227,3467 (X)

The wires do look like they're coated. Thanks for the suggestion.

Hugo

There is 1 Reply.

#: 9842 S10/OS9/6809 (CoCo)
    17-Mar-91  16:06:57
Sb: #9834-#satellite upgrade
Fm: LARRY OLSON 72227,3467
To: Hugo Bueno 71211,3662 (X)

Hugo,
    Yea, sandpaper works pretty good on enameled wires, you don't run the
chance of nicking the wires. Another process I have used is to run the wire
through the flame of a match or lighter. This will burn the insulation off,
leaving a charred residue on the wire that can be easily removed.
    I only do the flame trick as a last resort because I don't know if heating
the wire up like that weakens it or makes it brittle.
    Maybe someone with more or a metallurgy background would know for sure.

 larry

There are 2 Replies.

#: 9853 S10/OS9/6809 (CoCo)
    18-Mar-91  00:53:15
Sb: #9842-#satellite upgrade
Fm: DAVID DE FEO 71630,721
To: LARRY OLSON 72227,3467 (X)

RE: using the flame method.....I learned about using flame to get insulation
off wires in the army setting up commo equipment.  As a matter of fact, its the
only method I use cause its so easy.  You just have to make sure that the flame
doesn't stay on the wire too long (ie about 3 sec) or else some of the metal
might lose some of its conducting capability.  A good way to be careful is to
watch the insulation.  As soon as it starts to melt, that is long enough.  The
insulation can then be easily pulled off the wire. --Dave

There is 1 Reply.

#: 9861 S10/OS9/6809 (CoCo)
    19-Mar-91  09:53:39
Sb: #9853-satellite upgrade
Fm: LARRY OLSON 72227,3467
To: DAVID DE FEO 71630,721

David,
   I have to agree that if it is done carefully the flame method is in some
cases much better. A very slight nick in a vibration prone wire will cause more
problems then the damage that might be done to the wire by heating it.

Larry

#: 9858 S10/OS9/6809 (CoCo)
    18-Mar-91  19:20:14
Sb: #9842-#satellite upgrade
Fm: Hugo Bueno 71211,3662
To: LARRY OLSON 72227,3467 (X)

As of yesterday, I installed the satellite board and the whole computer still
works! (pat on back).  By the way, I ended up using a pocket knife to slice the
insulation off, it was plastic.

Thanks for your reply, though.

Hugo

There is 1 Reply.

#: 9862 S10/OS9/6809 (CoCo)
    19-Mar-91  10:00:57
Sb: #9858-satellite upgrade
Fm: LARRY OLSON 72227,3467
To: Hugo Bueno 71211,3662

Hugo,
   Thats great, Success stories are always welcome news.



#: 9813 S10/OS9/6809 (CoCo)
    15-Mar-91  19:19:16
Sb: Gshell+
Fm: Denise Tomlinson 71021,3274
To: [F] All

Where can I get Gshell+ ? Is it in the forum or is it commercial software
available? I did a bro Gshell+ but didn't get anything in Lib 10. Thanks,
Denise

#: 9818 S4/MIDI and Music
    16-Mar-91  06:20:02
Sb: MIDIPACK
Fm: Everett Chimbidis 76370,1366
To:  76476,464

Do you need a midipack to use you midi files?

#: 9823 S10/OS9/6809 (CoCo)
    16-Mar-91  14:20:33
Sb: #Gfx2-Help
Fm: Brother Jeremy, CSJW 76477,142
To: All

GFX2-Help Needed I have been working on some ce to run under the upgraded GFX2.
What I want to do is: 1. Open an overlay window. 2. Direct a path to it. 3.
Create either a framed window with scroll bars, or one without. This would be
similar to gport under Multi_Vue. I keep getting 189-Illegal co-ordinates
errors. Is it possible to open an over lay window and start another procedure
in it that would have its own menu bar, etc. Then when finished could you
return to the first window. I have tried to right the code but with no luck.
Also is there any way to have a split/screen with several procedures running at
the same time? Thank you, Brother Jeremy, CSJW

There is 1 Reply.

#: 9825 S10/OS9/6809 (CoCo)
    16-Mar-91  18:05:50
Sb: #9823-#Gfx2-Help
Fm: Floyd Resler 72500,2572
To: Brother Jeremy, CSJW 76477,142 (X)

Keep in mind that any MV window has at least a one character border all the way
around the screen.  If you try to do this, for example, RUN
gfx2("owset",1,0,0,80,24,2,0), it won't work.

There is 1 Reply.

#: 9832 S10/OS9/6809 (CoCo)
    16-Mar-91  23:37:16
Sb: #9825-#Gfx2-Help
Fm: Brother Jeremy, CSJW 76477,142
To: Floyd Resler 72500,2572 (X)

I will try that. What I would like to be able to do is similar to what can be
done on a MAC. Open an overlay with scroll bars, move up and down on it, click
on whatever. Close the overlay, and return to the original window. Can this be
done under OS9 on the COCO3?

There is 1 Reply.

#: 9843 S10/OS9/6809 (CoCo)
    17-Mar-91  17:42:31
Sb: #9832-#Gfx2-Help
Fm: Floyd Resler 72500,2572
To: Brother Jeremy, CSJW 76477,142 (X)

I have opened up an overlay and have establish another MV window in it. However
I have never had any luck with the scroll bars working in an overlay. I'll mess
around with it again and let you know what I come up with.

Floyd

There are 2 Replies.

#: 9846 S10/OS9/6809 (CoCo)
    17-Mar-91  21:14:27
Sb: #9843-Gfx2-Help
Fm: Brother Jeremy, CSJW 76477,142
To: Floyd Resler 72500,2572

Thank you for your response. I will keep trying also, and I will let you know
what I can come up with. I hope that maybe someone else will have some ideas
here on CIS.

With all best wishes, Brother Jeremy, CSJW

#: 9851 S10/OS9/6809 (CoCo)
    17-Mar-91  22:08:23
Sb: #9843-Gfx2-Help
Fm: Kevin Darling 76703,4227
To: Floyd Resler 72500,2572

Yeah, there's a bug in windint having to do with calculating the offsets of
overlay controls... like scrollbars.  Only an overlay in the upper left corner
will work for those right now.

One solution: draw your own controls! <grin>

#: 9828 S10/OS9/6809 (CoCo)
    16-Mar-91  20:06:14
Sb: #MULTI-VUE
Fm: Bob Archambault 76506,3544
To: ALL

I just acquired Multi-Vue from Radio Shack at a nice low price :-) Now I have a
question. Can it be used to run any other programs besides its own?

If I try to run another program like a game or anything that did not come on
the MV disk, it doesn't work. Also some of the files ON that disk won't run
either. A small blue window will pull down from the center of the screen and
then I'll get errors.

So far I've asked myself - WHY did I buy this? What GOOD is it?

I'm hoping that some of you will have the expertise with this thing to help me
out!!

Thanx,

  Bob



There is 1 Reply.

#: 9829 S10/OS9/6809 (CoCo)
    16-Mar-91  20:45:03
Sb: #9828-#MULTI-VUE
Fm: James Jones 76257,562
To: Bob Archambault 76506,3544 (X)

Read up on how to set up aif files to run applications, and check out some of
the examples here in DL 10.  (While you're at it, I'd seriously recommend
grabbing Kent Meyers's patches to gshell.)

There is 1 Reply.

#: 9841 S10/OS9/6809 (CoCo)
    17-Mar-91  15:06:30
Sb: #9829-MULTI-VUE
Fm: Bob Archambault 76506,3544
To: James Jones 76257,562 (X)

Thanx very much, James!

I definitely will do all the things that you mentioned. Last night, after
posting that message, I read further and noticed the section on AIF files and I
wondered if they were the key. But I  thought I would wait for a reply here
from someone who KNEW what they were doing :-)

Is it just me? Or are all the manuals that Tandy put out for OS-9 about as
clear as MUD??  I say this because when I first got into OS-9 itself, I had
about a million questions! So I was just wondering, is it me (am I THAT dumb?),
or are the manuals confusing for a beginner?

Thanx a million again, James, for your advice!!

Bob



#: 9830 S1/General Interest
    16-Mar-91  22:33:52
Sb: Order
Fm: Butch Mooney 76702,1126
To: Dave Myers 71750,210


Hi Dave,

  I have tried to access your BBS as I have done before to place a order and
was unable to. I typed COCOPRO at login but couldn't get past the password. Has
something been changed?

Butch Mooney



#: 9837 S3/Languages
    17-Mar-91  10:51:59
Sb: #termcap.l docs?
Fm: Ken Drexler 75126,3427
To: Pete Lyall

Pete,

I am trying to write a terminal independent clearscreen function in c and want
to use your termcap library from Mark Griffith's sterm package. I have grabbed
the unix termcap manual posted here but it does not have the special functions
you added to get around the lack of an environment under 6809/OS9. Also from
reading sterm.c, the parameters for each function do not seem to correspond to
the unix manual page.

Have you posted the documents for your version of the tercap.l or a header file
for use with it? If so, where should I look?

Thanks for the help.

Ken

There is 1 Reply.

#: 9855 S3/Languages
    18-Mar-91  11:23:49
Sb: #9837-termcap.l docs?
Fm: Pete Lyall 76703,4230
To: Ken Drexler 75126,3427

Ken -

As far as the termcap.l stuff, the biggest thing that changes is that if you
don't allocate a buffer for the tgetent() function, you may use a NULL and a
buffer will be auto-allocated for you. I used it this way for convenience, but
there may be some memory allocation bugs. Simmy Turner took to just allocating
the buffers manually.

As far as the ttytype file, see the 'update' command, if it's here. My 6809
stuff is offline, but I could get to it if you have no other paths.
Essentially, the ttytype file looks like this:

  [+|-|@]devname crttype

There may be multiple lines, one per device. The syntax is:

  + = enabled local terminal
  @ = enabled modem based terminal
  - = disabled terminal

..WHOOPS! I just realized I'm combining two descriptions here! One is the
'ttylist' file associated with Mtsmon, and the other is ttytype.. sorry! The
layout is just:

 /devname  crt_type
 /t2 vt100
 /w1 coco3
 /t3 wyse50

etc.

The file may be in /dd/sys or /r0/sys (latter is faster), and is manipulated
with a utility I called 'ttyset', which should be in DL9.

Sorry about the confusion, and toggle me if you need to be further confused!

Pete

#: 9838 S14/misc/info/Soapbox
    17-Mar-91  12:00:05
Sb: CM-8 $85.00 UPS incl.
Fm: Mike Passer 72750,420
To: All

Need an economical display alternative for your Coco III?

Radio Shack CM-8 RGB monitor for sale...

Yours for $85.00 including UPS ground shipping within the 48 contiguous
states.  Please leave email to 72750,420 or call (203) 445-2285 before
8:30 pm evenings Eastern Standard Time.

Have a good one,
Mike Passer

#: 9839 S10/OS9/6809 (CoCo)
    17-Mar-91  14:26:11
Sb: #Inside OS9 Level II
Fm: Paul Rinear 73757,1413
To: Kevin Darling


    Kevin,
          Have been trying to get a copy of your book "Inside OS9
     Level II". Microcom said it was out of print when I called and
     to try at a later date. I called back a month later and was
     told that they have a lot of requests for this book but they
     still don't have any. Know of another source?

                                           Paul



There is 1 Reply.

#: 9850 S10/OS9/6809 (CoCo)
    17-Mar-91  21:38:42
Sb: #9839-Inside OS9 Level II
Fm: Lee Veal 74726,1752
To: Paul Rinear 73757,1413

Frank Hogg Labs had them for a while.  They might yet.

Lee



#: 9840 S10/OS9/6809 (CoCo)
    17-Mar-91  14:27:58
Sb: #Remote terminal
Fm: Paul Rinear 73757,1413
To: Bruce Isted , Pete Lyall


     Was reading the message string about tsmon and saw that you
  require a different driver SACIA instead of ACIAPAK. Where can
  I get this?
     Also, here is what I want to do; I have an IBM compatible in
  another room which I want to hook to my Coco3 via the RS232 ports.
  I have a multipack with an RS232pak connected to a modem and will
  get another RS232pak for this remote terminal.
     Is it possible with a configuration like this to somehow
  pipeline the modem through OS9 and out to the remote terminal
  where the remote can do an X-modem download at 2400 baud using its
  own program timing?
     When using tsmon with a IBM PC on the other end, what keys
  generate an escape in OS9 ?
     Hope you can help with this,
                                    Thanks,
                                      Paul



There are 2 Replies.

#: 9849 S10/OS9/6809 (CoCo)
    17-Mar-91  21:15:14
Sb: #9840-Remote terminal
Fm: Bruce Isted 76625,2273
To: Paul Rinear 73757,1413

~
Paul,
  You'll find the SACIA driver in my esw110.ar package, available here on CIS
in this forum's CoCo OS-9 data library.  You can hook your CoCo up to a PC,
but you will need to modify the 2nd RS-232 Pak to work at a different address,
even though the two RS-232 Paks are plugged into different MPI slots.  There
is a text file that describes how to do this, but I don't know where it is or
what it is called... maybe BRO/KEY:RS232 in the appropriate LIBs will turn it
up.
  You may also want to install the "MPI IRQ Hack" to allow both RS-232 Paks to
be IRQ driven.  The "MPI IRQ Hack" is described in the manual in esw110.ar, as
well as in other files available for DL here.
  If you're using a serial port descriptor that is set up with "standard" OS-9
values, you'll find that the PC's Esc is CONTROL-BREAK (ESCAPE), Ctrl-E is
BREAK, and Ctrl-C is SHIFT-BREAK.
  Bruce

#: 9856 S10/OS9/6809 (CoCo)
    18-Mar-91  11:28:09
Sb: #9840-Remote terminal
Fm: Pete Lyall 76703,4230
To: Paul Rinear 73757,1413

Paul -

I used to do that when I had the Gimix hooked up. I had 6 terminals and 2
modems connected. I also had a PC in the studio, attached by serial line to the
Gimix. I'd log into the gimix using Procomm to make the PC look like a VT100,
and then use Sterm on the gimix to dial into cis. I'd use Kermit to transfer
files between the two boxes.

You could probably also write a very simple pass-thru utility, but it gets
complicated when you try to figure out how to pass out of band information,
like how to disconnect, for example.

Pete

#: 9844 S8/BBS Systems/TSMon
    17-Mar-91  17:48:42
Sb: Help with LogIn
Fm: Jeff Dugas 74746,3412
To:  76070,41

Mark,

    I downloaded your LogIn utilities and am having some problems setting it
up.  My problem is with the ADDUSER utility.  When I run it it accesses /dd for
a moment then asks for the username and UID.  After answering the prompts, it
reports "adding new user ..." and then ends (I'm back to the shell). I gathered
from the docs that it was supposed to create the necessary files and generally
"set things up".  Do I need to create any files/directories before running
ADDUSER?

-Jeff

#: 9845 S12/OS9/68000 (OSK)
    17-Mar-91  21:11:00
Sb: #The MM/1 Serial Port!
Fm: Keith H. March 70541,1413
To: all

Hello:

Can any one tell me how to hook up my CoCo 3 to a MM/1 a hundred sixty feet
away?

I would like to run spreadsheets, word processors, graphics programs from the
CoCo.

Any Help would be greatly appreached <sp?>

Throught the MM/1 RS-232 port , Serial or Parallel ?

Thanks for the  HELP.

Keith H. March

There are 2 Replies.

#: 9854 S12/OS9/68000 (OSK)
    18-Mar-91  05:59:21
Sb: #9845-The MM/1 Serial Port!
Fm: James Jones 76257,562
To: Keith H. March 70541,1413

At 160 feet you may run into problems.  The RS-232 standard says no more than
fifty feet--this constraint is present because if a serial device puts out a
signal that is just within specs, past that distance it isn't usable.  A place
I used to work had trouble with that once: we had terminals hooked up over a
distance of fifty feet or a bit over, and they worked just fine, but a lab
instrument with RS-232 out was flaky.  A friend with more hardware knowledge
than me or my boss hooked up an oscilloscope, and one could see very easily the
effects of cable capacitance and resistance.  Smoothed that signal right out
into mush.

One can get special low-capacitance cable for longer serial runs, though I
don't recall how far one can go with it.

#: 9857 S12/OS9/68000 (OSK)
    18-Mar-91  11:30:32
Sb: #9845-The MM/1 Serial Port!
Fm: Pete Lyall 76703,4230
To: Keith H. March 70541,1413

Keith -

While the serial spec (well, RS-232C) states a maximum length of 50 feet, I
regularly get away with many times that. Had runs in my old house that were in
excess of 200 feet, and I have been to sites where customers run lines
approaching 1000 feet.

Pete

#: 9863 S4/MIDI and Music
    19-Mar-91  15:25:08
Sb: #New Keyboard Advice
Fm: Mark Wuest 74030,332
To: all

Hi, all.
 I am seeking advice about a keyboard I plan to buy my wife. She wants to learn
to play piano, and I thought an electronic keyboard would be a good way to let
both of us see how serious we are. I have only $500 budgeted. Do you guys have
any suggestions?

 Thanks!
 Mark

There is 1 Reply.

#: 9864 S4/MIDI and Music
    19-Mar-91  16:39:31
Sb: #9863-New Keyboard Advice
Fm: Pete Lyall 76703,4230
To: Mark Wuest 74030,332 (X)

Mark -

Some questions back at you:

Do you want it to be MIDI capable? (highly recommended, and most are)

Do you want full sized keys? (also recommended)

Do you want it to be multi-timbral (be able to play many instruments at once,
i.e. piano, flute, drums, etc.)?

Best bet would be to get something on the lines of a Roland D5 or D10, or
possibly a Kawai K1 or K1-II. The used market has the K1's at under $450
frequently, the D5 may also be near that point (discounted) new.

Two suggestions:

a) Check out the local for sale rags... we have the Recycler here in LA, and
have 4-5 PAGES each week of used musical equipment for sale, mostly priced
aggressively.

b) Type GO MAO (Music Alley Online...a music store here on CIS) and leave a
note for Jamie Robertson. Lots of folks have bought (new) stuff from Jamie at
incredible prices (self included). He's also very friendly, and helpful.
Telling what you're looking for, and what your dollar cap is, and I'm sure he
can provide some suggestions. He's very well thought of on both the MIDI Forum
and on USENET's rec.music.synth group.

Also, pop over to the MIDI Forum and ask questions. Very active forum over
there, and probably every piece of musical gear available has passed through
_somebody's_ hands over there. You'll get the straight skinny on what performs
well, and what doesn't.

Lastly - worst thing you can do is walk into your local music store
uninitiated... The prices posted are fictitious. There's list price, the posted
price, and then there's what the dealer will REALLY sell it for (typically
20-30% below list, sometimes lower). Have your facts together, your reviews
read, and know what the going prices are (approximately). If you have a
reasonable music dealer, he'll come to know you andwill give you the discounted
price w/o asking once you're a regular.

Pete

Press <CR> !>