AT&T 1710

NOTES:   This is a dual NAM unit.
         The ESN prefix is 132 decimal & 84 hex (Hitachi).
         A T & T west: 213-726-5360, east: 1-800-222-5111

NAM programing:

1.  Select the NAM to be programed by entering FCN 6 2 N # FCN.  Where "N"
    is the NAM number 1 or 2 (ignore the error tone).

2.  Enter FCN 6 2 6 RCL to enter programing mode.  (626 spells NAM)

3.  The DOWN key stores each entry and increments the step number.

4.  At any time press FCN 6 2 6 STO to complete and exit programing.

PROGRAMING DATA:

STEP#    #OF DIGITS/RANGE    DISPLAY   DESCRIPTION

01       0000 - 32767        SIDH      SYSTEM ID
02       0 OR 1              LOCAL     LOCAL USE MARK
03       0 OR 1              MINMK     MIN MARK
04       0 OR 1              A-B       A/B SWITCH MARK
05       0 OR 1              NROAM     ROAM INHIBIT
06       10 DIGITS           AREA/TEL  MIN (AREA CODE & PHONE NUMBER)
07       2 DIGITS            SCM       STATION CLASS MARK
08       333 OR 334          IPCH      INITIAL PAGING CHANNEL
09       2 DIGITS            OLC       ACCESS OVERLOAD
10       0 OR 1              SYS       PREFERRED SYSTEM
11       2 DIGITS            GIM       GROUP ID (10 FOR USA)
12       3 DIGITS            LCODE     LOCK CODE
13       0 OR 1              DTMF      CONTINUOUS DTMF
14       0 OR 1              HF        HANDS FREE

NOTE:  1 enables, 0 disables in all single digit entries.

LOCK: Press and hold LOCK for 1.5 seconds.  UNLOCK: Enter three digit code.

SYSTEM SELECT:  F 9 */down to scroll, STO to store.