DIAMONTEL MESA 90X, 99X, 200

NOTES:  These are dual NAM units.
        The ESN prefix is 134 decimal, 86 hex.
        See file MITSTEST.TXT for test mode access.

NAM programing:

1.  Press PWR key for one second to turn on phone.

2.  Wait for wake up cycle to end and display to clear.

3.  Within ten seconds press and hold the END key while entering
    6 9 7 2 8 1 4 (reset code).

4.  Release END.

5.  The phone will display the first data entry.

6.  Press the SEND key to store information and increment the step number.

7.  Press CLR to correct any item.

8.  Press END to complete programing and exit.

PROGRAMING DATA:

STEP#    #OF DIGITS/RANGE    DISPLAY        DESCRIPTION

01       0 OR 1              DUAL NO        0=1 NAM, 1=2 NAMS
02       10 DIGITS           NO1            NAM 1 MIN (AREA CODE AND TEL#)
03       00000 - 32767       SID1           NAM 1 SYSTEM ID
04       0 OR 1              LU             NAM 1 LOCAL USE MARK
05       0 OR 1              E1             NAM 1 MIN MARK
06       333 OR 334          IPCH1          NAM 1 INITIAL PAGING CHANNEL
07       2 DIGITS            AACCOLC1       NAM 1 ACCESS OVERLOAD
08       0 OR 1              PREF           NAM 1 PREFERRED SYSTEM (SEE NOTES)
09       00 TO 15            GIM1           NAM 1 GROUP ID (10 FOR USA)
10       0 OR 1              RI1            NAM 1 ROAM INHIBIT
11       0 OR 1              DTX1           NAM 1 VOX OPERATION
12       0 OR 1              AR1            NAM 1 SYSTEM BUSY REDIAL

If you selected 0 in step 01 go to step 24.

13       10 DIGITS           NO2            NAM 2 MIN (AREA CODE & TEL#)
14       00000 - 32767       SID2           NAM 2 SYSTEM ID
15       0 OR 1              LU2            NAM 2 LOCAL USE MARK
16       0 OR 1              E2             NAM 2 MIN MARK
17       0333 OR 0334        IPCH2          NAM 2 INITIAL PAGING CHANNEL
18       00 TO 15            ACCOLC2        NAM 2 ACCESS OVERLOAD CLASS
19       0 OR 1              PREF2          NAM 2 PREFERRED SYSTEM (SEE NOTES)
20       00 TO 15            GI2            NAM 2 GROUP ID (10 IN USA)
21       0 OR 1              RI2            NAM 2 ROAM INHIBIT
22       0 OR 1              DTX2           NAM 2 VOX OPERATION
23       0 OR 1              AR2            NAM 2 SYSTEM BUSY REDIAL

24       4 DIGITS            SEC            SECURITY CODE
25       0 OR 1              EE             DTMF SIGNALLING (SEE NOTES)
26       0 OR 1              C TONE         CONTINUOUS DTMF
27       0 OR 1              AL             AUTO LOCK
28       0 OR 1              BO             HORN ALERT
29       0 OR 1              BEEP           SERVICE ENTRY BEEP


NOTES:

Preferred system and end to end signalling are automatically set on the
99X model.

To install lock code: With phone out of programing mode press FCN, 7,
NNNN LLL CLR (where NNNN is 4 digit security code and LLL is new lock code).

LOCK: F 2. UNLOCK: Enter three digit code.

SYSTEM SELECT: F 1 displays current, then one of the following to change, CLR
to exit:  0 = Pref/Non pref, 1 = Non pref/pref, 2 = Home only, 3 = Pref only,
4 = Non pref only.