COLT TP 832

NOTES:  This is a single NAM unit.
        The ESN prefix is 174 decimal & AE hex.
        Shintom:  213-328-7200


NAM PROGRAMING:

1.  Turn power on.

2.  If not locked press FUNC 5 to lock.

3.  Enter FUNC # 6 2 6 # FUNC.  (626 SPELLS NAM)

4.  The SEND key stores and increments each step.

5.  You can jump to any entry by pressing END STEP# SEND.

6.  At any time press END FUNC END to complete and exit programing.

7.  The first two (unnumbered) steps below are not strictly programing
    data, and can not be altered, but are shown for clarity.

PROGRAMING DATA:

STEP#    #OF DIGITS/RANGE    DESCRIPTION

         CAN NOT BE CHANGED  MODEL NUMBER & SOFTWARE VERSION
         CAN NOT BE CHANGED  ESN IN HEX
01       3 DIGITS            AREA CODE
02       7 DIGITS            PHONE NUMBER
03       00000 - 32767       SYSTEM ID
04       2 DIGITS            ACCESS OVERLOAD CLASS
05       2 DIGITS            GROUP ID (10 IN USA)
06       0 OR 1              LOCAL USE MARK
07       0 OR 1              MIN MARK
08       3 DIGITS            LOCK CODE
09       0 OR 1              AUTO LOCK
10       3 DIGITS            CALL RESTRICTION CODE (DEFAULTS TO LOCK CODE)
11       2 DIGITS            CALL COUNTER RESET CODE (DEFAULTS TO FIRST TWO
                             DIGITS OF LOCK CODE)
12       0 OR 1              HANDS FREE
13       0 OR 1              HORN ALERT
14       0 TO 3              HORN ALERT TURN OFF DELAY (0 = 2 hrs, 1 = 4 hrs,
                             2 = 8 hrs, 3 = no turn off)
15       2 DIGITS            TOTAL AIRTIME RESET CODE (DEFAULTS TO FIRST TWO
                             DIGITS OF LOCK CODE)

LOCK: F5, UNLOCK: 3 DIGIT CODE

SYSTEM SELECT: F7 = A ONLY, F8 = B ONLY (F7 OR F8 AGAIN WILL TOGGLE BACK TO
PREF/NON PREF)