PART VI.
                 NAM Programming (Reprogramming) Instructions

                          For 30+ Cellular Telephones


-----------------------------------------------------------------------------
PLEASE NOTE: Area specific numbers contained within these programming
             instructions may not be accurate for your cellular area.
-----------------------------------------------------------------------------

                        Programming Instructions for:

                        DIAMONDTEL MESA90X HANDHELD


ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
PRESS FCN 7
ENTER 4 DIGIT SECURITY CODE
ENTER NEW 3 DIGIT UNLOCK CODE
PRESS CLR

PWR up unit
Press "END" and hold within 10 seconds of pwr up
Enter "5132920"
Release END key.

0                                 SEND                DUAL NO

XXXXXXXXXX                        SEND                NO1

_ _ _ _ _                         SEND                SID1

1                                 SEND                LU1

1                                 SEND                EX1

334                               SEND                IPCH1

07                                SEND                ACCOLC1

0                                 SEND                PREF1

10                                SEND                GIM1

0                                 SEND                RI1

1                                 SEND                DTX1

1                                 SEND                AR1

1234                              SEND                SEC

1                                 SEND                EE

1                                 SEND                C TONE

0                                 SEND                AL

0                                 SEND                BO

1                                 SEND                BEEP


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME

TO RESET NAM FROM THE LIMIT OF 3 PROGRAM ATTEMPTS
PWR up unit
Press "END" and hold within 10 seconds of pwr up
TO RESET NAM OF MESA 90 HANDHELD USE THE CODE "6972814"




                        Programming Instructions for:

                        DIAMONDTEL MESA99X HANDHELD


ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
PRESS FCN 7
ENTER 4 DIGIT SECURITY CODE
ENTER NEW 3 DIGIT UNLOCK CODE
PRESS CLR

PWR up unit
Press "END" and hold within 10 seconds of pwr up
Enter "5132920"
Release END key.

0                                 SEND                DUAL NO

XXXXXXXXXX                        SEND                NO1

_ _ _ _ _                         SEND                SID1

1                                 SEND                LU1

1                                 SEND                MIN MARK1

334                               SEND                IPCH1

07                                SEND                ACCOLC1

10                                SEND                GIM1

0                                 SEND                RI1

0                                 SEND                DTX1

0                                 SEND                AR1

1234                              SEND                SEC

1                                 SEND                CONTINUE D.T.M.F.

0                                 SEND                AUTO LOCK

0                                 SEND                BOOSTER


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME




                        Programming Instructions for:

                          GATEWAY CP 900 HANDHELD

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
CURRENT UNLOCK CODE CAN NOT BE SEEN AND MUST BE KNOWN TO CHANGE
THE CURRENT UNLOCK CODE.
PRESS MENU
ENTER 03
ENTER CURRENT 4 DIGIT SECURITY CODE
ENTER NEW 4 DIGIT SECURITY CODE
PHONE WILL AUTO EXIT TO READY

ACTION                            TO STORE            DISPLAY

PRESS MENU  99  ENTR SCRTY CODE(FCTRY PRST IS 9999)  PROGRAM NAM

_ _ _ _ _                         SEND                SID

XXXXXXXXXX                        SEND                PHONE NUMBER

0334                              SEND                IPC

07                                SEND                ACCOL

10                                SEND                GIM

1                                 SEND                MOBILE I.D. NUMBER

1                                 SEND                LOCAL USE MARK

2                                 SEND                SYSTEM SELECT (B)

UPON PRESSING SEND THE PHONE WILL CYCLE TO WAIT  AND THEN RETURN TO THE
READY MODE.

TO DISPLAY THE NEW PHONE NUMBER:

PRESS RCL 00




                         Programming Instructions for:

                           GENERAL ELECTRIC MINI II

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
PRESS FCN 7
ENTER 4 DIGIT SECURITY CODE
ENTER NEW 3 DIGIT UNLOCK CODE
PRESS CLR

PWR up unit
Press and hold END key within 10 seconds of pwr up
Enter "6282905"
Release END key

0                                 Press SEND          DUAL NO

XXXXXXXXXX                        Press SEND          NO1

_ _ _ _ _                         Press SEND          SID1

1                                 Press SEND          LU1

1                                 Press SEND          EX1

0334                              Press SEND          IPCH1

07                                Press SEND          ACCOLC1

0                                 Press SEND          PREF1

10                                Press SEND          GIM1

0                                 Press SEND          RI1

1                                 Press SEND          DTX1

1                                 Press SEND          AR1

1234                              Press SEND          SEC

1                                 Press SEND          EE

1                                 Press SEND          C DTMF

0                                 Press SEND          AL

0                                 Press SEND          BEEP

0                                 Press SEND          BO


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME




                       Programming Instructions for:

                            GENERAL ELECTRIC MINI

ACTION                            TO STORE            DISPLAY
USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
UNLOCK CODES WILL BE CHANGED ONLY IN PROGRAMMING MODE
FOLLOW THE INSTRUCTIONS THAT FOLLOW

PWR up unit
Press and hold CL key within 10 seconds of pwr up
0Enter "7591122"
Release CL key


XXXXXXXXXX                        PRESS SEND          MIN

123                               PRESS SEND          UNLOCK

_ _ _ _ _                         PRESS SEND          SID

1                                 PRESS SEND          LU

1                                 PRESS SEND          MIN MARK

334                               PRESS SEND          IPCH

07                                PRESS SEND          ACCOLC

0                                 PRESS SEND          PS

10                                PRESS SEND          GIM

1                                 PRESS SEND          EE
0                                 PRESS SEND          BOOSTER

1                                 PRESS SEND          AR


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME




                       Programming Instructions for:

                              MITSUBISHI  800

ACTION                            TO STORE            DISPLAY

PWR up unit
Press and Hold STO within 10 Seconds of pwr up
Enter "5474432"
Release STO


0                                 Press SEND          dUAL

XXXXXXXXXX                        Press SEND          NO1

_ _ _ _ _                         Press SEND          SId1

1                                 Press SEND          LU1

0                                 Press SEND          MIN Mark

0334                              Press SEND          IPCH

07                                Press SEND          ACCOLC

0                                 Press SEND          PS1

10                                Press SEND          GI1

1234                              Press SEND          SECUrity

1                                 Press SEND          EE

0                                 Press SEND          dt

1                                 Press SEND          HF

0                                 Press SEND          InHIbit

1                                 Press SEND          C tOnE

0                                 Press SEND          SyS A/B

0                                 Press SEND          dUAL HS

0                                 Press SEND          InHibit Ld


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME




                        Programming Instructions for:

                                MITSUBISHI 900

ACTION                            TO STORE            DISPLAY

PWR up unit
Press and Hold END key within 10 seconds of pwr up
Enter "6972814"
Release END key

0                                 Press SEND          DUAL NO

XXXXXXXXXX                        Press SEND          NO1

_ _ _ _ _                         Press SEND          SID1

1                                 Press SEND          LU1

0                                 Press SEND          EX1

0334                              Press SEND          IPCH1

07                                Press SEND          ACCOLC1

0                                 Press SEND          PREF1

10                                Press SEND          GIM1

0                                 Press SEND          RI1

1                                 Press SEND          DTX1

1                                 Press SEND          AR1

1234                              Press SEND          SEC

1                                 Press SEND          EE

1                                 Press SEND          C DTMF

0                                 Press SEND          AL

0                                 Press SEND          BO

1                                 Press SEND          BEEP

TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME

TO ENTER TEST MODE HOLD END ON PWR UP-CODE 0944635




                        Programming Instructions for:

                              MOTOROLA 8000H


ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED IN STEP 9 OF THE PROGRAMMING
MODE


PWR up unit
Enter   STORE #123456123456 RCL
If the phone is fresh from factory then
Enter   STORE #000000000000 RCL
If the phone is used or already programmed then
Enter   STORE #123456123456 RCL

DISPLAY WILL SHOW    01
PRESS  *

_ _ _ _ _                         *                   02  (SID)

XXX                               *                   03  (Area Code)

XXX XXXX                          *                   04  (Phone #)

14                                *                   05

07                                *                   06

00                                *                   07

123456                            *                   08

123                               *                   09

334                               *                   10

010100                            *                   11

000                               *

PRESS * TO REVIEW ENTRIES

TO BURN NAM:  PRESS SEND WHILE 01,02,03, ETC. IS DISPLAYED

SET TO SCAN B MODE BY :

RCL *  :  PRESS * UNTIL SCAN B MODE SHOWS then:

press store




                        Programming Instructions for:

                      MOTOROLA ULTRA CLASSIC HANDHELD

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THE UNLOCK CODE IS PROGRAMMED IN STEP 8 OF THE PROGRAMMING
MODE


FOR NEW PHONE:  Press FCN, 0 + Security code entered twice (Factory
                preset is 000000),  RCL

The message 01 will appear in the display to confirm programming mode.

Press *                                               01        Press *

1)  _ _ _ _ _                     Press *             02        Press *

2)  XXX                           Press *             03        Press *

3)  XXX XXXX                      Press *             04        Press *

4)  14                            Press *             05        Press *

5)  07                            Press *             06        Press *

6)  10                            Press *             07        Press *

7)  123456                        Press *             08        Press *

8)  123                           Press *             09        Press *

9)  0334                          Press *             10        Press *

10) 010101                        Press *             11        Press *

11) 101                           Press *             12        Press *

Review entries by pressing  "*" repeatedly.

Press SEND to program phone.




                        Programming Instructions for:

                             NEC  P300


ACTION                            TO STORE            DISPLAY

   THESE INSTRUCTIONS FOR SERIAL NUMBERS AFTER 135-839601

Insert NAM Programming Adapter (NECAM #41-2019) into plug connector on P300
phone bottom.

PWR On

RCL # 0 1   to enter test mode.  Phone will display shaded blocks.

RCL # 7 6   to select NAM.  Phone will show 76-
Press 0 #   to program NAM 1.   (NAM 1=0,NAM 2=1,NAM 3=2,NAM 4=3)

RCL # 7 1   to enter programming mode.

XXXXXXXXXX                        PRESS #             MIN

1234                              PRESS #             LOCK CODE

_ _ _ _ _                         PRESS #             SID

10                                PRESS #             GROUP I.D.

0334                              PRESS #             INITIAL PAGING CH

0                                 PRESS #             SYSTEM SELECT (1=A)

07                                PRESS #             ACCOLC

1                                 PRESS #             MIN MARK 1

1                                 PRESS #             LOCAL USE

911                               PRESS #             EMERGENCY NO.

Press Clr (and hold) to exit programming and return to TEST MODE.

Press RCL # 0 2  to burn and exit to standby.



   THESE INSTRUCTIONS FOR SERIAL NUMBERS PRIOR TO 135-839601

Insert NAM Programming Cable (41-2019)
PWR on
RCL # 7 6 to enter TEST MODE
Press 0 # to select NAM.
RCL # 7 1
You are now in Programming Mode.
Enter NAM info as above.
Press and hold CLR to exit.
Pwr down.




                        Programming Instructions for:

                             NEC  P9100


ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
UNLOCK CODES WILL BE CHANGED ONLY IN PROGRAMMING MODE
FOLLOW THE INSTRUCTIONS THAT FOLLOW



Make sure NAM battery is fully charged before attempting programming
Switch power on
Press RCL #01 display will then show shaded blocks

For a USED phone - to clear nam and accumulated call timer
Press RCL #39

To program NAM1
Press RCL #760#
To enter programming mode Press RCL #71

XXXXXXXXXX                        Press #             MIN

1234                              Press #             Lock Code

_ _ _ _ _                         Press #             SYS. I.D.

10                                Press #             G.I. Mark

0334                              Press #             First Paging Channel

0                                 Press #             System Select

07                                Press #             ACCOLC

0                                 Press #             MIN Mark

1                                 Press #             Local Use


TO EXIT PROGRAM MODE AT THIS TIME PRESS CLR AND HOLD
DISPLAY WILL SHOW TEST MODE

TO EXIT TEXT MODE PRESS RCL#02

IF THE MEMORY IS CLEARED VIA RCL #39 DURING THE PROGRAMMING THEN THE PHONE
WILL AUTOMATICALLY ENTER FULL-LOCK AFTER EXITING THE TEST MODE
TO UNLOCK: FCN #XXXX(4 DIGIT LOCK CODE FOR LAST NAM PROGRAMMED).




                        Programming Instructions for:

                                 NOKIA P-30

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
PRESS SEL 7 UNLCODE APPEARS ON THE DISPLAY
ENTER 5 DIGIT SECURITY CODE AND THE CURRENT UNLOCK CODE APPEARS IN
THE DISPLAY PRESS CLR AND ENTER THE NEW FOUR DIGIT UNLOCK CODE
PRESS SEL TO STORE THE NEW CODE - NOTE: IF YOU DON'T PRESS SEL WITHIN
FIVE SECONDS THE DISPLAY WILL CLEAR AND CANCEL THE FUNCTION


PWR up unit
Enter  *17*2001*12345*
HO-Id must appear on display
Press SEL to view current value
Display will be one step behind TO STORE instructions


_ _ _ _ _                         Press SEL           ACCESS  (SID)

1                                 Press SEL           LOCAL

1                                 Press SEL           PhonE n

XXXXXXXXXX                        Press SEL           CLASS

10                                Press SEL           PAGE ch

334                               Press SEL           O-LOAd

07                                Press SEL           GrouP

10                                Press SEL           SEC

12345                             Press SEL          AUTO EXIT PROGRAM MODE

TO EXIT PROGRAMMING MODE AT ANY TIME PRESS "END"

WHEN THE SEL KEY IS PRESSED FOLLOWING THE LAST PARAMETER VALUE, THE PHONE
WILL AUTOMATICALLY EXIT THE NAM PROGRAMMING MODE AND RETURN TO NORMAL
OPERATION




                        Programming Instructions for:

                                NOVATEL PTR800



ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
UNLOCK CODES WILL BE CHANGED ONLY IN PROGRAMMING MODE
FOLLOW THE INSTRUCTIONS THAT FOLLOW


PWR up unit
Press FCN
Press FCN again
Enter *626776*
Display will show CMT REV and a date code - Press Volume Up
Display will show NAM SELECT1  Press Volume Up

_ _ _ _ _       PRESS #           PRESS VOLUME UP     SIDH
                                  PRESS VOLUME UP     SCM
XXXXXXXXXX      PRESS #           PRESS VOLUME UP     MIN
0333            PRESS #           PRESS VOLUME UP     IDCCA
0334            PRESS #           PRESS VOLUME UP     IDCCB
0334            PRESS #           PRESS VOLUME UP     IPCH
07              PRESS #           PRESS VOLUME UP     ACCOLC
10              PRESS #           PRESS VOLUME UP     GIM
123             PRESS #           PRESS VOLUME UP     LOCK A
456             PRESS #           PRESS VOLUME UP     LOCK B
1               PRESS #           PRESS VOLUME UP     OPTION LC
1               PRESS #           PRESS VOLUME UP     OPTION EX
0               PRESS #           PRESS VOLUME UP     OPTION PS
0               PRESS #           PRESS VOLUME UP     OPTION NSC
1               PRESS #           PRESS VOLUME UP     OPTION EE
1               PRESS #           PRESS VOLUME UP     OPTION REP
0               PRESS #           PRESS VOLUME UP     OPTION HA
0               PRESS #           PRESS VOLUME UP     OPTION HF
0               PRESS #           PRESS VOLUME UP     OPTION F1
0               PRESS #           PRESS VOLUME UP     OPTION F2
0               PRESS #           PRESS VOLUME UP     OPTION F3
0               PRESS #           PRESS VOLUME UP     OPTION F4

TO EXIT PROGRAMMING MODE AT ANY TIME PRESS FCN END

FCN FCN *6462257* WILL CLEAR THE NAM IF IT HAS BEEN PROGRAMMED MORE THAN
3 TIMES OR IF THE NEED EXISTS TO CLEAR THE MEMORY




                        Programming Instructions for:

                                NOVATEL PTR825

ACTION                            TO STORE            DISPLAY
PWR up unit
Press FCN
Press FCN again
Enter *697201*
Display will show CMT REV 972  105  Press Volume Up

1                                 PRESS # VOL UP      NAM SELECT 1
_ _ _ _ _                         PRESS # VOL UP      SIDH
10                                PRESS VOL UP        SCM
XXXXXXXXXX                        PRESS # VOL UP      MIN
0333                              PRESS VOL UP        IDCCA
0334                              PRESS VOL UP        IDCCB
0334                              PRESS # VOL UP      IPCH
07                                PRESS # VOL UP      ACCOLC
10                                PRESS # VOL UP      GIM
123                               PRESS # VOL UP      LOCK A
123                               PRESS # VOL UP      LOCK B
1                                 PRESS # VOL UP      LC
1                                 PRESS # VOL UP      OPTION EX
0                                 PRESS # VOL UP      PS - PREF SYSTEM
0                                 PRESS VOL UP        OPTION NSC
1                                 PRESS # VOL UP      OPTION EE-END TO END
1                                 PRESS # VOL UP      OPTION REP
0                                 PRESS # VOL UP      HORN ALERT
0                                 PRESS # VOL UP      HANDS FREE
0                                 PRESS # VOL UP      OPTION F1
0                                 PRESS # VOL UP      OPTION F2
0                                 PRESS # VOL UP      OPTION F3
1                                 PRESS # VOL UP      OPTION F4 AIR RND UP
0                                 PRESS # VOL UP      OPTION F5 FUTURE USE
0                                 PRESS # VOL UP      OPTION F6 FUTURE USE
0                                 PRESS # VOL UP      OPTION F7 FUTURE USE



Programming will now wrap to beginning SIDH display.
Press VOL UP to review entries




                       Programming Instructions for:

                         OKI HANDHELD MODEL # 750

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED FOR IN THE PROGRAMMING SEQUENCE




Pwr up unit
Press (*) and (#) simultaneously
Enter 10 digit Sec Code as follows:  *12345678#
What follows can be done only once!

The display "Enter NEW PW-Sto"
Enter 0123456789 then press STORE

Pwr unit down.

Pwr up unit
Press MENU and RCL simultaneously
Enter 0123456789                                      Software Version and
                                                      ESN Number in HEX

                                                      Clears in 2 secs.

                                                      Spd Dial Mem Clear

Press 0                           Press STO           Def Data Reset

Press 0                           Press STO

                                  NAM 1 Mode

                                                      Own #111 111-1111

XXX XXX XXXX                      Press STO  Vol Up   Security

123456                            Press STO  Vol Up   OPTION

1100                              Press STO  Vol Up   SCM

1010                              Press STO  Vol Up   GIM

10                                Press STO  Vol Up   Unlock #

1234                              Press STO  Vol Up   ACCOLC #

07                                Press STO  Vol Up   IPCH NO.

0334                              Press STO  Vol Up

_ _ _ _ _                         Press STO  Vol Up   System ID:

At this time you may exit the programming mode by pressing CLR to bypass
the other NAM modules.




                       Programming Instructions for:

                         OKI HANDHELD MODEL # 900

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED FOR IN THE PROGRAMMING SEQUENCE


Pwr up unit
Press RCL and MENU simultaneously
Enter 10 digit Sec Code as follows:  *12345678#
What follows can be done only once!

The display "Enter NEW PW-Sto"
Enter 0123456789 then press STORE.
The display "Re-Enter New PW-Sto"
Enter 0123456789 then press STORE to enter Programming Mode.
IF You don't wish to keep the new password then Pwr unit down.


                                                      Software Version and
                                                      ESN Number in HEX

                                                      Clears in 2 secs.

                                                      Spd Dial Mem Clear

Press *                           Press STO           SPD DIAL MEM CLEAR

Press *                           Press STO           DEFAULT DATA CLEAR

                                  NAM 1 Mode

                                                      Own #111 111-1111

XXX XXX XXXX                      Press STO  Vol Up   MIN

123456                            Press STO  Vol Up   SECURITY

_ _ _ _ _                         Press STO  Vol Up   SYSTEM ID:

0334                              Press STO  Vol Up   IPCH

07                                Press STO  Vol Up   ACCOLC #

15                                Press STO  Vol Up   GROUP I.D.

1234                              Press STO  Vol Up   UNLOCK CODE

1010                              Press STO  Vol Up   STATION CLASS

1110                              Press STO  Vol Up   OPTION



At this time you may exit the programming mode by pressing CLR to bypass
the other NAM modules.




                       Programming Instructions for:

                             PANASONIC EB3500



    Charged Battery and Nam Adaptor are needed.

ACTION                        TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED FOR IN THE PROGRAMMING SEQUENCE




*0000# to enter program mode


*1                           Press SND            NAM 1 MODE

_ _ _ _ _                    Press STO 01         SIDH

XXXXXXXXXX                   Press STO 02         OWNDL

0                            Press STO 03         PRESYS

334                          Press STO 04         IPCH

07                           Press STO 05         ACCOLC

10                           Press STO 06         GIM

00                           Press STO 07         DLMT

10                           Press STO 08         SCM

911                          Press STO 09         SPDL

1234                         Press STO 10         LOCK

1 1 0 1 1 0 0 0              Press STO 11         FCN 1

0 0 0 1 0 1 0 0              Press STO 12         FCN 2

1 1 1 1 0 1 1 1              Press STO 13         FCN 3

STO **
END   to program phone




                     Programming Instructions for:

                         COLT TRANSPORTABLE


ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
UNLOCK CODES WILL BE CHANGED ONLY IN PROGRAMMING MODE
FOLLOW THE INSTRUCTIONS THAT FOLLOW

Phone must be locked, to accomplish:   press FUNC 5
Enter:  FUNC #626# FUNC
The software revision date will be shown.
Press SEND
This will advance phone through memory locations.
E.S.N. will be displayed, press SEND again.

XXX                               Press SEND          AREA CODE

XXX XXXX                          Press SEND          PHONE NUMBER

_ _ _ _ _                         Press SEND          SYSTEM ID

07                                Press SEND          ACCOLC

10                                Press SEND          GIM

1                                 Press SEND          LOCAL USE MARK

1                                 Press SEND          MIN MARK (MOBILE ID)

123                               Press SEND          LOCK CODE

0                                 Press SEND          AUTOMATIC LOCK

123                               Press SEND          CALL RESTRICTION

12                                Press SEND          CALL COUNTER RESET

1                                 Press SEND          ENABLE HANDSFREE

0                                 Press SEND          DISABLE HORN ALERT

0                                 Press SEND          HA TURN OFF TIME

12                                Press SEND          TOTAL AIRTIME RESET

TO REVIEW PROGRAMMING AT THIS TIME PRESS SEND.

TO EXIT PROGRAMMING AND STORE DATA AT ANY TIME PRESS
END FUNC END   -    WAKE UP WILL SOUND, PHONE WILL BE LOCKED
ENTER UNLOCK CODE- 123

SYSTEM PREFERENCE MUST BE KEYPAD SELECTED!  PRESS  FUNC 7 FOR "A" NON W/L

                                  OR        PRESS  FUNC 8 FOR "B" W/L SYS.




                        Programming Instructions for:

                     DIAMONDTEL MESA 55 TRANSPORTABLE


ACTION                            TO STORE            DISPLAY

PWR up unit
Press "CL" and hold within 10 seconds of pwr up
Enter "1951426"
Current Mobile I.D. will display

XXXXXXXXXX                        Press SEND                      MIN

123                               Press SEND          1           SECURITY

_ _ _ _ _                         Press SEND          2           SID

1                                 Press SEND          3           LU

1                                 Press SEND          4           MIN MARK

334                               Press SEND          5           IPCH

07                                Press SEND          6           ACCOLC

0                                 Press SEND          7           PREF SYS

10                                Press SEND          8           GIM

1                                 Press SEND          9           EE

1                                 Press SEND          10     ENBL HANDSFREE

0                                 Press SEND          11          RI

04                                Press SEND          12          AUX 1

07                                Press SEND          13          AUX 2

Phone automatically returns to show the 10 digits MIN number at this time
and to indicate that the NAM has been programmed.  The END key should be
pressed to burn the NAM.




                        Programming Instructions for:

                       DIAMONDTEL MESA95 TRANSPORTABLE

ACTION                            TO STORE            DISPLAY

PWR up unit
Press and hold Clr within 10 Seconds of pwr up
Enter "1951426"
Release Clr


0                                 Press SEND          duaAL no

XXXXXXXXXX                        Press SEND          no1

_ _ _ _ _                         Press SEND          SId1

1                                 Press SEND          LU1

1                                 Press SEND          E1

334                               Press SEND          IPCH1

07                                Press SEND          ACCOLC1

0                                 Press SEND          PS1

10                                Press SEND          GI1

5                                 Press SEND          t InC1

1234                              Press SEND          SECUrIty

1                                 Press SEND          EE

0                                 Press SEND          dt

0                                 Press SEND          HF

0                                 Press SEND          InHIbIt

1                                 Press SEND          Ctone

0                                 Press SEND          dIS CU

0                                 Press SEND          dIS IGn
                                                      SEnSE

0                                 Press SEND          DUAL HS


TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME

TO RESET NAM FROM THE LIMIT OF 3 PROGRAM ATTEMPTS
FOLLOW THE BLOCK OF INSTRUCTIONS AT TOP USING "8291112" W/CLR

TO RESET NAM OF MESA 90 HANDHELD USE THE CODE "6972814"




                      Programming Instructions for:

                           FUJITSU MOBILE PHONE

ACTION                            TO STORE            DISPLAY

PWR up unit
Unit must be locked to program.
To lock press F+LOCK
PWR down unit.
PWR up unit.
Within 10 seconds press    #626#7764726 (#NAM#PROGRAM)
A continuous tone will be heard for 7 seconds.
PRESS AND HOLD THE   *   KEY WHILE THE TONE SOUNDS,
                 DO NOT LET GO!
The tone will change to an intermittent tone, then it will stop.
Release the  *  key.

CONGRATULATIONS!!! YOU ARE NOW IN PROGRAMMING MODE!

_ _ _ _ _                         PRESS STOR          1           SIDH

1                                 PRESS STOR          2           LOCAL

1                                 PRESS STOR          3           MIN MARK

XXXXXXXXXX                        PRESS STOR          4           MIN

10                                PRESS STOR          5           STATION

0334                              PRESS STOR          6           IPCH

07                                PRESS STOR          7           ACCOLC

0                                 PRESS STOR          8           PS

10                                PRESS STOR          9           GIM

1234                              PRESS STOR          10          LOCK

1                                 PRESS STOR          11          CALL TIME

2                                 PRESS STOR          12          AUTO LOCK

1                                 PRESS STOR          13          CALL REST

PRESS STOR TO REVIEW ENTRIES.
WHEN AT MODE #1 PRESS SEND TO BURN NAM AND RETURN TO NORMAL OPERATION.

IF PROGRAMMING WAS DONE INCORRECTLY A SHORT HIGH TONE WILL BE HEARD, YOU
MUST THEN REPEAT DATA ENTRY. YOU MUST PRESS STOR AFTER EACH ENTRY FOR THE
CHECKSUM FUNCTION TO BE FULFILLED.




                       Programming Instructions for:

                      GENERAL ELECTRIC CARFONE XR3000

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THE UNLOCK CODE IS PROGRAMMED IN STEP 2 OF THE PROGRAMMING
MODE



PWR up unit
Press "CL" and hold within 10 seconds of pwr up
Enter "923885"
Serial # will display
Press Send key to advance to first entry

XXXXXXXXXX                        Press SEND          MIN

123                               Press SEND          UNLOCK

_ _ _ _ _                         Press SEND          SID

1                                 Press SEND          LU

1                                 Press SEND          MIN MARK

334                               Press SEND          IPCH

07                                Press SEND          ACCOLC

0                                 Press SEND          PS

10                                Press SEND          GIM

0                                 Press SEND          AUX

1                                 Press SEND          HANDS


PRESS SEND TO REVIEW ENTRIES.  NOTE: AREA CODE (402) WILL DISPLAY FOR MIN
THEN AUTO SWITCH TO REST OF NUMBER ON DISPLAY - BE PATIENT

PRESS "E" KEY TO COMPLETE PROGRAMMING OF THE XR 3000 AT THIS TIME




                       Programming Instructions for:

                        GOLDSTAR SERIES 5000 MOBILE

ACTION                            TO STORE            DISPLAY

PWR up Unit
Press FCN 4 to see the selected NAM. Press * to advance. Select NAM1.
Press FCN, 9, 9, *    "Enter Code" will be displayed.
Enter   1234567890

XXXXXXXXXX                        PRESS MEM           Enter MIN

_ _ _ _ _                         PRESS MEM           Enter System ID

0334                              PRESS MEM           Enter IPCH

07  (ACCOLC)                      PRESS MEM           Enter OVLD Class

1234                              PRESS MEM           LOCK CODE

123456                            PRESS MEM           SECURITY CODE

1234                              PRESS MEM           ALARM DISARM CODE

0                                 PRESS MEM           PREFFERED SYSTEM

0                                 PRESS MEM           STATION CLASS MARK

1                                 PRESS MEM           HANDS FREE MARK (ON)

1                                 PRESS MEM           LOCAL USE MARK (ON)

1                                 PRESS MEM           MIN MARK (ON)

0                                 PRESS MEM           HORN ALERT (OFF)

0                                 PRESS MEM           OPT. SPEAKER (OFF)

TO SAVE TO NAM NOW                PRESS MEM

TO REVIEW ENTRIES USE THE VOLUME UP OR DOWN KEYS




                      Programming Instructions for:

                           MITSUBISHI  555,560,600

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
TO PROGRAM THIS FUNCTION YOU MUST BE OUT OF THE PROGRAMMING MODE
ENTER FCN 6 AND THEN ENTER THE NEW 3 DIGIT UNLOCK CODE
PRESS CLR.

To program from keypad remove and discard Nam Pad
PWR up unit
Press and Hold STO key within 10 seconds of pwr up
Enter "5474432"
Release STO key

XXXXXXXXXX                        Press SEND          MIN

123                               Press SEND          SECURITY CODE

_ _ _ _ _                         Press SEND          SID

1                                 Press SEND          LU

1                                 Press SEND          MIN MARK

334                               Press SEND          IPCH1

07                                Press SEND          ACCOLC1

0                                 Press SEND          PS1

10                                Press SEND          GIM

1                                 Press SEND          EE

1                                 Press SEND          HANDS FREE

0                                 Press SEND          ROAM INHIBIT

0                                 Press SEND          A/B SELECT

00                                Press SEND          f3-f0 DUAL HEAD

00                                Press SEND          f7-f4 LD INH

TO EXIT PROGRAMMING MODE PRESS "END" AT ANY TIME

Installing the LOCK CODE

To program the customer's lock code, the phone must be out ot the
programming mode.
To program, enter FCN, 6,3-digit security code, the a 3-digit lock code.
Press CLR.




                     Programming Instructions for:
                        NEC M3700 SERIES MOBILE

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
UNLOCK CODES WILL BE CHANGED ONLY IN PROGRAMMING MODE
FOLLOW THE INSTRUCTIONS THAT FOLLOW

A NAM PROGRAMMER ADAPTOR (NECAM #41-2012) IS
REQUIRED

PWR UP

TO ENTER TEST MODE:

RCL, #,0,1.                                           WILL CYCLE TO SHADED

TO CLEAR MEMORY:

RCL # 3 9
select nam
RCL # 7 6 0 #   nam 1
RCL # 7 6 1 #   nam 2

TO ENTER PROGRAMMING MODE:

RCL #71


XXX XXX XXXX                      PRESS #             Telephone No. (MIN)

1234                              PRESS #             Lock Code

_ _ _ _ _                         PRESS #             Home Area (SYS I.D.)

10                                PRESS #             G-NO  (Group I.D.)

0334                              PRESS #             First Paging Channel

0      for wireline               PRESS #             System Select

07                                PRESS #             ACCOLC

1                                 PRESS #             ACCESS

1                                 PRESS #             Local Use


To exit PROGRAMMING MODE          PRESS CLR and hold  TEST MODE will show

to exit TEST MODE                 RCL #02

IF MEM WAS CLEARED VIA RCL #39, PHONE WILL AUTOMATICALLY ENTER FULL-LOCK
AFTER EXITING THE TEST MODE.
TO UNLOCK PRESS FCN # 1234.




                      Programming Instructions for:

                                 NOKIA LX-11

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
PRESS SEL,5  THEN ENTER 5 DIGIT SECURITY CODE
PRESS SEL TO RECEIVE DISPLAY OF CURRENT UNLOCK CODE
PRESS 5 NOW TO CLEAR ALL CALL TIMERS
ENTER THE NEW UNLOCK CODE
PRESS SEL TO ACCEPT

PWR up unit
Enter *3001#12345 Then - SEL 9 END
IdEnt IF InFO should appear on display

Pressing END will move you through the parameters
Pressing SND will toggle between choices available

_ _ _ _ _                         Press END           HO-Id  (SID)

1                                 Press END           ACCESS

1                                 Press END           LOCL OPt

XXXXXXXXXX                        Press END           Phonxx

08                                Press END           St CLASS

334                               Press END           PAging Ch

07                                Press END           O-LOAd CLASS

B                                 Press END           PrEF SyS

10                                Press END           grOUP Id

12345                             Press END           SECUrIty

-------- (Can't be changed)       Press END           1 dAtE

00/00/90  (INSTALLATION DATE)     Press END           2 dAtE


TO EXIT PROGRAMMING MODE AT ANY TIME PRESS "END" TO STORE LAST PARAMETER
THEN POWER DOWN
WHEN THE "END" KEY IS PRESSED FOLLOWING THE LAST PARAMETER, THE TEXT
Prog donE  WILL APPEAR ON DISPLAY




                      Programming Instructions for:

                                NOKIA M-10

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED BY THE SECURITY CODE PROGRAMMED AT THE
TIME OF PROGRAMMING



PWR up unit
Enter  *17*3001*1234*
HO-Id must appear on display
Press SEL to view current value
Display will be one step behind TO STORE instructions


_ _ _ _ _                         Press SEL           ACCESS  (SID)

1                                 Press SEL           LOCAL

1                                 Press SEL           PhonE n

XXXXXXXXXX                        Press SEL           CLASS

08                                Press SEL           PAGE ch

334                               Press SEL           O-LOAd

07                                Press SEL           GrouP

10                                Press SEL           SEC

1234                              Press SEL          AUTO EXIT PROGRAM MODE

TO EXIT PROGRAMMING MODE AT ANY TIME PRESS "END"

WHEN THE SEL KEY IS PRESSED FOLLOWING THE LAST PARAMETER VALUE, THE PHONE
WILL AUTOMATICALLY EXIT THE NAM PROGRAMMING MODE AND RETURN TO NORMAL
OPERATION




                        Programming Instructions for:

                        NOVATEL 8305 TRANSPORTABLE

CA08 SOFTWARE VERSION

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
IF EQUIPMENT IS PROVIDED WITH A MENU KEY THEN ENTER THE MENU PORTION OF
THE PHONE AND DISPLAY AND IF NECESSARY REPROGRAM THE UNLOCK CODE FROM
THERE.
IF PHONE DOES NOT HAVE A MENU KEY THEN THERE CAN BE NO PROGRAMMING OF THE
UNLOCK CODE... THE SECURITY CODE WILL BE ALL THAT IS PROVIDED

Lock Phone  by pressing FCN 1
Enter Programming Mode by pressing #259

Screen will display the software revision number
Press Volume Up

Screen will display Phone's E.S.N.
Press Volume Up

Screen will display INIT REP USE SND
Press SEND to erase any numbers stored in the phones memory
Press Volume Up

_ _ _ _ _                         Send Vol. Up        SIDH      system I.D.

XXX XXX XXXX                      Send Vol. Up        MIN       mobile I.D.

Must be changed when done         Send Vol. Up        LOCK CODE 1
programming - BY CUSTOMER
Must be changed when done         Send Vol. Up        LOCK CODE 2
programming - BY CUSTOMER
SET                               Vol. Up             Option EX extnd adrss
334 press send to change          Vol. Up             IPCH      initial pge
07                                Send Vol. Up        ACCOLC    overload
10                                Send Vol. Up        GIM       group i.d.
333                               Vol. Up             IDCCA     initl a
334                               Vol. Up             IDCCB     initl b
1                                 Vol. Up             REG TBL SIZE
Volume up through the four invalid System I.D. addresses
SET                               Vol. Up             OPTION LU local use
B   press send to change          Vol. Up             OPTION PS (prefered sys)
CLR                               Vol. Up             OPTION IRI  rm inhbt
CLR                               Vol. Up             OPTION SSD
SET                               Vol. Up             OPTION QRC  qck rcall
SET                               Vol. Up             OPTION QST  qck store
SET                               Vol. Up             OPTION WUT  wake tone
SET                               Vol. Up             OPTION EE   use dtmf
SET                               Vol. Up             OPTION FD   use dtmf
SET                               Vol. Up             OPTION MFD  ext dtmf
SET                               Vol. Up             OPTION 32D  dgt dial
CLR                               Vol. Up             OPTION MLH  timer
CLR                               Vol. Up             OPTION LHM  timer
CLR                               Vol. Up             OPTION CRU  timer dsp
CLR                               Vol. Up             OPTION NLM  timer
SET for on CLR for off            Vol. Up             OPTION HA   hrn alert
CLR                               Vol. Up             OPTION ONL  diagnostc
END to exit or VOLUME UP to review entries.




                     Programming Instructions for:

                             OKI  CDL400

ACTION                            TO STORE            DISPLAY

To Enter Programming mode:

Press IN SEQUENCE:
END  RCL  FUNC  CLR  SND

Screen shows Entr id

Enter 08693427

XXX XXX XXXX     PRESS #          PRESS *             PHon

_ _ _ _ _        PRESS #          PRESS *             S id no

0334             PRESS #          PRESS *             iPCH

07               PRESS #          PRESS *             ACC oLC

123              PRESS #          PRESS *             LoC Cod

10               PRESS #          PRESS *             G id

0000             PRESS #          PRESS *             Stn CLS

0111             PRESS #          PRESS *             HORN ALERT, HANDS
                                                      FREE, LOCAL USE,
                                                      MIN. MARK.

PRESS END AT THIS TIME TO EXIT PROGRAMMING MODE.

__________________________________________________________________________

TO REPROGRAM TELEPHON NUMBER AND SYSTEM I.D. # -

PRESS IN SEQUENCE THE FOLLOWING KEYSTROKES:

FUNC  90 *  123 (SECURITY CODE)

PHon WILL DISPLAY

ENTER NEW PHONE NUMBER

XXX XXX XXXX     PRESS #          PRESS *             PHon

_ _ _ _ _        PRESS #          PRESS *             S id no

PRESS END AT THIS TIME TO EXIT PROGRAMMING MODE.

___________________________________________________________________________

To Re-Initialize Nam Memory for Handset Programmable Models -
Func 99*
Enter Last 8 digits of S.N.
Press *




                   Programming Instructions for:

                         PANASONIC  EB362



Charged Battery and Nam Adaptor(Grey Cord w/25pin Connector)are needed.

ACTION                        TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED FOR IN THE PROGRAMMING SEQUENCE




*0000# to enter program mode

*1                            Press SND

50                            Press SND           NAM 1 MODE

_ _ _ _ _                     Press STO 01        SIDH

XXXXXXXXXX                    Press STO 02        OWNDL

1 2 3                         Press STO 03        LOCK

0 0 0 0 0 0 0 0 0 0 0 0 (12)  Press STO 04        SPDL

00                            Press STO 05        SCM

334                           Press STO 06        IPCH

07                            Press STO 07        ACCOLC

10                            Press STO 08        GIM

1 1 0 1 1 1 0 0               Press STO 09        FEATURE A

0 0 0 0 0 1 0 0               Press STO 10        FEATURE B

1 0 0 0 0 0 1 1               Press STO 11        FEATURE C

00                            Press STO 12        DLMT

STO **
Turn power off




                      Programming Instructions for:

                        PANASONIC EB-500 OR TP-500

ACTION                            TO STORE            DISPLAY

USED EQUIPMENT: TO DISPLAY CURRENT UNLOCK CODE -
THIS FUNCTION IS PROVIDED FOR IN THE PROGRAMMING SEQUENCE

Attach Nam Programmer Cable (Our Stock # 823)

Pwr up unit

Enter *0000#                                          0

*1  SND
You are now in the NAM 1 Program mode.

_ _ _ _ _                         Press STO 01        S.I.D.

XXXXXXXXXX                        Press STO 02        OWN #

0                                 Press STO 03        O for W/L system

334                               Press STO 04        IPCH

07                                Press STO 05        ACCOLC

10                                Press STO 06        GIM

00                                Press STO 07        Digit Dial Limit

08                                Press STO 08        SCM (3watt i.d.)

911                               Press STO 09        Rcl 00

1234                              Press STO 10        Security Code

11000000                          Press STO 11        FUNCTION BYTE 1

00010010                          Press STO 12        FUNCTION BYTE 2

10010111                          Press STO 13        FUNCTION BYTE 3

TO BURN NAM AT THIS TIME          Press STO **        NAM is burned

Turn off unit
Detach programming cable




                       Programming Instructions for:

                     RADIO SHACK 17-1002 TRANSPORTABLE

THIS UNIT REQUIRES A SERVICE HANDSET TO BE PROGRAMMED!!!

A Mobira Service Handset (Modified) may be used.  It is made from an ME53
or ME57 handset by opening and adding a jumper to the left of the one
factory installed just below the white 24 pin connector joining the top and
bottom PCB's. Also, pins 1 and 14 of the handset connector must be jumpered
at the radio end.  To disassemble the handset, carefully pry off the
plastic earpad retaining housing to expose on hexdrive screw.  Two other
screws are under the rubber plugs at either side of the microphone.  The
handset then splits apart.  This is a ticklish job and isn't recommended
except in an extreme case and not with the customer's handset.  The 
modification does not affect normal operation of the handset.  It is not 
known if a Radio handset will work the same.

After the Service Handset has been applied:

        To enter LOCAL MODE (which takes the phone off the air and allows
service commands to be obeyed) press 01#.  The display should clear and noise
is heard from the earpiece.

        To enter the NAM programming mode, enter 48#.  The display shows 48
briefly and clears.

ACTION              KEYBOARD ENTRY            DISPLAY

0                         *                 (5-digit SID)
1                         *
1                         *
XXXXXXXXXX                *
10                        *
334                       *
07                        *
0                         *
10                        *
12345                     *

        Press * to exit NAM programming mode and return to Local Mode.
To enter the NAM reading mode, press 49#.  The display will show  49.


*****************************************************************************
