Subject: Motorola Users Guide 
NNTP-Posting-Host: dispatch.demon.co.uk 
X-Newsreader: Demon Internet Simple News v1.29 
X-Posting-Host: illumini.demon.co.uk 
 
 
Here it is, enjoy ppl.... 
 
-=*( Prophet )*=- 
 
 
*****************************************************************************                  
*                                                                           * 
*                MOTOROLA USERS AND PROGRAMMING GUIDES                      * 
*                           By Mike Larsen                                  * 
*                                                     Ver. 1.1a             * 
*                                                                  03/26/95 * 
***************************************************************************** 
 
        Following the programming text are additional files from several 
people on hacking the FOVC, the trik clip, and cable specs for all Motorola  
phones.  If you have any corrections or additional information to be added to  
this text, please E-mail me at: 
 
        Mike.Larsen@uti.com 
        Stularsenmic@vax.colsf.edu 
 
        ****** READ THIS ******   I will be going to my Motorola Technical  
school in a month or so for certification.  So if anybody has any questions 
they'd like me to ask the "experts", drop me a line.  They say they will  
answer any valid questions...oh, goody!  I assume asking about the guy's sex 
life or why they make it so hard to get in the fone is PROBABLY the types of 
questions they are trying to avoid.  If it's perverted, don't reply...I take 
it back.  If the guy is a loser, I'll ask him anyway.  If the question is a  
hack question, try to phrase it in a way that it could be for LEGITIMATE  
reasons.  They are kinda funny about ESN hacking questions...go figure. 
 
        Added Note:  Motorola is trying like hell to get their blue books  
back.  If you have one, don't mention to any cellular providers you have one. 
They are taking names and other personal info and who knows what they are 
doing with it. 
 
----------------------------------------------------------------------------- 
 
        Before going in to the programming of the cellular phone, it is 
important for the user to know the normal things necessary for day to day 
operation.  While the majority of the stuff in the users manual is intended 
for people that have problems programming their VCR, their are a few things 
that are very important and are only mentioned in the users manual. 
 
                          Turn On: [Pwr] 
                           Unlock: Three digit unlock code.  If you make an  
                                   error, [Clr] and enter again. 
                       Place Call: Enter number, [Snd] 
                     Receive Call: [Snd] or open flip fone 
                         End Call: [End] or close flip fone 
                     Store Number: Phone number, [Sto], 2-digit location number 
                    Recall Number: [Rcl], 2-digit location number 
              Super Speed Dialing: Directory location number, [Snd] 
                 Changing Entries: Press [Rcl] and the 2-digit location number  
                                   so that the number to be changed is  
                                   displayed.  Press and release [Clr] to back  
                                   out each of the digits. Enter a new number  
                                   and press [Sto]. 
            Call Number Displayed: [Snd] 
                Microphone Muting: Press [Fcn], [6].   
                                   To unmute, press [Fcn], [6] 
                        Lock Unit: [Fcn], [5] or [LOCK] 
              Display Unlock Code: Press [Fcn], [0], your six-digit security 
                                   code, [Rcl]. 
        Changing Your Unlock Code: Press [Fcn], [0], your six-digit security 
                                   code, your NEW 3-digit unlock code, [Sto]. 
             Review Battery Meter: Press [Fcn], [4] and release. 
                    Adjust Volume: Earpiece - Press and hold [Vol] to increase. 
                                              Release, press again to decrease. 
                                     Ringer - [Fcn], then Vol as above. 
          Recall Last Number Used: [Rcl], [0], [0] 
          Recall Own Phone Number: [Rcl], [#] 
            Individual Call Timer: [Rcl], [#], [#] 
            Resettable Call Timer: [Rcl], [#], [#], [#] 
      Reset Resettable Call Timer: [Fcn], [0], [7], [Clr] 
            Cumulative Call Timer: [Rcl], [#], [#], [#], [#] 
                  Access Features: Press [Fcn], [1].  To change features, press 
                                   [*] and [#] to scroll and [Clr] to change. 
                                   To exit feature menu, press [END]. 
      Review/Scroll Menu Features: Press [*] or [#] 
                    Status Review: [Fcn], [0], [9], [Rcl], [#] or [*] scrolls  
                                   messages.  To end press [END]. 
             Changing System Type: Press [Rcl], [*].  Repeatedly press [*]  
                                   until the desired system type appears.  To 
                                   select press [Sto]. 
       Outgoing Call Restrictions: Press [Fcn], [0], 6-digit security code,  
                                   [1], [Sto].  Phone will place calls only 
                                   from memory locations 1-10. 
                                   To change back to unrestricted dialing 
                                   press [Fcn], [0], 6-digit security code, 
                                   [4], [Sto]. 
 
        I would like to add that while I have extensively worked on finding 
additional test mode commands, I (and anyone else) have never worked with the 
normal operation commands as listed above.  For example, above you will   
notice sequences with [Fcn], [1] or [Fcn], [0], [7].  This is totally 
unexplored teritory.  Happy hacking :)  
 
------------------------------------------------------------------------------ 
 
NOTES:  Some units have dual NAM's. 
        The ESN prefix is 130 decimal, 82 hex. 
        Motorola: 1-800-331-6456 
 
There are MANY different models of Motorola phones sold under various 
brand names, if you think it's a Motorola, it probably is. 
 
Determine which access sequence to use: 
 
HAND HELD PORTABLE MODELS 
 
If the phone has a FCN button and no MENU button use sequence 1. 
If the phone has no FCN button use sequence 2. 
If the phone has a MENU button and a FCN button use sequence 4. 
 
INSTALLED MOBILE PHONES AND TRANSPORTABLE MODELS 
 
If the phone has no FCN button and no RCL button use sequence 3. 
If the phone has a FCN button use sequence 4. 
If the phone has a MEM button use sequence 5. 
If the phone has a RCL button and no FCN button use sequence 6. 
 
 
SEQUENCE#     ACCESS CODE 
 
1             FCN   (SECURITY CODE TWICE) RCL 
2             STO # (SECURITY CODE TWICE) RCL 
3             CTL 0 (SECURITY CODE TWICE) * 
4             FCN 0 (SECURITY CODE TWICE) RCL 
5             FCN 0 (SECURITY CODE TWICE) MEM 
6             CTL 0 (SECURITY CODE TWICE) RCL 
 
The default security code is 000000.  The CTL (control) button is the 
single black button on the side of the handset. 
 
 
NAM programing: 
 
1.  Turn the power on. 
 
2.  Within ten seconds enter the access sequence as determined above. 
 
3.  The phone should now show "01" in the left of the display, this is the 
    first programing entry step number.  If it does not the security code 
    is incorrect, or the programing lock-out counter has been exceeded.  In 
    either case you can still program the unit by following the steps under 
    TEST MODE PROGRAMING below. 
 
4.  The * key is used to increment each step: 
 
    Each time you press * the display will increment from the step number, 
    displayed on the left, to the data stored in that step, displayed on 
    the right.  When the data is displayed make any necessary changes and 
    press * to increment to the next step number. 
 
5.  The SND key is used to complete and exit programing when any STEP 
    NUMBER is displayed. 
 
    If you have enabled the second phone number bit in step 10 below then 
    pressing SND will switch to NAM 2.  Steps 01 thru 06, 09 and 10 will 
    repeat for NAM 2, the step number will be followed by a "2" to indicate 
    NAM two. 
 
5.  The CLR key will revert the display to the previously stored data. 
 
6.  The # key will abort programing at any time. 
 
 
PROGRAMING DATA: 
 
STEP#    #OF DIGITS/RANGE    DESCRIPTION 
 
01       00000 - 32767       SYSTEM ID 
02       3 DIGITS            AREA CODE 
03       7 DIGITS            TEL NUMBER 
04       2 DIGITS            STATION CLASS MARK 
05       2 DIGITS            ACCESS OVERLOAD CLASS 
06       2 DIGITS            GROUP ID (10 IN USA) 
07       6 DIGITS            SECURITY CODE 
08       3 DIGITS            LOCK CODE 
09       0333 OR 0334        INITIAL PAGING CHANNEL 
10       6 DIGIT BINARY      OPTION PROGRAMING (SEE NOTE 1) 
11       3 DIGIT BINARY      OPTION PROGRAMING (SEE NOTE 2) 
 
 
NOTES: 
 
Take care with Motorola's use of "0" and "1".  Some options use "0" to 
enable, some use "1". 
 
1.  This is a 6 digit binary field used to select the following options: 
 
    Digit 1:  Internal handset speaker, 0 to enable. 
    Digit 2:  Local Use Mark, 0 or 1. 
    Digit 3:  MIN Mark, 0 or 1. 
    Digit 4:  Auto Recall, always set to 1 (enabled). 
    Digit 5:  Second phone number (not all phones), 1 to enable. 
    Digit 6:  Diversity (Two antennas, not all phones), 1 to enable. 
 
2.  This is a 3 digit binary field used to select the following options: 
 
    Digit 1:  Continuous DTMF, 1 to enable. 
    Digit 2:  Transportable Ringer/Speaker, 0=Transducer, 1=Handset. 
    Digit 3:  8 hour time out in transportable mode, 0 to enable. 
 
 
On newer models, they have added and changed some numbers.  The numbers 
as of the 3/27/92 manual are as follows: 
 
1.  The 6 digit binary field is still the same.   
 
2.  The 3 digit binary field has become a 5 digit binary field. 
     
    Digit 1:  Failed Page Indicator                        1=Disabled;0=Enabled 
    Digit 2:  Motorola Enhanced Scan                       1=Enabled; 0=Disabled 
    Digit 3:  Long Tone DTMF                               1=Enabled; 0=Disabled 
    Digit 4:  Transportable Internal Ringer Speaker        1=Handset; 0=Transdcr 
    Digit 5:  Eight Hour Timeout                           1=Disabled;0=Enabled 
 
 
 
                              TEST MODE ACCESS: 
 
 
 
INSTALLED MOBILE PHONES AND TRANSPORTABLE MODELS 
 
To enter test mode on units with software version 85 and higher you must 
short pins 20 and 21 of the transceiver data connector.  An RS232 break out 
box is useful for this, or construct a test mode adaptor from standard 
Radio Shack parts. 
 
For MINI TR or Silver Mini Tac transceivers (smaller data connector) you 
can either short pins 9 and 14 or simply use a paper clip to short the 
hands free microphone connector. 
 
HAND HELD PORTABLE MODELS: 
 
There are two basic types of Motorola portable phones, the Micro-Tac series 
"Flip" phones, and the larger 8000 and Ultra Classic phones.  Certain newer 
Motorola and Pioneer badged Micro-Tac phones do not have a "flip", but 
follow the same procedure as the Micro-Tac. 
 
8000 & ULTRA CLASSIC SERIES: 
 
If you have an 8000 series phone determine the "type" before trying to 
enter test mode.  On the back of the phone, or on the bottom in certain 
older models, locate the F09... number this is the series number.  If the 
FOURTH digit of this number is a "D" you CAN NOT program the unit through 
test mode, a Motorola RTL4154/RTL4153 programer is required to make any 
changes to this unit. 
 
Having determined that you do not have a "D" series phone the following 
procedure is used to access test mode: 
 
Remove the battery from the phone and locate the 12 contacts at the top 
near the antenna connector.  These contacts are numbered 1 through 12 from 
top left through bottom right.  Pin 6, top right, is the Manual Test Mode 
Pin. You must ground this pin while powering up the phone.  Pin 7 (lower 
left) or the antenna connector should be used for ground.  Follow one of 
these procedures to gain access to pin 6: 
 
1.  The top section of the battery that covers the contacts contains 
nothing but air.  By careful measuring you can drill a small hole in the 
battery to gain access to pin 6, alternately simply cut the top off the 
battery with a hack saw.  Having gained access use a paper clip to short 
pin six to the antenna connector ground while powering up the phone. 
 
2.  If you do not want to "destroy" a battery you can apply an external 7.5 
volts to the + and - connectors at the bottom of the phone, ground pin 6 
while powering up the phone as above. 
 
3.  You can also try soldering or jamming a small jumper between pins 6 and 
7 (top right to lower left), or between pin 6 and the antenna connector 
housing ground.  Carefully replace the battery and power up the phone.  Use 
caution with this method not to short out any other pin. 
 
4.  A cigarette lighter adaptor, if you have one, also makes a great test 
mode adaptor as it can be disassembled to give you easier access to pin 6. 
Many are pre marked, or even have holes in the right location.  This is 
because they are often stamped from the same mold that the manufacturer 
uses for making hands free adaptor kits and these kits require access to 
the phone's connectors. 
 
 
MICRO-TAC "FLIP" SERIES: 
 
This phone follows similar methods as outlined for the 8000 series above. 
 
Remove the battery and locate the three contacts at the bottom of the 
phone, the two outer contacts are raised and connect with the battery.  The 
center contact is recessed, this is the Manual Test Mode connector. 
 
Now look at the battery contacts, the two outer ones supply power to the 
phone, the center contact is an "extra" ground.  This ground needs to be 
shorted to the test mode connector on the phone.  The easiest way to do 
this is to put a small piece of solder wick, wire, aluminum foil or any 
other conductive material into the recess on the phone.  Having done this 
carefully replace the battery and turn on the power, if you have been 
successful the phone will wake up in test mode. 
 
GENERAL NOTES: 
 
HANDSETS:  Most Motorola handsets are interchangeable, when a handset is 
used with a transceiver other than the one it was designed for the display 
will show "LOANER".  Some features and buttons may not work, for instance 
if the original handset did not have a RCL or STO button, and the 
replacement does, you will have to use the control * or control # sequence 
to access memory and A/B system select procedures. 
 
 
 
LOCK/UNLOCK PROCEDURES: 
 
     Phones with "LOCK" buttons:  Press lock for at least 1/2 a second. 
 
     Phones with a "FCN" button:  Press FCN 5, note that 5 has the letter's 
                                  "J,K, and L" for lock. 
 
     Phones with no FCN or LOCK button:  Press Control 5, control is the black 
                                         volume button on the side of the 
                                         handset. 
 
 
SYSTEM SELECT PROCEDURES: 
 
     Phones with a RCL button:  Press RCL *, then * to select, STO to store. 
 
     Phones with no RCL button: Press Control * then * to select, # to store. 
 
     Options are:    CSCAn:    Preferred/Non preferred with system lockout. 
                     Std A/b, or Std b/A:  Preferred/Non preferred. 
                     SCAn Ab, or SCAn bA:  Non preferred/Preferred 
                     SCAn A:  "A" ONLY 
                     SCAn b:  "B" ONLY 
                     HOME:     Home only 
 
     (these are typical options, some phone's vary.  C-Scan is only available  
     on newer models and does not appear unless programed, see below.) 
 
 
 
 
                                 TEST MODE 
     
     
    Taken from the July 1993 Cellular Subscriber Technical Training Manual 
    Item# 68P09300A60-C and the Curtis Namfax vol.4.  I believe this is a 
    complete listing of all the commands that were ever possible.  This  
    includes old phones and the new ones.  If there are two entries for a 
    particular number, the first one is the current command and the second 
    is for older models. 
 
NOTE: Not all commands work on all telephones.  If a command is not valid the 
      display will show "ErrOr."  Not all numbers have been assigned.  Not all 
      numbers have been listed here.  Some commands were intended only for 
      Motorola factory applications.   (This is the disclaimer in the 
      technical training manual.  I have included all of the other commands I  
      have discovered one way or another.  I do believe this is a complete list 
      of the commands.) 
     
 
Three test commands are significant for programming and registering the 
the telephone for service:  see full descriptions under TEST MODE COMMANDS. 
 
32#  Clears the telephone.  (Older Motorola allowed either three or fifteen  
changes in the MIN.  After that, the phone had to be sent to Motorola to reset  
the counter.  This is the command they use.)  
 
38#  Displays the ESN 
 
55#  This is the TEST MODE PROGRAMMING (as described below). 
 
 
                          TEST MODE COMMANDS: 
 
 
#    Enter Test Command Mode 
 
00#  no function 
 
01#  Restart (Re-enter DC power start-up routine.)  On TDMA telephones, this 
     command has the same effect as pressing the PWR button. 
 
02#  Display Current Telephone Status (This is a non-altering version of the 
     STATUS DISPLAY.  On a 14 character display, all the information is shown. 
     On a 7 character display only the information on the second line of a 14 
     character display is shown.  On a 10 character display, all the  
     information on the second line of a 14 charcter display plus the last  
     three characters of the first line are shown.) 
 
     STATUS DISPLAY, ALTERNATES BETWEEN: 
      
     AAA BBB   AAA = Channel Number (decimal)    BBB = RSSI reading for channel 
     CDEFGHI   are as follows: 
 
     C = SAT frequency (0=5970, 1=6000, 2=6030, 3=no channel lock) 
     D = Carrier (0=off, 1=on) 
     E = Signalling tone (0=off, 1=on) 
     F = Power attenuation level (0 through 7) 
     G = Channel mode (0=voice channel, 1=control channel) 
     H = Receive audio mute (0=unmuted, 1=muted) 
     I = Transmit audio mute (0=unmuted, 1=muted) 
 
     Press * to hold display and # to end. 
 
03#  Reset Autonomous Timer.   This command results in the reset of the  
     autonomous timer but does not provide any test function on these models. 
 
04#  Initializes Telephone to Standard Default Conditions: 
     Carrier Off, Power Level 0, Receiver Audio Muted, Transmit Audio Muted, 
     Signalling Tone Off, SAT Off, Resetting of Watch-Dog Timer Enabled,  
     DTMF and Audio Tones Off, Audio Path Set to Speaker 
 
05#  TX Carrier On (Key Transmitter) 
 
06#  TX Carrier Off 
 
07#  RX Audio Off (Mute Receiver Audio) 
 
08#  RX Audio On (Unmute Receiver Audio) 
 
09#  TX Audio Off 
 
10#  TX Audio On 
 
11(Ch.No.)# Set Tranceiver to Channel xxxx (Receive and Transmit in Decimal; 
            accepts 1, 2, 3, or 4 digits) 
 
            see end of file for more info on this command 
 
12x# Set Power Step to x; (0,1-7) 0=Maximum Power (3 Watts) 7=Minimum Power Out 
 
13#  Power Off (Shuts off the radio) 
 
14#  10 kHz Signalling Tone On 
 
15#  10 kHz Signalling Tone Off 
 
16#  Setup  (Transmits a five word RECC message; each of the five words will  
     be "FF00AA55CC33."  Transmitter de-keys at the end of the message.) 
 
17#  Voice  (Transmits a two word REVC message; each of the two words will be 
     "FF00AA55CC33."  Transmitter de-keys at the end of the message.) 
 
18#  C-Scan  (Allows for entry of as many as 5 negative SID's for each NAM.) 
 
     Newer Motorola phones are equipped with a feature called C-Scan, this is  
     an option along with the standard A/B system selections.  C-Scan allows  
     the phone to be programed with up to five inhibited system ID's per NAM.   
     This is designed to prevent the phone from roaming onto specified non-home 
     systems and therefore reduce "accidental" roaming fees. 
 
     1.  C-Scan can only be programed from test mode, power phone up with the 
         relevant test mode contact grounded (see above). 
 
     2.  Press # to access test mode. 
 
     3.  Press 18#, the phone will display "0    40000". 
 
     4.  Enter the first inhibited system ID and press *. 
 
     Continue to enter additional system ID's if required.  After the 5th entry 
     the phone will display "N2". Press * to continue and add system ID's for 
     NAM 2 as required. 
 
     5.  If an incorrect entry is made (outside the range of 00000-32767) the 
         display will not advance, press CLR and re-enter.  Use a setting of 
         40000 for any un-needed locations. 
 
     6.  When the last entry has been made press * to store and press # to exit, 
         turn off power. 
 
     or 
      
     [**Phones without the C-Scan option used this command to SEND NAM.**] 
 
18#  SEND NAM.  Display shows AA BB.  Where AA=Address and BB=Data.  Displays    
     the contents of the NAM, one address at a time, advanced by pressing the 
     * key.  The following data is contained in NAM.  The test is exited by 
     depressing the # key. 
     SIDH                 Sec. Code 
     OPT. (1,2,&3)        MIN 
     MIN1, MIN2           FCHNA 
     SCM                  FCHNB 
     IPCH                 NDED 
     ACCOLC               CHKSUM       GIM 
 
19#  Display Software Version Number  (4 digits displayed as year and week) 
 
NOTE:  Entering commands 20# through 23# or 27# causes the tranceiver to begin 
       a counting sequence or continous transmission as described below.  In 
       order to exit from the commands to enter another test command, the #  
       key must be depressed; all other key depressions are ignored. 
 
20#  Receive control channel messages counting correctable and uncorrectable 
     errors.  When the command starts, the number of the command will be  
     displayed in the upper-right corner of the display.  Entering a # key 
     will terminate the command and display two three-digit numbers in the  
     display.  The first number is the number of correctable errors and the 
     second is the uncorrectable errors. 
 
21#  Received voice channel messages counting correctable and uncorrectable 
     errors.  When the command starts, the number of the command will be  
     displayed in the upper right-hand corner of the display.  Entering a #  
     key terminates the command and will display two three-digit numbers in  
     display.  The first is the number of correctable errors and the second  
     is the uncorrectable errors. 
 
22#  Receive control channel messages counting word sync sequence.  When the 
     command starts, the number of the command will be displayed in the upper 
     right-hand corner of the display.  Entering a # key will terminate the 
     command and display the number of word sync sequences in the display. 
 
23#  Receive voice channel messages counting word sync sequences.  When the 
     command starts, the number of the command will be displayed in the upper 
     right-hand corner of the display.  Entering a # key will terminate the  
     command and display the number of word sync sequences in the display. 
 
24#  Receive control channel data and display the majority voted busy/idle 
     bit.  0=idle  1=busy 
 
25x# SAT On         When                        x=0, SAT=5970HZ 
                                                x=1, SAT=6000HZ 
                                                x=2, SAT=6030HZ 
 
26#  SAT Off 
 
27#  Transmit Data  (Transmits continuous control channel data.  All words  
     will be "FF00AA55CC33."  When the command starts, '27' will be displayed 
     in the right side of the display.  Entering a # key will terminate the 
     command.  The transmitter de-keys when finished.) 
 
28#  Activate the high tone (1150 Hz +/- 55 Hz) 
 
29#  De-activate the high tone 
 
30#  Activate the low tone (770 Hz +/- 40 Hz) 
 
31#  De-activate the low tone 
 
32#  Clear (Sets non-volatile memory to zeroes or factory default.  This  
     command will affect all counters, all repertory memory including the last 
     number called stack, and all user programmable features including the 
     setting of System Registration.  It does not affect the ESN, NAM, phasing 
     data, or lock code.  This takes a minute or so.  DO NOT TURN OFF THE  
     TELEPHONE WHILE THIS IS SHOWING '32' ON THE DISPLAY.  WAIT UNTIL THE  
     NORMAL SERVICE LEVEL DISPLAY RESUMES!) 
 
33x# Turn on DTMF for x  (1-9, *, 0, #, plus the single tones)      
        Where x=1    697 Hz + 1209 Hz       10  697 Hz 
                2    697 Hz + 1336 Hz       11  770 Hz 
                3    697 Hz + 1477 Hz       12  852 Hz 
                4    770 Hz + 1209 Hz       13  941 Hz 
                5    770 Hz + 1336 Hz       14  1150 Hz (not used in cellular) 
                6    770 Hz + 1477 Hz       15  1209 Hz  
                7    852 Hz + 1209 Hz       16  1336 Hz 
                8    852 Hz + 1336 Hz       17  1477 Hz 
                9    852 Hz + 1477 Hz       18  1633 Hz (not used in cellular) 
                *    941 Hz + 1209 Hz 
                0    941 Hz + 1336 Hz 
                #    941 Hz + 1477 Hz 
 
34#  Turn DTMF Off 
 
35#  Display RSSI ("D" Series Portable Only) 
 
     or 
 
35x# Set Audio Path to x    x=0, V.S.P Microphone (Applies to mobiles only.) 
                            x=1, Speaker 
                            x=2, Alert 
                            x=3, Handset 
                            x=4, Mute 
                            x=5, External Telephone (Applies to Portables Only) 
                            x=6, External Handset (Applies to NEWER Portables) 
 
36nnn# Scan (TDMA Telephones only.  Scans the primary control channels and  
     attempts to decipher the forward data stream.  The display will show PASS1 
     if the strongest control channel was accessed, PASS2 if the second  
     strongest was accessed, and FAIL if no control channel could be accessed.) 
 
     (nnn=Scan speed in milliseconds).  Tunes from channel 1 to 666 in order. 
     Entering a * pauses the scan and displays current Channel Number and 
     RSSI reading (AAA=Channel Number and BBB=RSSI Reading).  When scan speed 
     is 300 milliseconds or greater, the current status is displayed during the 
     scan; when less than 300 milliseconds the status is displayed only during 
     pause.  Entering * during a pause causes the scan to resume.  Entering # 
     aborts the scan and leaves the mobile tuned to the current channel.  During 
     this command only the * and # keys are recognized. 
 
37#  Sets Low Battery Threshold.  Usage: #37#x# where x is any number    
     from 1 to 255.  If set to 1, the Low Battery indicator will come up 
     when the phone is powered on.  If set to 255, it may never come up. 
 
38#  Display ESN (Displays ESN in four steps, two hexadecimal digits at a time 
     in a for digit display.  The decimal shows the address, 00 through 03 as 
     the first two digits, and two digits of the ESN as the last two digits. 
     Use the 'G' to step through the entire hexadecimal ESN.) 
 
     Compander OFF ("D" Series Portables) 
 
     or 
 
38#  SND-SNM.  Display shows AA BB.  Where AA=Address;BB=Data.  Send the SNM 
     to the display.  All 32 bytes of the SNM will be displayed, one byte at  
     a time.  The byte address will be displayed in the upper right-hand 
     corner and the contents of that address will be displayed in the hex.   
     The * key is used to step through the address similar to the SEND-NAM 
     (18#) command. 
 
39#  Compander ON ("D" Series Portables) 
 
     or 
 
39#  RCVSU.  Receive one control channel word.  When the word is received it 
     is displayed in hex.  This command will be complete when a control channel  
     word is received or when the # key is entered to abort the command. 
 
40#  RCVVC.  Receive one voice channel word.  When the word is received it is 
     displayed in hex.  This command will be complete when a voice channel 
     word is received or when the # key is entered to abort the command. 
 
41#  Enables Diversity (On F19CTA... Series only.) 
 
42#  Disables Diversity (On F19CTA... Series only.) 
 
43#  Disable Diversity 
     USE T/R ANTENNA (On F19CTA... Series only.)   
     USE R ANTENNA (On D.M.T./ Mini TAC) 
 
44#  Disable Diversity 
     USE R ANTENNA (On F19CTA... Series only.)   
     USE T/R ANTENNA (On D.M.T./ Mini TAC)  
 
45#  Display Current RSSI (Displayed as a three-digit decimal number)    
 
46#  Display Cumulative Call Timer 
 
47x# Set RX Audio level to X 
     (For F19CTA ...Series Tranceivers)  
                                       X=0, Lowest Volume 
                                       X=6, Highest Volume 
                                       X=7, mute 
                                       Normal setting is 4. 
     (For D.M.T./ Mini TAC Tranceivers) 
                                       X=0, Lowest Volume 
                                       X=7, Highest Volume 
                                       Normal setting is 4. 
     (For TDMA Tranceivers and F09F... Series and Higher Portables) 
                                       X=0, Lowest Volume 
                                       X=15, Highest Volume 
                                       Normal setting is 2 to 4.  (On TDMA 
                                       Tranceivers and Micro TAC portables,  
                                       settings 8 through 15 are for DTMF 
                                       applications only.) 
 
48#  Side Tone On.  Use this command in conjunction with 350# to test the  
     entire audio path in hands-free applications. 
 
49#  Side Tone Off 
 
50#  Maintenance data is transmitted and test results displayed: 
     PASS=received data is correct 
     FAIL 1=2second timeout, no data rec. 
     FAIL 2=received data is incorrect 
 
51#  Test of mobile where maintenance data is transmitted and looped back.   
     Display is as follows: 
     PASS=looped-back data is correct 
     FAIL 1=2 second timeout, no looped-back data 
     FAIL 2=looped-back data is incorrect 
 
52x# SAT Phase Adjustment.  A decimal value that corresponds to phase shift 
     compensation in 4.5 degree increments.  Compensation added to inherent 
     phase shift in tranceiver to achieve a total of 0 degrees phase shift. 
 
     Do NOT enter any values except those shown below. 
 
     0 degrees = 0          121.5 degrees = 59           243.0 degrees = 86 
     4.5       = 1          126.0         = 60           247.5         = 87 
     9.0       = 2          130.5         = 61           252.0         = 112 
     13.5      = 3          135.0         = 62           256.5         = 113 
     18.0      = 4          139.5         = 63           261.0         = 114 
     22.5      = 5          144.0         = 40           265.5         = 115 
     27.0      = 6          148.5         = 41           270.0         = 116 
     31.5      = 7          153.0         = 42           274.5         = 117 
     36.0      = 16         157.5         = 43           279.0         = 118 
     40.5      = 17         162.0         = 44           283.5         = 119 
     45.0      = 18         166.5         = 45           288.0         = 120 
     49.5      = 19         171.0         = 46           292.5         = 121 
     54.0      = 20         175.5         = 47           297.0         = 122 
     58.5      = 21         180.0         = 64           301.5         = 123 
     63.0      = 22         184.5         = 65           306.0         = 124 
     67.5      = 23         189.0         = 66           310.5         = 125 
     72.0      = 48         193.5         = 67           315.0         = 126 
     76.5      = 49         198.0         = 68           319.5         = 127 
     81.0      = 50         202.5         = 69           324.0         = 104 
     85.5      = 51         207.0         = 70           328.5         = 105 
     90.0      = 52         211.5         = 71           333.0         = 106 
     94.5      = 53         216.0         = 80           337.5         = 107 
     99.0      = 54         220.5         = 81           342.0         = 108 
     103.5     = 55         225.0         = 82           346.5         = 109 
     108.0     = 56         229.5         = 83           351.0         = 110 
     112.5     = 57         234.0         = 84           355.5         = 111 
     117.0     = 58         238.5         = 85           360.0         = 70 
               
53#  Enable scrambler option, when equipped. 
 
54#  Disable scrambler option, when equipped. 
 
55#  Display/Program N.A.M. (Test Mode Programming) 
 
     TEST MODE PROGRAMING: 
 
     Assuming you have completed one of the above steps correctly the phone 
     will wake up in test mode when you turn the power on.  When you first 
     access test mode the phone's display will alternate between various status 
     information that includes the received signal strength and channel number. 
     The phone will operate normally in this mode.  You can now access Service 
     Mode by pressing the # key, the display will clear and a ' will appear. 
     Use the following procedure to program the phone: 
 
     1.  Enter 55# to access programing mode. 
 
     2.  The * key advances to the next step.  (NOTE that test mode programing 
         does NOT have step numbers, each time you press the * key the phone  
         will display the next data entry). 
 
     3.  The CLR key will revert the display to the previously stored data. 
 
     4.  The # key aborts programing at any time. 
 
     5.  To complete programing you must scroll through ALL entries until a ' 
         appears in the display. 
 
     6.  Note that some entries contain more digits than can be displayed by the 
         phone, in this case only the last part of the data can be seen. 
 
     TEST MODE PROGRAMING DATA: 
 
     STEP#    #OF DIGITS/RANGE    DESCRIPTION 
 
     01       00000 - 32767       SYSTEM ID 
     02       8 DIGIT BINARY      OPTION PROGRAMING, SEE NOTE 1 BELOW 
     03       10 DIGITS           MIN (AREA CODE & TEL#) 
     04       2 DIGITS            STATION CLASS MARK 
     05       2 DIGITS            ACCESS OVERLOAD CLASS 
     06       2 DIGITS            GROUP ID (10 IN USA) 
     07       6 DIGITS            SECURITY CODE 
     08       3 DIGITS            LOCK CODE 
     09       3 DIGITS            SERVICE LEVEL (LEAVE AT 004) 
     10       8 DIGIT BINARY      OPTION PROGRAMING, SEE NOTE 2 BELOW 
     11       8 DIGIT BINARY      OPTION PROGRAMING, SEE NOTE 3 BELOW 
     12       0333 OR 0334        INITIAL PAGING CHANNEL 
     13       0333                "A" SYSTEM IPCH 
     14       0334                "B" SYSTEM IPCH 
     15       3 DIGIT             NUMBER PAGING CHANNEL (021 IN USA) 
     16       8 DIGIT BINARY      OPTION PROGRAMING, SEE NOTE 4 BELOW 
 
     Steps 01 through 06 and 12 will repeat for NAM 2 if the second phone  
     number bit has been enabled in step 11. 
 
     NOTES: 
 
     Take care with Motorola's use of "0" and "1".  Some options use "0" to 
     enable, some use "1". 
 
     These are eight digit binary fields used to select the following options: 
 
     1.  (step 02 above, suggested entry is: 11101001 for "A" system, 10101001 
         for "B" sys) 
 
         Digit 1: Local use mark, 0 or 1. 
         Digit 2: Preferred system, 0 or 1. 
         Digit 3: End to end (DTMF) dialing, 1 to enable. 
         Digit 4: Not used, enter 0. 
         Digit 5: Repertory (speed) dialing, 1 to enable. 
         Digit 6: Auxiliary (horn) alert, 1 to enable. 
         Digit 7: Hands free (VSP) auto mute, 1 to enable (mutes outgoing hands 
                  free audio until the MUTE key is pressed). 
         Digit 8: Min mark, 0 or 1. 
 
     2.  (step 10 above, suggested entry is: 00000100) 
 
         Digits 1 - 4: Not used in USA, enter 0. 
         Digit 5: Single system scan, 1 to enable (scan A or B system only, 
                  determined by bit 2 of step 02. Set to "0" to allow user the 
                  option). 
         Digit 6: Super speed dial, 1 to enable (pressing N, or NN SND will  
                  dial the number stored in memory location NN). 
         Digit 7: User selectable service level, 0 to enable (allows user to  
                  set long distance/memory access dialing restrictions). 
         Digit 8: Lock function, 0 to enable (allows user to lock/un-lock the 
                  phone, if this is set to 1 the phone can not be locked). 
 
     3.  (step 11 above, suggested entry is: 00000000) 
 
         Digit 1: Handset programing, 0 to enable (allows access to programing 
                  mode without having to enter test mode). 
         Digit 2: Second phone number (not all phones), 1 to enable. 
         Digit 3: Call timer access, 0 to enable. 
         Digit 4: Auto system busy redial, 0 to enable. 
         Digit 5: Speaker disable, 1 to enable (use with select VSP units only, 
                  do not use with 2000 series mobiles). 
         Digit 6: IMTS/Cellular, 1 to enable (rarely used). 
         Digit 7: User selectable system registration, 0 to enable. 
         Digit 8: Dual antennae (diversity), 1 to enable. 
 
     4.  (step 16 above, suggested entry is: 0011010 for portable and 0011011 
         for mobile units) 
 
         Digit 1: Not used, 0 only. 
         Digit 2: Not used, 0 only 
         Digit 3: Continuous DTMF, 1 to enable (software version 8735 and later) 
         Digit 4: 8 hour time-out, 0 to enable (software version 8735 and later) 
         Digit 5: Not used, 0 only. 
         Digit 6: Failed page indicator, 0 to enable (phone beeps when an 
             incoming call is detected but signal conditions prevent 
             completion of the call). 
         Digit 7: Portable scan, 0 for portable, 1 for mobile units. 
 
 
56#  no function 
 
57x# Call Processing Mode    
                   x=0, AMPS 
                   x=1, NAMPS 
                   x=2-4, RESERVED  
                   x=5, TDMA signalling 
                   x=6, TDMA signalling with loopback before decoding 
                   x=7, TDMA signalling with loopback voice after decoding 
                   x=8, TDMA signalling with loopback FACCH after decoding 
                   x=9, TDMA forced synchronization 
 
58#  Compander On (Audio compressor and expander) (See 39#) 
 
59#  Compander Off (Audio compressor and expander) (See 38#) 
 
60#  no function 
 
61#  ESN Transfer (For Series I D.M.T./Mini TAC only) 
 
62#  Turn On Ringer Audio Path 
 
63#  Turn Off Ringer Audio Path 
 
64#-65#  no function 
 
66#  Identity Transfer (Series II Tranceivers and some Current Shipping Portables) 
 
67#  no function 
 
68#  Diaplay FLEX and Model Information 
 
69#  Used with Identity Transfer 
 
70#  Abbreviated field transmitter audio deviation command, for tranceivers 
     with FCC ID ABZ89FT5668. 
 
71#  Abbreviated field power adjustment command, for tranceivers with FCC ID 
     ABZ89FT5668. 
 
72#  Field audio phasing commands. 
 
73#  Field power adjustment command. 
 
74#-99# no function 
 
Notes:  As far as I know, this is it.  There are NO MORE commands.  As new  
        fones come out, more commands will be added.   So if anyone gets a 
        new fone, please check for more commands...I am poor.  Also, a friend 
        of mine lives in Canada and has Motorola Canada fones.  He says he 
        has found that 99# is a possible command.  So if everyone could check    
        the "no function" command numbers and give me some feedback I would 
        REALLY appreciate it.  Despite popular belief, I still say you can 
        change ESN from the keypad with NO modifications, software, or opening 
        the phone.   
------------------------------------------------------------------------------- 
Note:  This is NOT my hack.  Thanks to Patrk@delphi.com for this addition. 
 
 
                   HACKING THE FOVC 
  
 
Problem:  When listening to something interesting (a conversation), 
just when that sexy sounding horny broad begins to give her 
phone number to some lucky guy, HANDOFF!!! then static... DAMN! 
  
Trick:    Hack the FOVC. 
  
    a quick definition:  FOVC  = FOward Voice Channel 
                         FOCC  = FOward Control Channel 
                         REVC  = REverse Voice Channel 
                         RECC  = REverse Control Channel 
  
As the phone travels through cells, the FOVC is where the tower tells 
the phone to adjust power levels for the current cell or to change to 
a new channel for use in the new cell. This info can be hacked apart. 
So. When you've found a good conversation, don't be lazy! Enter 40#! 
This makes the phone listen for commands on the voice channel 
(embedded in the audio portion- you can hear it as a "bump" sound). It 
will just sit there and the display will read '40' , but the 
conversation will still be audible.  Now when the phone receives a 
FOVC command (a 40 bit sequence) data will flow across the display, in 
hex format, and stop. Listen to the phone, if the conversation is 
still there, then the command was only to adjust power levels. If the 
conversation is gone, then its a handoff. If you only got a power 
adjustment command just press # or clr,  which ever gets you back to 
the ' prompt. Enter 40# and keep listening. You can also use the # key 
to cancel the 40# command, if you want to change channels or something. 
  
If it was a handoff, its time for some quick math. You have to convert 
some of the numbers to binary, and then to decimal. I don't know how 
many characters your phone's display will show. Mine only shows the 
last seven of the ten hex digits. Count left from the end 6 digits. 
Write down that digit and the next two on a piece of paper, ie: 
  
  
    ???j16djjj    j=junk numbers  (hex numbers range from 0-9,a-f) 
       / \ 
      these are lost due to scrolling 
  
       write down  16d then convert it to a binary string: 
  
       1 = 0001 
       6 = 0110 
       d = 1101    (d=13) 
  
       now you have a binary string like this:  000101101101 
       throw away the first 2 bits and get:       0101101101 
       convert this to decimal and get:                  365 
  
  
365 is the new channel the conversation has moved to! Enter 110365# 
and voila! You too, can hear the horny babe's phone number! 
  
Don't forget to enter 40# again, as the call may be moving quickly 
through cells ( small cells or freeway driving ) or the call can get 
bounced around by the tower for cell traffic purposes. 
  
Here's one more example of the hex>binary>decimal conversion. 
  
        ???j5aejjj 
  
        5  =  0101 
        a  =  1010 
        e  =  1110 
  
        full string        = 010110101110 
        truncate 2 msb     =   0110101110 
        convert to decimal =          430 
 
 
------------------------------------------------------------------------------- 
 
 
============================================================================== 
||                                                                          || 
||           Assembling a _QUALITY_ Motorola Flip programming cable         || 
||                    from a standard battery eliminator.                   || 
||                                                                          || 
||                 Written by KG/Control Team/Umf 02/07/94                  || 
||                                                                          || 
============================================================================== 
 
     Word.  It seems that alot of bad cables are being sold by some lame asses 
here on the west coast.  The result, alot of _rare_ LO phonez are being fried. 
Welp,  this  file should clear things up.   Even if you've never made anything 
but clay pots this should be easy for ya.  Take your time and this, along with 
your phone will last a lifetime... 
 
                      Parts:  (1) 550 Battery Eliminator 
                              (2) IN4001 Diodes 
                              (1) Head pins(single row straight stick headers) 
                              (1) DB25/RS232 Connector for connection to LPT1 
                              (1) METAL DB25 cover/protector 
                              (1) 1 1/2 foot of 5 line ribbon 
                              (1) jumper wire (be creative) 
 
                      Tools:  Sizzors (I like sizzors for splicing wires) 
                              Soldering Iron 
                              Hot glue gun (borrow mom's) 
                              Exacto knife (optional) 
                              DMM w/continuity 
 
     I'll try and be as  verbose as possible.   All  references to the plastic 
part that connects the phone  to the cable will be known here as the  ADAPTER. 
The hardest  thing to  find, at  least in  where I am, is a battery eliminator 
that has all  8 pins on the  ADAPTER.   So if ya do have a cable  with all the 
pins you can  skip this  paragraph.    What I did was to go  ahead  and  shell 
out the 35 duckets for a battery  eliminator that only had pin's 7 & 8 (power) 
on the ADAPTER.   Go to you  local electronix  shop and pick up a pack of head 
pins. These  puppies are the EXACT same thing as what's in the ADAPTER,  'cept 
their nickel instead of copper.  Cut 4 of them off the plastic but be carefull 
not to bend them when you do so. 
 
     Carefully pry off the  cover of the  ADAPTER  and use the exacto knife to 
get the pins  and attatched  wires out of the  cover.   Otherwise  you'll  end 
up  melting the  cover,  and trashing  the project.  Now  de-solder the  wires 
connected to pins 7 & 8, wrap then with 2 of the ribbon's leads then re-solder 
them  back to the  same pins.   Once  again,  be  carefull  not to  bend them. 
Now  solder the other  4  ribbon lead to the pins 1, 4-6.   Now  carefully put 
each  pin  back into the  ADAPTER cover,  if some of the holes are filled with 
resin (batt eliminator),  simply push an  _extra_  bridge pin thru to get that 
shit out!  Make a note of their colors, then take the  DMM and and go over all 
the connections, making sure that no pin one pin on  the  ADAPTER is _touching 
another:  1-4, 2-8, 4-6 ect...   * note that  pins 7 & 8 will show values from 
due to the voltage regulator inside the ciggy plug. 
 
    Fire up that hot  glue gun and  place some on the cover to make sure those 
pins/ wires / solder don't move around  when ya put the ADAPTER back together. 
Don't put too much on or you wont be able to close it.   Wait a min or 2 until 
that dries, then throw some glue into the ADAPTER and quickly close it up. 
 
    As for the DB25 you shouldn't have any trouble.  Just make sure you solder 
the Diode to the wire before soldering it the the port.  Remember parallel pin 
specs are not the same as serial!! 
 
    The  following is a diagram of a  DB25 connector (soldering side). The "*" 
marks the plain  wires,  "@" marks placement of the diodes,  and the "+" marks 
where the jumper connects to the anode side of diode one: 
 
 
                                                           + 
              13  12  11  10   9   8   7   6   5   4   3   2   1 
               *   *   .   .   .   .   .   .   .   @   .   @   * 
 
                 .   .   .   .   .   .   .   *   .   .   .   . 
                25  24  23  22  21  20  19  18  17  16  15  14 
 
 
 
    Connect the cathode(black striped) side of the IN4001 to the port!!!! 
 
                        Cathode              Anode 
                        -------   |    /     ----- 
                                  |   /| 
                                  |  / | 
         LPT1/pin4 or 2   ________| /__|_________    ADAPTER pin 1 
                                  | \  |             or Jumper wire 
                                  |  \ | 
                                  |   \| 
                                  |    \ 
 
                                  IN4001 
                                                   (educational innit?) 
 
 
                               ____________ 
                              / !THE SHIT! \ 
                             /              \ 
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++ 
+                                                                            + 
+                                                                            + 
+ DB25        FLIP                                  Battery Eliminator cable + 
+ ----        ----                                  attatchment pins up:     + 
+   1(--------)4                                                             + 
+                                                     --------=              + 
+   2(--|<----)Jump this line to the Center                1  =              + 
+              Pin on the back of phone.              --------=              + 
+                                                             =              + 
+   4(--|<----)1   "|<" is the IN4001 diode.          --------=              + 
+                                                             =              + 
+  12(--------)5                                      --------=              + 
+                                                          4  =  -->To phone + 
+  13(--------)6                                      --------=              + 
+                                                          5  =              + 
+  18(-+------)8                                      --------=              + 
+      |                                                   6  =              + 
+      |    +-)7                                      --------=              + 
+      |    |                                              7* =              + 
+      |    |                                         --------=              + 
+      |    |                                              8* =              + 
+     NeG  PoS ---Cig adapter                         --------=              + 
+                                                                            + 
+                                                                            + 
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++ 
 
 
     This cable  will work with the 6.6, 9.11 & 9.9 software.  This means that 
without  a) AMPS  or  b) The Trick Clip  you'll need to find a Flip that has a 
firmware  revision  equal to or below 9122.   A good  sign  that the  phone is 
indeed a LO, is to check the ESN located on the  back and  look for any prefix 
below A2A.   If  you can't locate the  ESN sticker, usually cause it's stolen, 
then look  for a MCsquared printed along with the menu sticker.   If the phone 
has the MC2 don't buy it.   If the phone doesn't  have the menu  sticker don't 
buy it!  Also before you fork over the $$$ make sure that all the ports on the 
phone are in good condition. 
 
     Some people may experience  problems with 486 machines.  I'm looking into 
slowing the shit down in order for the phone to respond.  One way is to divide 
your  BIOS bus clock by 6,  another is to load a  TSR that actually slows your 
CPU,  although I haven't yet  found this to work for me.   286-386  processors 
work fine.  Short cables are a must! 
 
 
------------------------------------------------------------------------------ 
 
 
From: locke@dfw.net 
Date: Thu, 20 Oct 1994 09:53:54 GMT 
 
I just thought I would lend a little help to those of you that may try and  
actually USE this schematic.  While _close_ to the actual pinouts... this 
diagram will not work. 
 
I have included corrections for the FLIP and the BRICK below, with  
the word [LOCKE] next to my corrections.  Sorry if I confuse anyone. 
 
Anyway, I hope this helps, you CANNOT program the phones without 
twisting/connecting the additional 19 & 20 DB25 connections. 
 
Motorol Transciever,s 
_____________________ 
4500x,4800x,6800x,Etc. 
______________________ 
Female 25 Pin                                Male 25 Pin 
D-Connector                                  D-connector 
To transciever                               To P.C.Parallel Port 
          Pin                                     Pin 
          1._____________________________________  4. 
          2._____________________________________ 18. 
                                     ___10k______ 13. 
                                    /  
  ______4+5._______________________/____10K______ 12. 
 |       12.____________________________________/ 
 |       11._____________________________________ 13. 
 |       18._____________________________________  1. 
 |       21._____________________________________  2. 
 |    ___14+17+20+23.____________________________ 18. 
 |    | 
 |    |___ -ve 
 | 
 |________ +ve 9 Volt 
 
 
> Motorola 8500x 8800x(early type) 
> ________________________________ 
>   
> 25 Pin D-plug(P.C.lpt1)           Phone Back(battery removed) 
>   
> Pin          Diode,s         []    []    []      []    []    [] 
>  3.--orange-|<1n4001---------------------/       /           /  
>  4.--blue---|<1n4001----------------------------/           /  
>  2.--red----|<1n4001---------------------------------------/ 
>   
 
  [LOCKE]    ------19, 20  (all tied together & connected to 18) 
             | |  
>            | |               []    []    []     []     []    [] 
> 18.--black-------------------/     /            /      / 
> 13.--yellow-----------------------/            /      / 
> 12.--brown------------------------------------/      / 
>  1.--grey-------------------------------------------/ 
>   
>   
>   
>                              []                              []  
>                          -8 to -12V.                     +8 to =12V. 
> NOTE Diode protocol: Kathode---|<diode---Anode 
 
> Motorola 9800x Personal tac1 etc. 
> 25 pin D-plug(P.C. LPT1)                     Phone Back(battery removed) 
>   
> Pin            Diode,s             Battery terminals--> [] [] [] 
>                                                            | 
>  2.--black----|<1n4001-------------------------------------| 
>                                                             \ 
>                                                              \black fly lead 
>   
>                              Data plug---> |    |    |    |    |    | 
   |    | 
>                                            |    |    |    |    |    | 
   |    | 
> [LOCKE]  ----- 19, 20                    white  /   blue  /  yellow     red 
>          | |                              /    /    /  green  /         / 
>          | |                             /    /    /    /    /         / 
> 18.--white----Neg 8-12V-----------------/    /    /    /    /         / 
    
   [LOCKE] the POSITIVE connection goes 
           here (below) it does not connect 
           to ANY of the DBxx cable wires. 
                               | (+12v) 
>              +8 to +12V---------------------/    /    /    /         / 
> 13.--blue---------------------------------------/    /    /         / 
> 12.--green------------------------------------------/    /         / 
>  1.--yellow---------------------------------------------/         / 
>  4.--red------|<1n4001-------------------------------------------/ 
>   
> NOTE Diode protocol: Kathode---|<diode---Anode 
 
NEC 9A 
______                           __                             __ 
                                 ||                             || 
 25 Pin D-Plug(LPT1)             ||                             || 
____________________             ||                             || 
                                 ||                             || 
Pin                             _||__________         __________||__ 
  1.green                       |           |         |            | 
  6.-|<1n4148------             | phone     /          \  phone    | 
  8.-|<1n4148--   |             |          /            \          | 
              |   |             |          |            |          | 
              |   |      back-->|          |<---front-->|          |<--back 
 10.-----------   |             |          |            |          | 
 13.-----------------red        |          \            /          | 
 15.------blue                    | | | |                 | | | | 
 18.------black                       |                     / |  \ 
                                      |                    /  |   \ 
                                    black             blue/ green  \red  
 
Diodes = 1N4148 
 
NOTE Diode protocol: Kathode---|<diode---Anode 
NEC 11A transciever 
 
**NOTE-A car kit power loom is required to power phone, also a handset  
is required, and is plugged into the female end of the gender change plug. 
 
**NOTE-The gender change plug is a male 15 pin D plug soldered back to back 
back with a female 15 pin D socket. Male end interfaces transceiver, female 
end interfaces the handset. 
 
 25 Pin D-Plug(LPT1)                       15 Pin D-Gender changer 
____________________                       _______________________ 
 Pin                                        Pin 
  1.------green----------------------------- 13. green 
  6.-|<1n4148------  
  8.-|<1n4148--   |  
              |   |  
 10.-----------   |  
 13.------red--------------------------------12. red 
 15.------blue-------------------------------14. blue 
 18.------black-------------------------------2. black 
    \-----black------------------------------11. black 
Power supply 12V dc. Power up using handset BEFORE interfacing computer LPT1. 
NOTE Diode protocol: Kathode---|<diode---Anode 
NEC P3. 
_______ 
 
25 Pin D-plug LPT1.                         Plug on end of curly cord. 
___________________                         __________________________ 
 
Pin 25.--------------------black--------------------------------------| 
Pin 15.--------------------red-------------------------------------|  | 
Pin  6.---|<In4148--|                                              |  | 
Pin 13.-------------|------white--------------------------------|  |  | 
                                                  ||   [] [] [] [] [] [] 
                         view into plug:aerial---><> 
Pin  3.---|<1N4148---|                            ||   [] [] [] [] [] [] 
Pin 12.--------------|-----brown--------------------------------| 
 
NOTE Diode protocol: Kathode---|<diode---Anode 
  NEC P4 
  ______ 
 
  25 Pin D-plug LPT1.   Transistors 2N3904 npn   NAM Adaptor Plug    
  ___________________   ______________________   __________________ 
 
  Pin 15.-----C-\------green----------------------------------------| 
                 \                                                  | 
  Pin  2.-10K-B---O                                                 | 
                 /                                                  | 
  Pin 19.-----E-/------blue-----------------------------|           | 
  Pin 19.-----E-\                                       |           | 
                 \                                      |           | 
  Pin  4.-10K-B---O                                     |           | 
                 /                                      |           | 
  Pin 12.-----C-/---|--yellow                           |           | 
                    |                                   |           | 
                    |                                   |           | 
                    |   NAM Adaptor plug: aerial ---><> [] [] [] [] [] [] [] [] 
                    |                                            |      | 
  Pin 13.----red---(|)-------------------------------------------|      | 
                    |                                                   | 
                    |---------------------------------------------------| 
Panasonic D,E,F  
---------------- 
  Build the Maplins 'RS232 to TTL conversion board 'MAX232(Order Code 
LM75S)to    specification, except do not include resistor R5. 
Switches SW-1 must be in the  OFF position. 
 
 
--------------------------Press any Key to continue--------------------------- 
 9 PIN SERIAL D-PLUG                                  Interface PL2 on MAX232 
Pin 8.----------------|--IN4148>|----\ 
Pin 7.----------------|               \___________________ 1.Pin 
                                      / 
Pin 4.----------------|--IN4148>|----/ 
Pin 6.----------------| 
Pin 3.-----------------------------------------------------7.Pin 
Pin 2.-----------------------------------------------------6.Pin 
Pin 5.-----------------------------------------------------8.Pin 
***************************************************************************** 
 PL1.on MAX232----------'F'Lead------------'D'Lead-----------'E'Lead 
 Pin 2+6                 pin 1.             pin 6.            pin 5.        
 Pin 5                   pin 6.             pin 5.            pin 1. 
 Pin 7.                  pin 2.             pin 4.            Link to program 
                                                          ___ Pin/Power lead  
 Pin 8.                  pin 8.           aerial brade  /     Pin 8.          
                                                       /       /////           
                        1 3 5 7             2  4  6   /1_______|  |_________12 
                        [][][][]            [] [] []  [][][][][][][][][][][][] 
   View of Plugs-->   <>                 <>           |______________________| 
                        [][][][]            [] [] []       |_________________| 
                        2 4 6 8             1  3  5 
Diode Protocol: Anode---diode>|--Kadthode 
 
-------------------------------------------------------------------------------- 
 
Final Note:  I HAVE NEVER TESTED ANY OF THESE CABLE SPECS!!!  I REPEAT.   
             I HAVE NEVER TRIED ANY OF THESE CABLE SPECS!  THE USE OF THESE 
             CABLES COULD DESTROY YOUR PHONE IF THE CABLES ARE MADE  
             INCORRECTLY.  Whether these specs are good or bad is news to me. 
             So if someone could e-mail me to let me know one way or another I 
             would be REALLY obliged.  The reason I have never tried these is 
             because I HAVE NO DAMN SOFTWARE to use them with.  Someone  
             UUENCODE a copy of the newest Motorola software to me (unless it  
             is that crap floating around that only changes shit you could do 
             with the above commands.  ESN changing software is what I need.) 
             Anyone with experience in disassembling Motorola's software 
             should e-mail me.  We need to get together.   
 
        Mike.Larsen@uti.com 
        Stularsenmic@vax.colsf.edu 
 
----------------------------------------------------------------------------- 
The following text was mailed to me but there was no credit given to the source 
of this info.  I'm sorry and will correct it if given the proper credits. 
                                                                -ML 
 
CELLULAR PHONE FREQUENCIES AND MOTOROLA 
TEST MODE NUMERIC CODES. 
( Motorola test mode channel numbers ) 
( are for use in motorola test mode  ) 
( with function 11xxxx#              ) 
( All frequencies in Megahertz FM    ) 
Lower Set (1-666) 
 
Tower Freq.  Mobile Freq.    11xxxx# Channel 
 
Tx  870.03   Rx  825.03  Chan  0001  #1 
Tx  870.06   Rx  825.06  Chan  0002  #2 
Tx  870.09   Rx  825.09  Chan  0003  #3 
Tx  870.12   Rx  825.12  Chan  0004  #4 
Tx  870.15   Rx  825.15  Chan  0005  #5 
Tx  870.18   Rx  825.18  Chan  0006  #6 
Tx  870.21   Rx  825.21  Chan  0007  #7 
Tx  870.24   Rx  825.24  Chan  0008  #8 
Tx  870.27   Rx  825.27  Chan  0009  #9 
Tx  870.30   Rx  825.30  Chan  0010  #10 
Tx  870.33   Rx  825.33  Chan  0011  #11 
Tx  870.36   Rx  825.36  Chan  0012  #12 
Tx  870.39   Rx  825.39  Chan  0013  #13 
Tx  870.42   Rx  825.42  Chan  0014  #14 
Tx  870.45   Rx  825.45  Chan  0015  #15 
Tx  870.48   Rx  825.48  Chan  0016  #16 
Tx  870.51   Rx  825.51  Chan  0017  #17 
Tx  870.54   Rx  825.54  Chan  0018  #18 
Tx  870.57   Rx  825.57  Chan  0019  #19 
Tx  870.60   Rx  825.60  Chan  0020  #20 
Tx  870.63   Rx  825.63  Chan  0021  #21 
Tx  870.66   Rx  825.66  Chan  0022  #22 
Tx  870.69   Rx  825.69  Chan  0023  #23 
Tx  870.72   Rx  825.72  Chan  0024  #24 
Tx  870.75   Rx  825.75  Chan  0025  #25 
Tx  870.78   Rx  825.78  Chan  0026  #26 
Tx  870.81   Rx  825.81  Chan  0027  #27 
Tx  870.84   Rx  825.84  Chan  0028  #28 
Tx  870.87   Rx  825.87  Chan  0029  #29 
Tx  870.90   Rx  825.90  Chan  0030  #30 
Tx  870.93   Rx  825.93  Chan  0031  #31 
Tx  870.96   Rx  825.96  Chan  0032  #32 
Tx  870.99   Rx  825.99  Chan  0033  #33 
Tx  871.02   Rx  826.02  Chan  0034  #34 
Tx  871.05   Rx  826.05  Chan  0035  #35 
Tx  871.08   Rx  826.08  Chan  0036  #36 
Tx  871.11   Rx  826.11  Chan  0037  #37 
Tx  871.14   Rx  826.14  Chan  0038  #38 
Tx  871.17   Rx  826.17  Chan  0039  #39 
Tx  871.20   Rx  826.20  Chan  0040  #40 
Tx  871.23   Rx  826.23  Chan  0041  #41 
Tx  871.26   Rx  826.26  Chan  0042  #42 
Tx  871.29   Rx  826.29  Chan  0043  #43 
Tx  871.32   Rx  826.32  Chan  0044  #44 
Tx  871.35   Rx  826.35  Chan  0045  #45 
Tx  871.38   Rx  826.38  Chan  0046  #46 
Tx  871.41   Rx  826.41  Chan  0047  #47 
Tx  871.44   Rx  826.44  Chan  0048  #48 
Tx  871.47   Rx  826.47  Chan  0049  #49 
Tx  871.50   Rx  826.50  Chan  0050  #50 
Tx  871.53   Rx  826.53  Chan  0051  #51 
Tx  871.56   Rx  826.56  Chan  0052  #52 
Tx  871.59   Rx  826.59  Chan  0053  #53 
Tx  871.62   Rx  826.62  Chan  0054  #54 
Tx  871.65   Rx  826.65  Chan  0055  #55 
Tx  871.68   Rx  826.68  Chan  0056  #56 
Tx  871.71   Rx  826.71  Chan  0057  #57 
Tx  871.74   Rx  826.74  Chan  0058  #58 
Tx  871.77   Rx  826.77  Chan  0059  #59 
Tx  871.80   Rx  826.80  Chan  0060  #60 
Tx  871.83   Rx  826.83  Chan  0061  #61 
Tx  871.86   Rx  826.86  Chan  0062  #62 
Tx  871.89   Rx  826.89  Chan  0063  #63 
Tx  871.92   Rx  826.92  Chan  0064  #64 
Tx  871.95   Rx  826.95  Chan  0065  #65 
Tx  871.98   Rx  826.98  Chan  0066  #66 
Tx  872.01   Rx  827.01  Chan  0067  #67 
Tx  872.04   Rx  827.04  Chan  0068  #68 
Tx  872.07   Rx  827.07  Chan  0069  #69 
Tx  872.10   Rx  827.10  Chan  0070  #70 
Tx  872.13   Rx  827.13  Chan  0071  #71 
Tx  872.16   Rx  827.16  Chan  0072  #72 
Tx  872.19   Rx  827.19  Chan  0073  #73 
Tx  872.22   Rx  827.22  Chan  0074  #74 
Tx  872.25   Rx  827.25  Chan  0075  #75 
Tx  872.28   Rx  827.28  Chan  0076  #76 
Tx  872.31   Rx  827.31  Chan  0077  #77 
Tx  872.34   Rx  827.34  Chan  0078  #78 
Tx  872.37   Rx  827.37  Chan  0079  #79 
Tx  872.40   Rx  827.40  Chan  0080  #80 
Tx  872.43   Rx  827.43  Chan  0081  #81 
Tx  872.46   Rx  827.46  Chan  0082  #82 
Tx  872.49   Rx  827.49  Chan  0083  #83 
Tx  872.52   Rx  827.52  Chan  0084  #84 
Tx  872.55   Rx  827.55  Chan  0085  #85 
Tx  872.58   Rx  827.58  Chan  0086  #86 
Tx  872.61   Rx  827.61  Chan  0087  #87 
Tx  872.64   Rx  827.64  Chan  0088  #88 
Tx  872.67   Rx  827.67  Chan  0089  #89 
Tx  872.70   Rx  827.70  Chan  0090  #90 
Tx  872.73   Rx  827.73  Chan  0091  #91 
Tx  872.76   Rx  827.76  Chan  0092  #92 
Tx  872.79   Rx  827.79  Chan  0093  #93 
Tx  872.82   Rx  827.82  Chan  0094  #94 
Tx  872.85   Rx  827.85  Chan  0095  #95 
Tx  872.88   Rx  827.88  Chan  0096  #96 
Tx  872.91   Rx  827.91  Chan  0097  #97 
Tx  872.94   Rx  827.94  Chan  0098  #98 
Tx  872.97   Rx  827.97  Chan  0099  #99 
Tx  873.00   Rx  828.00  Chan  0100  #100 
Tx  873.03   Rx  828.03  Chan  0101  #101 
Tx  873.06   Rx  828.06  Chan  0102  #102 
Tx  873.09   Rx  828.09  Chan  0103  #103 
Tx  873.12   Rx  828.12  Chan  0104  #104 
Tx  873.15   Rx  828.15  Chan  0105  #105 
Tx  873.18   Rx  828.18  Chan  0106  #106 
Tx  873.21   Rx  828.21  Chan  0107  #107 
Tx  873.24   Rx  828.24  Chan  0108  #108 
Tx  873.27   Rx  828.27  Chan  0109  #109 
Tx  873.30   Rx  828.30  Chan  0110  #110 
Tx  873.33   Rx  828.33  Chan  0111  #111 
Tx  873.36   Rx  828.36  Chan  0112  #112 
Tx  873.39   Rx  828.39  Chan  0113  #113 
Tx  873.42   Rx  828.42  Chan  0114  #114 
Tx  873.45   Rx  828.45  Chan  0115  #115 
Tx  873.48   Rx  828.48  Chan  0116  #116 
Tx  873.51   Rx  828.51  Chan  0117  #117 
Tx  873.54   Rx  828.54  Chan  0118  #118 
Tx  873.57   Rx  828.57  Chan  0119  #119 
Tx  873.60   Rx  828.60  Chan  0120  #120 
Tx  873.63   Rx  828.63  Chan  0121  #121 
Tx  873.66   Rx  828.66  Chan  0122  #122 
Tx  873.69   Rx  828.69  Chan  0123  #123 
Tx  873.72   Rx  828.72  Chan  0124  #124 
Tx  873.75   Rx  828.75  Chan  0125  #125 
Tx  873.78   Rx  828.78  Chan  0126  #126 
Tx  873.81   Rx  828.81  Chan  0127  #127 
Tx  873.84   Rx  828.84  Chan  0128  #128 
Tx  873.87   Rx  828.87  Chan  0129  #129 
Tx  873.90   Rx  828.90  Chan  0130  #130 
Tx  873.93   Rx  828.93  Chan  0131  #131 
Tx  873.96   Rx  828.96  Chan  0132  #132 
Tx  873.99   Rx  828.99  Chan  0133  #133 
Tx  874.02   Rx  829.02  Chan  0134  #134 
Tx  874.05   Rx  829.05  Chan  0135  #135 
Tx  874.08   Rx  829.08  Chan  0136  #136 
Tx  874.11   Rx  829.11  Chan  0137  #137 
Tx  874.14   Rx  829.14  Chan  0138  #138 
Tx  874.17   Rx  829.17  Chan  0139  #139 
Tx  874.20   Rx  829.20  Chan  0140  #140 
Tx  874.23   Rx  829.23  Chan  0141  #141 
Tx  874.26   Rx  829.26  Chan  0142  #142 
Tx  874.29   Rx  829.29  Chan  0143  #143 
Tx  874.32   Rx  829.32  Chan  0144  #144 
Tx  874.35   Rx  829.35  Chan  0145  #145 
Tx  874.38   Rx  829.38  Chan  0146  #146 
Tx  874.41   Rx  829.41  Chan  0147  #147 
Tx  874.44   Rx  829.44  Chan  0148  #148 
Tx  874.47   Rx  829.47  Chan  0149  #149 
Tx  874.50   Rx  829.50  Chan  0150  #150 
Tx  874.53   Rx  829.53  Chan  0151  #151 
Tx  874.56   Rx  829.56  Chan  0152  #152 
Tx  874.59   Rx  829.59  Chan  0153  #153 
Tx  874.62   Rx  829.62  Chan  0154  #154 
Tx  874.65   Rx  829.65  Chan  0155  #155 
Tx  874.68   Rx  829.68  Chan  0156  #156 
Tx  874.71   Rx  829.71  Chan  0157  #157 
Tx  874.74   Rx  829.74  Chan  0158  #158 
Tx  874.77   Rx  829.77  Chan  0159  #159 
Tx  874.80   Rx  829.80  Chan  0160  #160 
Tx  874.83   Rx  829.83  Chan  0161  #161 
Tx  874.86   Rx  829.86  Chan  0162  #162 
Tx  874.89   Rx  829.89  Chan  0163  #163 
Tx  874.92   Rx  829.92  Chan  0164  #164 
Tx  874.95   Rx  829.95  Chan  0165  #165 
Tx  874.98   Rx  829.98  Chan  0166  #166 
Tx  875.01   Rx  830.01  Chan  0167  #167 
Tx  875.04   Rx  830.04  Chan  0168  #168 
Tx  875.07   Rx  830.07  Chan  0169  #169 
Tx  875.10   Rx  830.10  Chan  0170  #170 
Tx  875.13   Rx  830.13  Chan  0171  #171 
Tx  875.16   Rx  830.16  Chan  0172  #172 
Tx  875.19   Rx  830.19  Chan  0173  #173 
Tx  875.22   Rx  830.22  Chan  0174  #174 
Tx  875.25   Rx  830.25  Chan  0175  #175 
Tx  875.28   Rx  830.28  Chan  0176  #176 
Tx  875.31   Rx  830.31  Chan  0177  #177 
Tx  875.34   Rx  830.34  Chan  0178  #178 
Tx  875.37   Rx  830.37  Chan  0179  #179 
Tx  875.40   Rx  830.40  Chan  0180  #180 
Tx  875.43   Rx  830.43  Chan  0181  #181 
Tx  875.46   Rx  830.46  Chan  0182  #182 
Tx  875.49   Rx  830.49  Chan  0183  #183 
Tx  875.52   Rx  830.52  Chan  0184  #184 
Tx  875.55   Rx  830.55  Chan  0185  #185 
Tx  875.58   Rx  830.58  Chan  0186  #186 
Tx  875.61   Rx  830.61  Chan  0187  #187 
Tx  875.64   Rx  830.64  Chan  0188  #188 
Tx  875.67   Rx  830.67  Chan  0189  #189 
Tx  875.70   Rx  830.70  Chan  0190  #190 
Tx  875.73   Rx  830.73  Chan  0191  #191 
Tx  875.76   Rx  830.76  Chan  0192  #192 
Tx  875.79   Rx  830.79  Chan  0193  #193 
Tx  875.82   Rx  830.82  Chan  0194  #194 
Tx  875.85   Rx  830.85  Chan  0195  #195 
Tx  875.88   Rx  830.88  Chan  0196  #196 
Tx  875.91   Rx  830.91  Chan  0197  #197 
Tx  875.94   Rx  830.94  Chan  0198  #198 
Tx  875.97   Rx  830.97  Chan  0199  #199 
Tx  876.00   Rx  831.00  Chan  0200  #200 
Tx  876.03   Rx  831.03  Chan  0201  #201 
Tx  876.06   Rx  831.06  Chan  0202  #202 
Tx  876.09   Rx  831.09  Chan  0203  #203 
Tx  876.12   Rx  831.12  Chan  0204  #204 
Tx  876.15   Rx  831.15  Chan  0205  #205 
Tx  876.18   Rx  831.18  Chan  0206  #206 
Tx  876.21   Rx  831.21  Chan  0207  #207 
Tx  876.24   Rx  831.24  Chan  0208  #208 
Tx  876.27   Rx  831.27  Chan  0209  #209 
Tx  876.30   Rx  831.30  Chan  0210  #210 
Tx  876.33   Rx  831.33  Chan  0211  #211 
Tx  876.36   Rx  831.36  Chan  0212  #212 
Tx  876.39   Rx  831.39  Chan  0213  #213 
Tx  876.42   Rx  831.42  Chan  0214  #214 
Tx  876.45   Rx  831.45  Chan  0215  #215 
Tx  876.48   Rx  831.48  Chan  0216  #216 
Tx  876.51   Rx  831.51  Chan  0217  #217 
Tx  876.54   Rx  831.54  Chan  0218  #218 
Tx  876.57   Rx  831.57  Chan  0219  #219 
Tx  876.60   Rx  831.60  Chan  0220  #220 
Tx  876.63   Rx  831.63  Chan  0221  #221 
Tx  876.66   Rx  831.66  Chan  0222  #222 
Tx  876.69   Rx  831.69  Chan  0223  #223 
Tx  876.72   Rx  831.72  Chan  0224  #224 
Tx  876.75   Rx  831.75  Chan  0225  #225 
Tx  876.78   Rx  831.78  Chan  0226  #226 
Tx  876.81   Rx  831.81  Chan  0227  #227 
Tx  876.84   Rx  831.84  Chan  0228  #228 
Tx  876.87   Rx  831.87  Chan  0229  #229 
Tx  876.90   Rx  831.90  Chan  0230  #230 
Tx  876.93   Rx  831.93  Chan  0231  #231 
Tx  876.96   Rx  831.96  Chan  0232  #232 
Tx  876.99   Rx  831.99  Chan  0233  #233 
Tx  877.02   Rx  832.02  Chan  0234  #234 
Tx  877.05   Rx  832.05  Chan  0235  #235 
Tx  877.08   Rx  832.08  Chan  0236  #236 
Tx  877.11   Rx  832.11  Chan  0237  #237 
Tx  877.14   Rx  832.14  Chan  0238  #238 
Tx  877.17   Rx  832.17  Chan  0239  #239 
Tx  877.20   Rx  832.20  Chan  0240  #240 
Tx  877.23   Rx  832.23  Chan  0241  #241 
Tx  877.26   Rx  832.26  Chan  0242  #242 
Tx  877.29   Rx  832.29  Chan  0243  #243 
Tx  877.32   Rx  832.32  Chan  0244  #244 
Tx  877.35   Rx  832.35  Chan  0245  #245 
Tx  877.38   Rx  832.38  Chan  0246  #246 
Tx  877.41   Rx  832.41  Chan  0247  #247 
Tx  877.44   Rx  832.44  Chan  0248  #248 
Tx  877.47   Rx  832.47  Chan  0249  #249 
Tx  877.50   Rx  832.50  Chan  0250  #250 
Tx  877.53   Rx  832.53  Chan  0251  #251 
Tx  877.56   Rx  832.56  Chan  0252  #252 
Tx  877.59   Rx  832.59  Chan  0253  #253 
Tx  877.62   Rx  832.62  Chan  0254  #254 
Tx  877.65   Rx  832.65  Chan  0255  #255 
Tx  877.68   Rx  832.68  Chan  0256  #256 
Tx  877.71   Rx  832.71  Chan  0257  #257 
Tx  877.74   Rx  832.74  Chan  0258  #258 
Tx  877.77   Rx  832.77  Chan  0259  #259 
Tx  877.80   Rx  832.80  Chan  0260  #260 
Tx  877.83   Rx  832.83  Chan  0261  #261 
Tx  877.86   Rx  832.86  Chan  0262  #262 
Tx  877.89   Rx  832.89  Chan  0263  #263 
Tx  877.92   Rx  832.92  Chan  0264  #264 
Tx  877.95   Rx  832.95  Chan  0265  #265 
Tx  877.98   Rx  832.98  Chan  0266  #266 
Tx  878.01   Rx  833.01  Chan  0267  #267 
Tx  878.04   Rx  833.04  Chan  0268  #268 
Tx  878.07   Rx  833.07  Chan  0269  #269 
Tx  878.10   Rx  833.10  Chan  0270  #270 
Tx  878.13   Rx  833.13  Chan  0271  #271 
Tx  878.16   Rx  833.16  Chan  0272  #272 
Tx  878.19   Rx  833.19  Chan  0273  #273 
Tx  878.22   Rx  833.22  Chan  0274  #274 
Tx  878.25   Rx  833.25  Chan  0275  #275 
Tx  878.28   Rx  833.28  Chan  0276  #276 
Tx  878.31   Rx  833.31  Chan  0277  #277 
Tx  878.34   Rx  833.34  Chan  0278  #278 
Tx  878.37   Rx  833.37  Chan  0279  #279 
Tx  878.40   Rx  833.40  Chan  0280  #280 
Tx  878.43   Rx  833.43  Chan  0281  #281 
Tx  878.46   Rx  833.46  Chan  0282  #282 
Tx  878.49   Rx  833.49  Chan  0283  #283 
Tx  878.52   Rx  833.52  Chan  0284  #284 
Tx  878.55   Rx  833.55  Chan  0285  #285 
Tx  878.58   Rx  833.58  Chan  0286  #286 
Tx  878.61   Rx  833.61  Chan  0287  #287 
Tx  878.64   Rx  833.64  Chan  0288  #288 
Tx  878.67   Rx  833.67  Chan  0289  #289 
Tx  878.70   Rx  833.70  Chan  0290  #290 
Tx  878.73   Rx  833.73  Chan  0291  #291 
Tx  878.76   Rx  833.76  Chan  0292  #292 
Tx  878.79   Rx  833.79  Chan  0293  #293 
Tx  878.82   Rx  833.82  Chan  0294  #294 
Tx  878.85   Rx  833.85  Chan  0295  #295 
Tx  878.88   Rx  833.88  Chan  0296  #296 
Tx  878.91   Rx  833.91  Chan  0297  #297 
Tx  878.94   Rx  833.94  Chan  0298  #298 
Tx  878.97   Rx  833.97  Chan  0299  #299 
Tx  879.00   Rx  834.00  Chan  0300  #300 
Tx  879.03   Rx  834.03  Chan  0301  #301 
Tx  879.06   Rx  834.06  Chan  0302  #302 
Tx  879.09   Rx  834.09  Chan  0303  #303 
Tx  879.12   Rx  834.12  Chan  0304  #304 
Tx  879.15   Rx  834.15  Chan  0305  #305 
Tx  879.18   Rx  834.18  Chan  0306  #306 
Tx  879.21   Rx  834.21  Chan  0307  #307 
Tx  879.24   Rx  834.24  Chan  0308  #308 
Tx  879.27   Rx  834.27  Chan  0309  #309 
Tx  879.30   Rx  834.30  Chan  0310  #310 
Tx  879.33   Rx  834.33  Chan  0311  #311 
Tx  879.36   Rx  834.36  Chan  0312  #312 
Tx  879.39   Rx  834.39  Chan  0313  #313 
Tx  879.42   Rx  834.42  Chan  0314  #314 
Tx  879.45   Rx  834.45  Chan  0315  #315 
Tx  879.48   Rx  834.48  Chan  0316  #316 
Tx  879.51   Rx  834.51  Chan  0317  #317 
Tx  879.54   Rx  834.54  Chan  0318  #318 
Tx  879.57   Rx  834.57  Chan  0319  #319 
Tx  879.60   Rx  834.60  Chan  0320  #320 
Tx  879.63   Rx  834.63  Chan  0321  #321 
Tx  879.66   Rx  834.66  Chan  0322  #322 
Tx  879.69   Rx  834.69  Chan  0323  #323 
Tx  879.72   Rx  834.72  Chan  0324  #324 
Tx  879.75   Rx  834.75  Chan  0325  #325 
Tx  879.78   Rx  834.78  Chan  0326  #326 
Tx  879.81   Rx  834.81  Chan  0327  #327 
Tx  879.84   Rx  834.84  Chan  0328  #328 
Tx  879.87   Rx  834.87  Chan  0329  #329 
Tx  879.90   Rx  834.90  Chan  0330  #330 
Tx  879.93   Rx  834.93  Chan  0331  #331 
Tx  879.96   Rx  834.96  Chan  0332  #332 
Tx  879.99   Rx  834.99  Chan  0333  #333 
Tx  880.02   Rx  835.02  Chan  0334  #334 
Tx  880.05   Rx  835.05  Chan  0335  #335 
Tx  880.08   Rx  835.08  Chan  0336  #336 
Tx  880.11   Rx  835.11  Chan  0337  #337 
Tx  880.14   Rx  835.14  Chan  0338  #338 
Tx  880.17   Rx  835.17  Chan  0339  #339 
Tx  880.20   Rx  835.20  Chan  0340  #340 
Tx  880.23   Rx  835.23  Chan  0341  #341 
Tx  880.26   Rx  835.26  Chan  0342  #342 
Tx  880.29   Rx  835.29  Chan  0343  #343 
Tx  880.32   Rx  835.32  Chan  0344  #344 
Tx  880.35   Rx  835.35  Chan  0345  #345 
Tx  880.38   Rx  835.38  Chan  0346  #346 
Tx  880.41   Rx  835.41  Chan  0347  #347 
Tx  880.44   Rx  835.44  Chan  0348  #348 
Tx  880.47   Rx  835.47  Chan  0349  #349 
Tx  880.50   Rx  835.50  Chan  0350  #350 
Tx  880.53   Rx  835.53  Chan  0351  #351 
Tx  880.56   Rx  835.56  Chan  0352  #352 
Tx  880.59   Rx  835.59  Chan  0353  #353 
Tx  880.62   Rx  835.62  Chan  0354  #354 
Tx  880.65   Rx  835.65  Chan  0355  #355 
Tx  880.68   Rx  835.68  Chan  0356  #356 
Tx  880.71   Rx  835.71  Chan  0357  #357 
Tx  880.74   Rx  835.74  Chan  0358  #358 
Tx  880.77   Rx  835.77  Chan  0359  #359 
Tx  880.80   Rx  835.80  Chan  0360  #360 
Tx  880.83   Rx  835.83  Chan  0361  #361 
Tx  880.86   Rx  835.86  Chan  0362  #362 
Tx  880.89   Rx  835.89  Chan  0363  #363 
Tx  880.92   Rx  835.92  Chan  0364  #364 
Tx  880.95   Rx  835.95  Chan  0365  #365 
Tx  880.98   Rx  835.98  Chan  0366  #366 
Tx  881.01   Rx  836.01  Chan  0367  #367 
Tx  881.04   Rx  836.04  Chan  0368  #368 
Tx  881.07   Rx  836.07  Chan  0369  #369 
Tx  881.10   Rx  836.10  Chan  0370  #370 
Tx  881.13   Rx  836.13  Chan  0371  #371 
Tx  881.16   Rx  836.16  Chan  0372  #372 
Tx  881.19   Rx  836.19  Chan  0373  #373 
Tx  881.22   Rx  836.22  Chan  0374  #374 
Tx  881.25   Rx  836.25  Chan  0375  #375 
Tx  881.28   Rx  836.28  Chan  0376  #376 
Tx  881.31   Rx  836.31  Chan  0377  #377 
Tx  881.34   Rx  836.34  Chan  0378  #378 
Tx  881.37   Rx  836.37  Chan  0379  #379 
Tx  881.40   Rx  836.40  Chan  0380  #380 
Tx  881.43   Rx  836.43  Chan  0381  #381 
Tx  881.46   Rx  836.46  Chan  0382  #382 
Tx  881.49   Rx  836.49  Chan  0383  #383 
Tx  881.52   Rx  836.52  Chan  0384  #384 
Tx  881.55   Rx  836.55  Chan  0385  #385 
Tx  881.58   Rx  836.58  Chan  0386  #386 
Tx  881.61   Rx  836.61  Chan  0387  #387 
Tx  881.64   Rx  836.64  Chan  0388  #388 
Tx  881.67   Rx  836.67  Chan  0389  #389 
Tx  881.70   Rx  836.70  Chan  0390  #390 
Tx  881.73   Rx  836.73  Chan  0391  #391 
Tx  881.76   Rx  836.76  Chan  0392  #392 
Tx  881.79   Rx  836.79  Chan  0393  #393 
Tx  881.82   Rx  836.82  Chan  0394  #394 
Tx  881.85   Rx  836.85  Chan  0395  #395 
Tx  881.88   Rx  836.88  Chan  0396  #396 
Tx  881.91   Rx  836.91  Chan  0397  #397 
Tx  881.94   Rx  836.94  Chan  0398  #398 
Tx  881.97   Rx  836.97  Chan  0399  #399 
Tx  882.00   Rx  837.00  Chan  0400  #400 
Tx  882.03   Rx  837.03  Chan  0401  #401 
Tx  882.06   Rx  837.06  Chan  0402  #402 
Tx  882.09   Rx  837.09  Chan  0403  #403 
Tx  882.12   Rx  837.12  Chan  0404  #404 
Tx  882.15   Rx  837.15  Chan  0405  #405 
Tx  882.18   Rx  837.18  Chan  0406  #406 
Tx  882.21   Rx  837.21  Chan  0407  #407 
Tx  882.24   Rx  837.24  Chan  0408  #408 
Tx  882.27   Rx  837.27  Chan  0409  #409 
Tx  882.30   Rx  837.30  Chan  0410  #410 
Tx  882.33   Rx  837.33  Chan  0411  #411 
Tx  882.36   Rx  837.36  Chan  0412  #412 
Tx  882.39   Rx  837.39  Chan  0413  #413 
Tx  882.42   Rx  837.42  Chan  0414  #414 
Tx  882.45   Rx  837.45  Chan  0415  #415 
Tx  882.48   Rx  837.48  Chan  0416  #416 
Tx  882.51   Rx  837.51  Chan  0417  #417 
Tx  882.54   Rx  837.54  Chan  0418  #418 
Tx  882.57   Rx  837.57  Chan  0419  #419 
Tx  882.60   Rx  837.60  Chan  0420  #420 
Tx  882.63   Rx  837.63  Chan  0421  #421 
Tx  882.66   Rx  837.66  Chan  0422  #422 
Tx  882.69   Rx  837.69  Chan  0423  #423 
Tx  882.72   Rx  837.72  Chan  0424  #424 
Tx  882.75   Rx  837.75  Chan  0425  #425 
Tx  882.78   Rx  837.78  Chan  0426  #426 
Tx  882.81   Rx  837.81  Chan  0427  #427 
Tx  882.84   Rx  837.84  Chan  0428  #428 
Tx  882.87   Rx  837.87  Chan  0429  #429 
Tx  882.90   Rx  837.90  Chan  0430  #430 
Tx  882.93   Rx  837.93  Chan  0431  #431 
Tx  882.96   Rx  837.96  Chan  0432  #432 
Tx  882.99   Rx  837.99  Chan  0433  #433 
Tx  883.02   Rx  838.02  Chan  0434  #434 
Tx  883.05   Rx  838.05  Chan  0435  #435 
Tx  883.08   Rx  838.08  Chan  0436  #436 
Tx  883.11   Rx  838.11  Chan  0437  #437 
Tx  883.14   Rx  838.14  Chan  0438  #438 
Tx  883.17   Rx  838.17  Chan  0439  #439 
Tx  883.20   Rx  838.20  Chan  0440  #440 
Tx  883.23   Rx  838.23  Chan  0441  #441 
Tx  883.26   Rx  838.26  Chan  0442  #442 
Tx  883.29   Rx  838.29  Chan  0443  #443 
Tx  883.32   Rx  838.32  Chan  0444  #444 
Tx  883.35   Rx  838.35  Chan  0445  #445 
Tx  883.38   Rx  838.38  Chan  0446  #446 
Tx  883.41   Rx  838.41  Chan  0447  #447 
Tx  883.44   Rx  838.44  Chan  0448  #448 
Tx  883.47   Rx  838.47  Chan  0449  #449 
Tx  883.50   Rx  838.50  Chan  0450  #450 
Tx  883.53   Rx  838.53  Chan  0451  #451 
Tx  883.56   Rx  838.56  Chan  0452  #452 
Tx  883.59   Rx  838.59  Chan  0453  #453 
Tx  883.62   Rx  838.62  Chan  0454  #454 
Tx  883.65   Rx  838.65  Chan  0455  #455 
Tx  883.68   Rx  838.68  Chan  0456  #456 
Tx  883.71   Rx  838.71  Chan  0457  #457 
Tx  883.74   Rx  838.74  Chan  0458  #458 
Tx  883.77   Rx  838.77  Chan  0459  #459 
Tx  883.80   Rx  838.80  Chan  0460  #460 
Tx  883.83   Rx  838.83  Chan  0461  #461 
Tx  883.86   Rx  838.86  Chan  0462  #462 
Tx  883.89   Rx  838.89  Chan  0463  #463 
Tx  883.92   Rx  838.92  Chan  0464  #464 
Tx  883.95   Rx  838.95  Chan  0465  #465 
Tx  883.98   Rx  838.98  Chan  0466  #466 
Tx  884.01   Rx  839.01  Chan  0467  #467 
Tx  884.04   Rx  839.04  Chan  0468  #468 
Tx  884.07   Rx  839.07  Chan  0469  #469 
Tx  884.10   Rx  839.10  Chan  0470  #470 
Tx  884.13   Rx  839.13  Chan  0471  #471 
Tx  884.16   Rx  839.16  Chan  0472  #472 
Tx  884.19   Rx  839.19  Chan  0473  #473 
Tx  884.22   Rx  839.22  Chan  0474  #474 
Tx  884.25   Rx  839.25  Chan  0475  #475 
Tx  884.28   Rx  839.28  Chan  0476  #476 
Tx  884.31   Rx  839.31  Chan  0477  #477 
Tx  884.34   Rx  839.34  Chan  0478  #478 
Tx  884.37   Rx  839.37  Chan  0479  #479 
Tx  884.40   Rx  839.40  Chan  0480  #480 
Tx  884.43   Rx  839.43  Chan  0481  #481 
Tx  884.46   Rx  839.46  Chan  0482  #482 
Tx  884.49   Rx  839.49  Chan  0483  #483 
Tx  884.52   Rx  839.52  Chan  0484  #484 
Tx  884.55   Rx  839.55  Chan  0485  #485 
Tx  884.58   Rx  839.58  Chan  0486  #486 
Tx  884.61   Rx  839.61  Chan  0487  #487 
Tx  884.64   Rx  839.64  Chan  0488  #488 
Tx  884.67   Rx  839.67  Chan  0489  #489 
Tx  884.70   Rx  839.70  Chan  0490  #490 
Tx  884.73   Rx  839.73  Chan  0491  #491 
Tx  884.76   Rx  839.76  Chan  0492  #492 
Tx  884.79   Rx  839.79  Chan  0493  #493 
Tx  884.82   Rx  839.82  Chan  0494  #494 
Tx  884.85   Rx  839.85  Chan  0495  #495 
Tx  884.88   Rx  839.88  Chan  0496  #496 
Tx  884.91   Rx  839.91  Chan  0497  #497 
Tx  884.94   Rx  839.94  Chan  0498  #498 
Tx  884.97   Rx  839.97  Chan  0499  #499 
Tx  885.00   Rx  840.00  Chan  0500  #500 
Tx  885.03   Rx  840.03  Chan  0501  #501 
Tx  885.06   Rx  840.06  Chan  0502  #502 
Tx  885.09   Rx  840.09  Chan  0503  #503 
Tx  885.12   Rx  840.12  Chan  0504  #504 
Tx  885.15   Rx  840.15  Chan  0505  #505 
Tx  885.18   Rx  840.18  Chan  0506  #506 
Tx  885.21   Rx  840.21  Chan  0507  #507 
Tx  885.24   Rx  840.24  Chan  0508  #508 
Tx  885.27   Rx  840.27  Chan  0509  #509 
Tx  885.30   Rx  840.30  Chan  0510  #510 
Tx  885.33   Rx  840.33  Chan  0511  #511 
Tx  885.36   Rx  840.36  Chan  0512  #512 
Tx  885.39   Rx  840.39  Chan  0513  #513 
Tx  885.42   Rx  840.42  Chan  0514  #514 
Tx  885.45   Rx  840.45  Chan  0515  #515 
Tx  885.48   Rx  840.48  Chan  0516  #516 
Tx  885.51   Rx  840.51  Chan  0517  #517 
Tx  885.54   Rx  840.54  Chan  0518  #518 
Tx  885.57   Rx  840.57  Chan  0519  #519 
Tx  885.60   Rx  840.60  Chan  0520  #520 
Tx  885.63   Rx  840.63  Chan  0521  #521 
Tx  885.66   Rx  840.66  Chan  0522  #522 
Tx  885.69   Rx  840.69  Chan  0523  #523 
Tx  885.72   Rx  840.72  Chan  0524  #524 
Tx  885.75   Rx  840.75  Chan  0525  #525 
Tx  885.78   Rx  840.78  Chan  0526  #526 
Tx  885.81   Rx  840.81  Chan  0527  #527 
Tx  885.84   Rx  840.84  Chan  0528  #528 
Tx  885.87   Rx  840.87  Chan  0529  #529 
Tx  885.90   Rx  840.90  Chan  0530  #530 
Tx  885.93   Rx  840.93  Chan  0531  #531 
Tx  885.96   Rx  840.96  Chan  0532  #532 
Tx  885.99   Rx  840.99  Chan  0533  #533 
Tx  886.02   Rx  841.02  Chan  0534  #534 
Tx  886.05   Rx  841.05  Chan  0535  #535 
Tx  886.08   Rx  841.08  Chan  0536  #536 
Tx  886.11   Rx  841.11  Chan  0537  #537 
Tx  886.14   Rx  841.14  Chan  0538  #538 
Tx  886.17   Rx  841.17  Chan  0539  #539 
Tx  886.20   Rx  841.20  Chan  0540  #540 
Tx  886.23   Rx  841.23  Chan  0541  #541 
Tx  886.26   Rx  841.26  Chan  0542  #542 
Tx  886.29   Rx  841.29  Chan  0543  #543 
Tx  886.32   Rx  841.32  Chan  0544  #544 
Tx  886.35   Rx  841.35  Chan  0545  #545 
Tx  886.38   Rx  841.38  Chan  0546  #546 
Tx  886.41   Rx  841.41  Chan  0547  #547 
Tx  886.44   Rx  841.44  Chan  0548  #548 
Tx  886.47   Rx  841.47  Chan  0549  #549 
Tx  886.50   Rx  841.50  Chan  0550  #550 
Tx  886.53   Rx  841.53  Chan  0551  #551 
Tx  886.56   Rx  841.56  Chan  0552  #552 
Tx  886.59   Rx  841.59  Chan  0553  #553 
Tx  886.62   Rx  841.62  Chan  0554  #554 
Tx  886.65   Rx  841.65  Chan  0555  #555 
Tx  886.68   Rx  841.68  Chan  0556  #556 
Tx  886.71   Rx  841.71  Chan  0557  #557 
Tx  886.74   Rx  841.74  Chan  0558  #558 
Tx  886.77   Rx  841.77  Chan  0559  #559 
Tx  886.80   Rx  841.80  Chan  0560  #560 
Tx  886.83   Rx  841.83  Chan  0561  #561 
Tx  886.86   Rx  841.86  Chan  0562  #562 
Tx  886.89   Rx  841.89  Chan  0563  #563 
Tx  886.92   Rx  841.92  Chan  0564  #564 
Tx  886.95   Rx  841.95  Chan  0565  #565 
Tx  886.98   Rx  841.98  Chan  0566  #566 
Tx  887.01   Rx  842.01  Chan  0567  #567 
Tx  887.04   Rx  842.04  Chan  0568  #568 
Tx  887.07   Rx  842.07  Chan  0569  #569 
Tx  887.10   Rx  842.10  Chan  0570  #570 
Tx  887.13   Rx  842.13  Chan  0571  #571 
Tx  887.16   Rx  842.16  Chan  0572  #572 
Tx  887.19   Rx  842.19  Chan  0573  #573 
Tx  887.22   Rx  842.22  Chan  0574  #574 
Tx  887.25   Rx  842.25  Chan  0575  #575 
Tx  887.28   Rx  842.28  Chan  0576  #576 
Tx  887.31   Rx  842.31  Chan  0577  #577 
Tx  887.34   Rx  842.34  Chan  0578  #578 
Tx  887.37   Rx  842.37  Chan  0579  #579 
Tx  887.40   Rx  842.40  Chan  0580  #580 
Tx  887.43   Rx  842.43  Chan  0581  #581 
Tx  887.46   Rx  842.46  Chan  0582  #582 
Tx  887.49   Rx  842.49  Chan  0583  #583 
Tx  887.52   Rx  842.52  Chan  0584  #584 
Tx  887.55   Rx  842.55  Chan  0585  #585 
Tx  887.58   Rx  842.58  Chan  0586  #586 
Tx  887.61   Rx  842.61  Chan  0587  #587 
Tx  887.64   Rx  842.64  Chan  0588  #588 
Tx  887.67   Rx  842.67  Chan  0589  #589 
Tx  887.70   Rx  842.70  Chan  0590  #590 
Tx  887.73   Rx  842.73  Chan  0591  #591 
Tx  887.76   Rx  842.76  Chan  0592  #592 
Tx  887.79   Rx  842.79  Chan  0593  #593 
Tx  887.82   Rx  842.82  Chan  0594  #594 
Tx  887.85   Rx  842.85  Chan  0595  #595 
Tx  887.88   Rx  842.88  Chan  0596  #596 
Tx  887.91   Rx  842.91  Chan  0597  #597 
Tx  887.94   Rx  842.94  Chan  0598  #598 
Tx  887.97   Rx  842.97  Chan  0599  #599 
Tx  888.00   Rx  843.00  Chan  0600  #600 
Tx  888.03   Rx  843.03  Chan  0601  #601 
Tx  888.06   Rx  843.06  Chan  0602  #602 
Tx  888.09   Rx  843.09  Chan  0603  #603 
Tx  888.12   Rx  843.12  Chan  0604  #604 
Tx  888.15   Rx  843.15  Chan  0605  #605 
Tx  888.18   Rx  843.18  Chan  0606  #606 
Tx  888.21   Rx  843.21  Chan  0607  #607 
Tx  888.24   Rx  843.24  Chan  0608  #608 
Tx  888.27   Rx  843.27  Chan  0609  #609 
Tx  888.30   Rx  843.30  Chan  0610  #610 
Tx  888.33   Rx  843.33  Chan  0611  #611 
Tx  888.36   Rx  843.36  Chan  0612  #612 
Tx  888.39   Rx  843.39  Chan  0613  #613 
Tx  888.42   Rx  843.42  Chan  0614  #614 
Tx  888.45   Rx  843.45  Chan  0615  #615 
Tx  888.48   Rx  843.48  Chan  0616  #616 
Tx  888.51   Rx  843.51  Chan  0617  #617 
Tx  888.54   Rx  843.54  Chan  0618  #618 
Tx  888.57   Rx  843.57  Chan  0619  #619 
Tx  888.60   Rx  843.60  Chan  0620  #620 
Tx  888.63   Rx  843.63  Chan  0621  #621 
Tx  888.66   Rx  843.66  Chan  0622  #622 
Tx  888.69   Rx  843.69  Chan  0623  #623 
Tx  888.72   Rx  843.72  Chan  0624  #624 
Tx  888.75   Rx  843.75  Chan  0625  #625 
Tx  888.78   Rx  843.78  Chan  0626  #626 
Tx  888.81   Rx  843.81  Chan  0627  #627 
Tx  888.84   Rx  843.84  Chan  0628  #628 
Tx  888.87   Rx  843.87  Chan  0629  #629 
Tx  888.90   Rx  843.90  Chan  0630  #630 
Tx  888.93   Rx  843.93  Chan  0631  #631 
Tx  888.96   Rx  843.96  Chan  0632  #632 
Tx  888.99   Rx  843.99  Chan  0633  #633 
Tx  889.02   Rx  844.02  Chan  0634  #634 
Tx  889.05   Rx  844.05  Chan  0635  #635 
Tx  889.08   Rx  844.08  Chan  0636  #636 
Tx  889.11   Rx  844.11  Chan  0637  #637 
Tx  889.14   Rx  844.14  Chan  0638  #638 
Tx  889.17   Rx  844.17  Chan  0639  #639 
Tx  889.20   Rx  844.20  Chan  0640  #640 
Tx  889.23   Rx  844.23  Chan  0641  #641 
Tx  889.26   Rx  844.26  Chan  0642  #642 
Tx  889.29   Rx  844.29  Chan  0643  #643 
Tx  889.32   Rx  844.32  Chan  0644  #644 
Tx  889.35   Rx  844.35  Chan  0645  #645 
Tx  889.38   Rx  844.38  Chan  0646  #646 
Tx  889.41   Rx  844.41  Chan  0647  #647 
Tx  889.44   Rx  844.44  Chan  0648  #648 
Tx  889.47   Rx  844.47  Chan  0649  #649 
Tx  889.50   Rx  844.50  Chan  0650  #650 
Tx  889.53   Rx  844.53  Chan  0651  #651 
Tx  889.56   Rx  844.56  Chan  0652  #652 
Tx  889.59   Rx  844.59  Chan  0653  #653 
Tx  889.62   Rx  844.62  Chan  0654  #654 
Tx  889.65   Rx  844.65  Chan  0655  #655 
Tx  889.68   Rx  844.68  Chan  0656  #656 
Tx  889.71   Rx  844.71  Chan  0657  #657 
Tx  889.74   Rx  844.74  Chan  0658  #658 
Tx  889.77   Rx  844.77  Chan  0659  #659 
Tx  889.80   Rx  844.80  Chan  0660  #660 
Tx  889.83   Rx  844.83  Chan  0661  #661 
Tx  889.86   Rx  844.86  Chan  0662  #662 
Tx  889.89   Rx  844.89  Chan  0663  #663 
Tx  889.92   Rx  844.92  Chan  0664  #664 
Tx  889.95   Rx  844.95  Chan  0665  #665 
Tx  889.98   Rx  844.98  Chan  0666  #666 
 
Upper Set Part 1 (667-799) 
 
Tower Freq.  Mobile Freq.    11xxxx# Channel 
 
Tx  890.01   Rx  845.01  Chan  0667  #667 
Tx  890.04   Rx  845.04  Chan  0668  #668 
Tx  890.07   Rx  845.07  Chan  0669  #669 
Tx  890.10   Rx  845.10  Chan  0670  #670 
Tx  890.13   Rx  845.13  Chan  0671  #671 
Tx  890.16   Rx  845.16  Chan  0672  #672 
Tx  890.19   Rx  845.19  Chan  0673  #673 
Tx  890.22   Rx  845.22  Chan  0674  #674 
Tx  890.25   Rx  845.25  Chan  0675  #675 
Tx  890.28   Rx  845.28  Chan  0676  #676 
Tx  890.31   Rx  845.31  Chan  0677  #677 
Tx  890.34   Rx  845.34  Chan  0678  #678 
Tx  890.37   Rx  845.37  Chan  0679  #679 
Tx  890.40   Rx  845.40  Chan  0680  #680 
Tx  890.43   Rx  845.43  Chan  0681  #681 
Tx  890.46   Rx  845.46  Chan  0682  #682 
Tx  890.49   Rx  845.49  Chan  0683  #683 
Tx  890.52   Rx  845.52  Chan  0684  #684 
Tx  890.55   Rx  845.55  Chan  0685  #685 
Tx  890.58   Rx  845.58  Chan  0686  #686 
Tx  890.61   Rx  845.61  Chan  0687  #687 
Tx  890.64   Rx  845.64  Chan  0688  #688 
Tx  890.67   Rx  845.67  Chan  0689  #689 
Tx  890.70   Rx  845.70  Chan  0690  #690 
Tx  890.73   Rx  845.73  Chan  0691  #691 
Tx  890.76   Rx  845.76  Chan  0692  #692 
Tx  890.79   Rx  845.79  Chan  0693  #693 
Tx  890.82   Rx  845.82  Chan  0694  #694 
Tx  890.85   Rx  845.85  Chan  0695  #695 
Tx  890.88   Rx  845.88  Chan  0696  #696 
Tx  890.91   Rx  845.91  Chan  0697  #697 
Tx  890.94   Rx  845.94  Chan  0698  #698 
Tx  890.97   Rx  845.97  Chan  0699  #699 
Tx  891.00   Rx  846.00  Chan  0700  #700 
Tx  891.03   Rx  846.03  Chan  0701  #701 
Tx  891.06   Rx  846.06  Chan  0702  #702 
Tx  891.09   Rx  846.09  Chan  0703  #703 
Tx  891.12   Rx  846.12  Chan  0704  #704 
Tx  891.15   Rx  846.15  Chan  0705  #705 
Tx  891.18   Rx  846.18  Chan  0706  #706 
Tx  891.21   Rx  846.21  Chan  0707  #707 
Tx  891.24   Rx  846.24  Chan  0708  #708 
Tx  891.27   Rx  846.27  Chan  0709  #709 
Tx  891.30   Rx  846.30  Chan  0710  #710 
Tx  891.33   Rx  846.33  Chan  0711  #711 
Tx  891.36   Rx  846.36  Chan  0712  #712 
Tx  891.39   Rx  846.39  Chan  0713  #713 
Tx  891.42   Rx  846.42  Chan  0714  #714 
Tx  891.45   Rx  846.45  Chan  0715  #715 
Tx  891.48   Rx  846.48  Chan  0716  #716 
Tx  891.51   Rx  846.51  Chan  0717  #717 
Tx  891.54   Rx  846.54  Chan  0718  #718 
Tx  891.57   Rx  846.57  Chan  0719  #719 
Tx  891.60   Rx  846.60  Chan  0720  #720 
Tx  891.63   Rx  846.63  Chan  0721  #721 
Tx  891.66   Rx  846.66  Chan  0722  #722 
Tx  891.69   Rx  846.69  Chan  0723  #723 
Tx  891.72   Rx  846.72  Chan  0724  #724 
Tx  891.75   Rx  846.75  Chan  0725  #725 
Tx  891.78   Rx  846.78  Chan  0726  #726 
Tx  891.81   Rx  846.81  Chan  0727  #727 
Tx  891.84   Rx  846.84  Chan  0728  #728 
Tx  891.87   Rx  846.87  Chan  0729  #729 
Tx  891.90   Rx  846.90  Chan  0730  #730 
Tx  891.93   Rx  846.93  Chan  0731  #731 
Tx  891.96   Rx  846.96  Chan  0732  #732 
Tx  891.99   Rx  846.99  Chan  0733  #733 
Tx  892.02   Rx  847.02  Chan  0734  #734 
Tx  892.05   Rx  847.05  Chan  0735  #735 
Tx  892.08   Rx  847.08  Chan  0736  #736 
Tx  892.11   Rx  847.11  Chan  0737  #737 
Tx  892.14   Rx  847.14  Chan  0738  #738 
Tx  892.17   Rx  847.17  Chan  0739  #739 
Tx  892.20   Rx  847.20  Chan  0740  #740 
Tx  892.23   Rx  847.23  Chan  0741  #741 
Tx  892.26   Rx  847.26  Chan  0742  #742 
Tx  892.29   Rx  847.29  Chan  0743  #743 
Tx  892.32   Rx  847.32  Chan  0744  #744 
Tx  892.35   Rx  847.35  Chan  0745  #745 
Tx  892.38   Rx  847.38  Chan  0746  #746 
Tx  892.41   Rx  847.41  Chan  0747  #747 
Tx  892.44   Rx  847.44  Chan  0748  #748 
Tx  892.47   Rx  847.47  Chan  0749  #749 
Tx  892.50   Rx  847.50  Chan  0750  #750 
Tx  892.53   Rx  847.53  Chan  0751  #751 
Tx  892.56   Rx  847.56  Chan  0752  #752 
Tx  892.59   Rx  847.59  Chan  0753  #753 
Tx  892.62   Rx  847.62  Chan  0754  #754 
Tx  892.65   Rx  847.65  Chan  0755  #755 
Tx  892.68   Rx  847.68  Chan  0756  #756 
Tx  892.71   Rx  847.71  Chan  0757  #757 
Tx  892.74   Rx  847.74  Chan  0758  #758 
Tx  892.77   Rx  847.77  Chan  0759  #759 
Tx  892.80   Rx  847.80  Chan  0760  #760 
Tx  892.83   Rx  847.83  Chan  0761  #761 
Tx  892.86   Rx  847.86  Chan  0762  #762 
Tx  892.89   Rx  847.89  Chan  0763  #763 
Tx  892.92   Rx  847.92  Chan  0764  #764 
Tx  892.95   Rx  847.95  Chan  0765  #765 
Tx  892.98   Rx  847.98  Chan  0766  #766 
Tx  893.01   Rx  848.01  Chan  0767  #767 
Tx  893.04   Rx  848.04  Chan  0768  #768 
Tx  893.07   Rx  848.07  Chan  0769  #769 
Tx  893.10   Rx  848.10  Chan  0770  #770 
Tx  893.13   Rx  848.13  Chan  0771  #771 
Tx  893.16   Rx  848.16  Chan  0772  #772 
Tx  893.19   Rx  848.19  Chan  0773  #773 
Tx  893.22   Rx  848.22  Chan  0774  #774 
Tx  893.25   Rx  848.25  Chan  0775  #775 
Tx  893.28   Rx  848.28  Chan  0776  #776 
Tx  893.31   Rx  848.31  Chan  0777  #777 
Tx  893.34   Rx  848.34  Chan  0778  #778 
Tx  893.37   Rx  848.37  Chan  0779  #779 
Tx  893.40   Rx  848.40  Chan  0780  #780 
Tx  893.43   Rx  848.43  Chan  0781  #781 
Tx  893.46   Rx  848.46  Chan  0782  #782 
Tx  893.49   Rx  848.49  Chan  0783  #783 
Tx  893.52   Rx  848.52  Chan  0784  #784 
Tx  893.55   Rx  848.55  Chan  0785  #785 
Tx  893.58   Rx  848.58  Chan  0786  #786 
Tx  893.61   Rx  848.61  Chan  0787  #787 
Tx  893.64   Rx  848.64  Chan  0788  #788 
Tx  893.67   Rx  848.67  Chan  0789  #789 
Tx  893.70   Rx  848.70  Chan  0790  #790 
Tx  893.73   Rx  848.73  Chan  0791  #791 
Tx  893.76   Rx  848.76  Chan  0792  #792 
Tx  893.79   Rx  848.79  Chan  0793  #793 
Tx  893.82   Rx  848.82  Chan  0794  #794 
Tx  893.85   Rx  848.85  Chan  0795  #795 
Tx  893.88   Rx  848.88  Chan  0796  #796 
Tx  893.91   Rx  848.91  Chan  0797  #797 
Tx  893.94   Rx  848.94  Chan  0798  #798 
Tx  893.97   Rx  848.97  Chan  0799  #799 
 
Upper Set Part 2 (991-1023) 
 
Tower Freq.  Mobile Freq.    11xxxx# Channel 
 
Tx  869.04   Rx  824.04  Chan  0991  #800 
Tx  869.07   Rx  824.07  Chan  0992  #801 
Tx  869.10   Rx  824.10  Chan  0993  #802 
Tx  869.13   Rx  824.13  Chan  0994  #803 
Tx  869.16   Rx  824.16  Chan  0995  #804 
Tx  869.19   Rx  824.19  Chan  0996  #805 
Tx  869.22   Rx  824.22  Chan  0997  #806 
Tx  869.25   Rx  824.25  Chan  0998  #807 
Tx  869.28   Rx  824.28  Chan  0999  #808 
Tx  869.31   Rx  824.31  Chan  1000  #809 
Tx  869.34   Rx  824.34  Chan  1001  #810 
Tx  869.37   Rx  824.37  Chan  1002  #811 
Tx  869.40   Rx  824.40  Chan  1003  #812 
Tx  869.43   Rx  824.43  Chan  1004  #813 
Tx  869.46   Rx  824.46  Chan  1005  #814 
Tx  869.49   Rx  824.49  Chan  1006  #815 
Tx  869.52   Rx  824.52  Chan  1007  #816 
Tx  869.55   Rx  824.55  Chan  1008  #817 
Tx  869.58   Rx  824.58  Chan  1009  #818 
Tx  869.61   Rx  824.61  Chan  1010  #819 
Tx  869.64   Rx  824.64  Chan  1011  #820 
Tx  869.67   Rx  824.67  Chan  1012  #821 
Tx  869.70   Rx  824.70  Chan  1013  #822 
Tx  869.73   Rx  824.73  Chan  1014  #823 
Tx  869.76   Rx  824.76  Chan  1015  #824 
Tx  869.79   Rx  824.79  Chan  1016  #825 
Tx  869.82   Rx  824.82  Chan  1017  #826 
Tx  869.85   Rx  824.85  Chan  1018  #827 
Tx  869.88   Rx  824.88  Chan  1019  #828 
Tx  869.91   Rx  824.91  Chan  1020  #829 
Tx  869.94   Rx  824.94  Chan  1021  #830 
Tx  869.97   Rx  824.97  Chan  1022  #831 
Tx  870.00   Rx  825.00  Chan  1023  #832 
 
---------------------------------------------------------------------------- 
I got this from a bbs in the (708) are code.  It had no name associated 
with it.  Since NOONE has mailed me any other info on it, I will keep this 
in the bible until someone bitches or sends me something tangible. 
                                                                -ML 
 
                              MOTOROLA "TRIK-CLIP" 
 
 
This is the plans I recieved for the Flip.  Supposedly if one knew the 
pinouts on the other moto phones one could transpose. (maybe!)  I never 
tested this so I don't know if it works.  The chip in the flip the text 
is talking about is a 32 pin square plcc 
 
After Phone Disassembly Locate 27c512 Eprom on phone board.  This is 
On The Upper Right Side Of The Display Next To The Roam Indicator. 
This Is a 32 pin Square device.  **Note the dot and beveled edge 
for pin orientation (the dot is pin 1) Count to the left 
counter clock wise 2 3 4 5 and so on.  To the Right or clockwise 
of the dot is pin 32 Vcc.  This will aid you in your count to find 
pin 25 which is the eprom output enable.  This pin is at ground or 
Vss - Level.  **Note Pin 25 on Eprom in phone must be lifted from 
the phone board ground or Vss state.  Use an X-acto Knife and or 
soldering iron and tools to cut pin at board level where pin 
narrows.  Do not bend wide part of pin up on eprom as this could 
break off of Eprom.  Also Wide Part of pin Will be used to make 
contact with eprom test clip adapter.  The eprom test clip adapter 
will take pin 25 to logic high through an 8 to 10 thousand 
resistor to pin 32 Vcc.  This will Gate off all data Commands from 
the phone board eprom and allow the eprom test clip adaptor to 
take over.  **Note test clip could touch narrow part of cut off 
pin on board and cause phone not to power up please remove or fold 
down as low as possible so test clip only touches side of eprom. 
 
After programing is complete put pin 25 back together or find a 
suitable ground or Vss - source.  The phone will power up and work 
without pin 25 put back together but for long term precaution 
put back to a logic zero or ground to enable the output enable. 
 
To use the eprom test clip adapter pull the locking wedge on the 
test clip into the upper postition.  Seat the eprom test clip adapter 
onto the eprom in the phone.  Make sure to orient the dot and 
beveled edge with each other.  Push the locking wedge down to lock 
the the eprom test clip adapter onto the eprom in the phone.  Hook up 
the programing cable to the computer and plug into the jack on the 
base of the phone.  Also hook up the loose lead with a jumper to the 
center terminal between the battery contacts.  Turn power on green 
light on phone display should come on thgen a complete display test 
will light up after that the no service will blink along with the 
signal level mark in corner of display.  If the antenna is still on 
the phone it could change to roam or something else.  I  suggest 
remove the antenna so the cell sight will not see you.  If you do 
not get a power on test with the display there are 3 possible 
things (1) pin 25 on phone board is touching the test clip this 
can be checked by looking with a volt meter at pin 25 where 
resistor connects for 4 to 5 volts pos with reference to ground. 
(2) Test clip is not sitting on chip good some times you have pull 
the test clip up off of the eprom a 64th of an inch all the way 
around.  (3) there is corrupt data, Pull the eprom test clip off 
Phone check to see if power on display is there. 
 
Computer see if data or phone number or cell sight code or data 
whole is ok I've seen the cell sight ID corrrupt and the phone play 
dead on  the power on test. The test clip sometimes needs 
maintenance look at the gold pins. 
 
Make sure all the pins are level with the edge of it.  If not take 
an X-acto or pin and lightly bend them out so they are along the 
edge of the plastic of the test clip. 
 
Always check to see if eprom in phone contacts are clean before 
putting test clip on.  **Note when test clip is on phone - only 
change the ESN only. *The other data phone number lock and so on 
can be changed without the test clip and and should be done so. 
 
The software version in the test clip is 9148 you will see this in 
the right corner of the computer.  Sometimes the program will crash 
during the ESN wright this will put all zeros in the ESN field 
check the test clip try again.  Sometimes I've had to do this 3 an 4 
times.  Also watch the phone display for codes I've seen at the end 
of a wright the code (FO8) just before power down I've had no 
problem there but during the key wright (FO8) means i've crashed. 
 
Also during the time when the program is counting back into the 
phone i've had (F1O) show up in the display of the phone this 
problem means the next time you may not get the power on display 
test pull test clip read phone check data to see if cell sight 
code is corrupt or some other data correct try again.  A word of 
caution do not push on eprom on top of test clip as this could 
seat eprom lower into adapter and cause bad contact.  To remove 
test clip pull locking wedge up to unlock the eprom test clip 
adapter from the eprom in the phone.  Continue pulling up to lift 
the eprom test clip adapter from the eprom in the phone. 
 
----------------------------------------------------------------------------- 
 
DISCLAIMER:  I, Mike Larsen, accept NO responsibility for people using any 
info within this text for fraudulant purposes.  I did not intend for the info 
to be used towards fraud or theft of services.  The main reason I spent  
hundreds of hours creating and compiling this information is because  
programming fees are BULLSHIT and they know it.  If you notice, the 37# 
command is no longer a mystery and Motorola is quite pissed I found out.  I 
"engineered" it from a floor manager or some other head at the Motorola  
cellular division.  "Big Deal" you say.  Well, Motorola shipped Many flip 
fones with that command set for a different battery.  After 10 minutes of use 
the phone would die.  The phone had to be sent to Motorola to be "fixed." 
        If you found this text useful, please mail something interesting or 
just let me know you appreciated my efforts.  You can't believe how pissed 
I was when I found out some lamer is changing the name in the text to his 
own so people will like him or something.  Have fun. 
 
Oh, by the way, I forgot to mention in the above disclaimer that I do 
nothing fraudulant with MY fone.  I pay a bill and everything and can prove  
it.  So will the "feds" or whoever the Internet gestapo is that's been sending 
me mail about me being under thier "watchful eye", please go for someone else 
that's dealing child pornography or asking for WaReZ?  Thanks. 
 
 
        Mike.Larsen@uti.com 
        stularsenmic@vax.colsf.edu 
 
------------------------------------------------------------------------------ 
                             -=*( Prophet )*=- 
    ____                   __         __  
   / __ \_________  ____  / /_  ___  / /_   The Truth Is Out There... 
  / /_/ / ___/ __ \/ __ \/ __ \/ _ \/ __/ 
 / ____/ /  / /_/ / /_/ / / / /  __/ /_     Trust No-One... 
/_/   /_/   \____/ .___/_/ /_/\___/\__/   
                /_/                         Do Not Fear The Reaper, 
prophet@illumini.demon.co.uk                Fear Your God-Damn Government 
 
