AUDIOVOX PR 125.

NOTES:   This unit has three NAMS.
         The ESN prefix is 138 decimal, 8A hex (Toshiba)
         Audiovox: 516-231-6051/213-926-7758

NAM PROGRAMING:

1.  Turn on power & within 10 seconds press MUTE 6 2 6 #

2.  The phone will display "NAM PROGRAM"

3.  Enter 7 8 7 1 3 0 0 RCL

4.  The phone will display the ESN in hex format.

5.  Press the UP arrow key.

6.  The phone will display the ESN in decimal format.

7.  Press the UP arrow key to proceed to the first programing step.

8.  The UP arrow key is used to store each entry and increment each step.

9.  The CLR key can be used to correct an entry prior to the UP arrow key
    being pushed.

PROGRAMING DATA:

STEP#    #OF DIGITS/RANGE    DISPLAY     DESCRIPTION

01       10 DIGITS           TEL NO      MIN (AREA CODE & PHONE NUMBER)
02       00000 - 99999       SID         SYSTEM IDENTIFICATION
03       0 OR 1              Local Use   LOCAL USE MARK
04       0 OR 1              Min Mark    MIN MARK
05       0333 OR 0334        IPCH        INITIAL PAGING CHANNEL
06       2 DIGITS            Accolc      ACCESS OVERLOAD CLASS
07       0 OR 1              Prefer Sys  PREFERRED SYSTEM
08       10 OR 15            GIM         GROUP ID (10 IN USA)
09       4 DIGITS            Lock Code   LOCK CODE
10       0 OR 1              End to End  DTMF DIALING
11       0 OR 1              A/B SELECT  SYSTEM SELECT
12       0 OR 1              AREA CODE   DISPLAY AREA CODE
13       0 OR 1              DTX         VOX OPERATION

PHONE WILL DISPLAY "STO OR CLR" AT THIS STAGE, ENTER STO TO CONTINUE
OR CLR TO ABORT.

PHONE WILL THEN DISPLAY "SELECT 1-3", PRESS END TO COMPLETE AND EXIT
PROGRAMING, OR SELECT NAM 2 OR 3.  STEPS 1 THRU 9 WILL REPEAT FOR
NAM 2 AND/OR 3.