EddyHawk's Info List
---
MEMORY MANAGER
---
-HIMEM (HIgh MEMory)
 by: Microsoft
 year: 1988-1995
 type: XMS V3.0 driver
 V3.95 [1995]
 note:
  part of DOS/Win4+
  unreliable when RAM > 64Mb

-EMM386 (Expanded Memory Manager 386)
 by: Microsoft
 year: 1988-1995
 type: LIM/EMS V4.0 driver
 v4.95
 note: requires XMS driver

-QEMM (Quarterdeck Expanded Memory Manager) 386
 By: Dan Spear?/Quarterdeck Corporation (USA)
 Year: 1986-1996
 Type: memory manager, 386, DOS V3.1
 V8.01 [1996]
  (DOS-UP & DOSDATA).SYS
  QDPMI.SYS
   contains DOS Extension Technology [1991-1994] by Ergo Computing
  provides
   both XMS & EMS
   largest free base mem than other EMM
  fast boot
  stealth ROM
   many sw asks to turn off this feature
  Magna RAM: Win3+ memory presor
  EdH: this ver can't malloc more than 64Mb. also apply to all DOS EMM?
 V8.03
 V9.00

-All Charge 386
 V3.1
 prog x name: Allemm4.sys

-HPemm386.sys and HPemm486.sys

-HP
 prog x name: HPmm.sys

-Iemm.sys

-Intel(R) Expanded-Memory Emulator
 prog x name: Ilim386.sys

-Maximizer
 prog x name: Maximize.com

-NetRoom
 prog x name: RM386.sys

-QMAPS
 V5.16

-UMB PRO
 V1.07
---
MEMORY UTILITIES:
---
-MI (Memory Info)
 by: CPS (USA)
 V9.0 [1993]
  more thorough than DOS's MEM & DOS ver independent