Modem Online Diagnostic System
Telstra Corporation

Press to begin Login Session
Connected

Version: MTST_2.02a

Please enter your modem's phone number.
(include area code, eg 0855551234)
=> 0740532859

Telstra does not guarantee Modem and Facsimile Customer
Equipment not conforming to ITU-T recommendations V.18,
V.21, V.27ter or V.34 and data rates greater than 2400 bit/s

Transmitting test data for 6 minutes. Characters sent:
1559352
Please wait, extracting test results...

Modulation V90 digital
Symbol rate (Rx/Tx) 3200/2146
Carriers (Rx/Tx, Hz) 1920/0
Trellis rate (Rx/Tx) 64S-4D/16S-4D
Non-linear encoding (Rx/Tx) ON/OFF
Pre-coding (Rx/Tx) OFF/OFF
Shaping (Rx/Tx) OFF/OFF
Pre-emphasis/Index (Rx/Tx, dB) N/A
Level (Rx/Tx, -dB) 24/12
Near echo loss (dB) 0
Far echo loss (dB) 30
Signal to Noise Ratio (dB) 44
Round trip delay (msec) 50

Initialisation time (msec) N/A
Retrains requested 0
Retrains granted 0
Fallback OFF
Line reversals 0

Connect speed (Rx/Tx, bits/sec) 31200/45333
Line speed (Rx/Tx, bits/sec) 31200/45333
Highest speed (Rx/Tx, bits/sec) 31200/45333
Lowest speed (Rx/Tx, bits/sec) 31200/45333

Error correction V42
Receive block errors 1
Blocks sent 9990
Link NAKs 1
Blocks resent 15

Characters sent 1562377
Octets sent 69196
Characters lost 0
Characters received 12
Octets received 12
Data compression V42bis
Dictionary (size/string) N/A

Channel Probe:
Level +-+ Attn

The test is now complete. For further details call
your Telstra Service Centre.

MOLDS will now disconnect this call.

