
[:]-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-[:]
[:]                                                                       [:]
[:]                         DataMedia 1500 Notes                          [:]
[:]                                                                       [:]
[:]                              Written By:                              [:]
[:]                          FlAsHbAcK WhIpLaSh                           [:]
[:]                                                                       [:]
[:]                    In Association With: The TraxSter                  [:]
[:]                                                                       [:]
[:]-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-[:]
[:] Call These Boardz:                                                    [:]
[:]                                                                       [:]
[:]      The Fourth Dimension..... [305]/792-2024 BBS/AE 2400/1200 20mg   [:]
[:]      The Hotel.................[305]/431-3977 BBS    1200/300  10mg   [:]
[:]                                                      --- The TraxSter [:]
[:]-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
=-=-=-=-=-=-=-=-=-=-=-=-=-=-[:] 

=================
Format 80 columns
=================


Ascii Express/Datamedia 1500 screen control
-------------------------------------------
Written by FlAsHbAcK WhIpLaSh
Formatted in 80 columns

Cursor control:
---------------

   The cursor can be moved through a control character and two following
characters. The format is as follows:

     <CTRL-^(x,y)>

   The (Control (Shift 6)) character must be sent before the codes. The 80
column codes are as follows:

01234567890123456789012345678901234567890123456789012345678901234567890123456
 !"#$%&'()*+,-./0123456789:;<=>?@ABCDEFGHIJKLMNOPQRSTUVWXYZ[\]^_`abcdefghijkl
! 1
" 2          B
# 3
$ 4
% 5
& 6
' 7
( 8
) 9
* 10
+ 11
, 12
- 13
. 14                           A      G
/ 15
0 16                           Q
1 17
2 18
3 19
4 20
5 21
6 22
7 23

 I.e. To get the cursor to point 'A' terminal should recieve: (Ctrl-^?.)
      To get the cursor to point 'G' terminal should recieve: (Ctrl-^F.)
      To get the cursor to point 'Q' terminal should recieve: (Ctrl-^?0)
      To get the cursor to point 'B' terminal should recieve: (Ctrl-^-")

     Capitals and other forms of letters are VERY IMPORTANT.

Text Management:
----------------

For Inverse text: Ctrl-O
For Normal text : Ctrl-N
Flashing: Non existant

To Clear Screen: Ctrl-L
To Clear screen BELOW cursor: Ctrl-K
Send cursor to top of screen: Ctrl-Y
Clear line that cursor is on: Ctrl-Z


More coming soon,

Call: The Fourth Dimension [305] - /792/-\2024\

FlAsHbAcK WhIpLaSh



[B]y [T]he [W]ay: [BTW]:

         About the boards listed at the top...

         [/ The Fourth Dimension /]  is going 60 megs, and 9600/17.4k baud.  Now supporting IIgs/IIe warez.
         [/ The Hotel /] will hopefully be going to a transfer system and is going 20 or 30 megs.

                   Just A little Note From:

                                                 - The TraxSter -

See ya later...

JAMMIN'
