
Pacific Bell Computer Systems
=============================
Brought to you by Another Hacker
(^) The *Elite* Phreaker's Group (^)

Telephone Numbers For Pactime-A Computer (Logon instructions are at the end)

AREA		    TERMINAL		   TEL NUMBER	   TEL NUMBER
					   FIRST CHOICE       IF BUSY
------------------------------------------------------------------------

Los Angeles
300 Baud				 213-277-7698	     213-277-7942
1200 Baud (202S)			 213-557-0427	     213-553-4721
1200 Baud (212A)			 213-557-3639	     213-277-0668
110/300/1200 Baud(AUTO) 		 213-203-8120	     213-277-7942

Newport Beach
300 Baud				 714-752-4991	     714-752-4971
1200 Baud (212A)			 714-752-2036	     714-851-0261

Reno
300 Baud				 702-329-8417	     702-324-7829

Sacramento
300 Baud				 916-972-0300	     916-971-1881
1200 Baud (202S)			 916-972-1133	     ------------
1200 Baud (212A)			 916-972-0415	     ------------
1200 Baud (212A)			 916-972-0416	     916-971-1881

San Diego
300 Baud				 619-230-8613	     714-297-9260
1200 Baud (212A)			 619-230-8659	     714-297-6901
110/300/1200 Baud(AUTO) 		 619-230-8647	     ------------

San Francisco
300 Baud				 415-433-7950	     415-788-6800
1200 Baud (212A)			 415-433-7526	     415-986-5222
110/300/1200 Baud(AUTO) 		 415-397-7597	     ------------

Concord
110/300/1200 Baud(AUTO) 		 415-827-9365	     ------------
1200 Baud (202S)			 415-827-9384	     415-391-5656
1200 Baud (212A)			 415-827-0923	     ------------

San Jose
300 Baud				 408-280-6380	     408-245-6051
1200 Baud (202S)			 408-280-6376	     408-732-9791
1200 Baud (212A)			 408-280-6366	     408-245-6051
110/300/1200 Baud(AUTO) 		 408-297-3020	     ------------

Note - 1200 Full duplex uses 212A data sets while half duplex uses 202S data
       sets.

Note - Autobaud - Automatic selection of baud rate.  212A data set required for
       1200 baud.

How to log on to pactime-A
1.  At 300 baud type the letter O and a carriage return (CR).  At 1200 baud
    type the character "^" 5 or 6 times in a row then hit the carriage return.

2.  The computer will respond: CSS ONLINE -- PTTS

3.  Type:  L PTTS userid (CR) That is type the letter L a space your userid and
    then hit the carriage return button.

4.  The computer will then ask for your password.  Type the password in the
    blacked out area.

5.  The computer will then ask for A/C info.  Answer as directed by your
    department.

6.  The log on procedure is now completed.

Pacific Bell Computers brought to you by

%%%%> Another Hacker <%%%%
[/The *Elite* Phreaker's Group\]
Call The Works BBS - 1600+ Textfiles! - [914]/238-8195 - 300/1200 - Always Open

[BROUGHT TO AUCKLAND, NEW ZEALAND COURTESY OF THE BANANA REPUBLIC BBS]
 by Arnold Schwarzenegger
