N


Public Message 
Message # 3951 *MM1 TECH Echo*
To      : Colin Mckay
From    : Warren Hrach
Subject : Re: UUCP works
Date    : 94/04/17 12:21:03
Previous Reply is Message 3945   

              On Friday, April 15th, 1994 - Colin Mckay wrote:
 
CM> You know what your tsmon problem sounds like? It sounds like you're 
CM> being  bitten by the serial port bug in /t0.
CM> Try using /t3 or /t4, and see if you have the same problem. You could 
CM> also try 
CM> running Guardian.
CM> I don't think the stock TSMON logs callers. You'd have to get Carl 
CM> Kreider's  MTSMON package. It has caller logging, as I recall.
CM> @c=*X-m?zN,-f-x5**E r
 
Colin,
      I posted a prev. msg. to All that explained what I found.
Basically init the modem to ATQ1 (result codes off).  Now it works fine
with /t0, no gardian and now will try mtsmon.  Also need to find out how 
to trip DTR to hang up the modem. As it is now the caller has to hang
up.
-Warren
 
--- RiBBS v2.10        
 * Origin: Ocean Beach BBS 619-224-4878 MM1 TECH moderator (1:202/343)


Public Message (Rec)
Message # 3953 *MM1 TECH Echo*
To      : Alan Weston
From    : James Jones
Subject : dial.sys contents
Date    : 94/04/17 12:59:11
Next Reply is Message 4070

OK...here's my dial.sys file (aside from my putting a space at the
beginning of each line, to try to avoid RiBBS reformatting it):
 
 Ocean Beach (14.4K);16192244878;DT*70,;38400;8N1;YES
 Delphi (2400);2886206;DT*70,;38400;8N1;YES
 Delphi (9600);2884626;DT*70,;38400;8N1;YES
 ACS Inc. BBS;14046362991;DT*70,;38400;8N1;YES
 
(There are another couple of lines, but this should give you the idea.)
I say they're all 38400 bps because the modem is set up to always
communicate with me at 38.4 no matter what the far end uses, and the
*70, is there to kill call waiting.  With this setup, ladial seems to
pause part way through dialing a number, and then the rest of the number 
is echoed followed immediately by "NO DIALTONE."
 
--- RiBBS v2.10        
 * Origin: Ocean Beach BBS 619-224-4878 MM1 TECH moderator (1:202/343)


Public Message 
Message # 4060 *MM1 TECH Echo*
To      : James Jones
From    : Colin Mckay
Subject : Re: Time Change 
Date    : 94/04/18  17:01:00

JJ> What do people in the states or regions (without Daylight Savings Time)

Curse the clock manufacturer twice a year, I guess!

I'd imagine that they could:

   1. Hunt for a new clock chip.
   2. Set up a CRON entry to run a program to fix the time by
      an hour twice a year.
   3. Manually reset the clock twice a year.

TTYL. Colin.


--- Maximus-CBCS v1.02
 * Origin: Micro80 Computer Club of Ottawa BBS (1:163/306)


Public Message 
Message # 4061 *MM1 TECH Echo*
To      : Warren Hrach
From    : Colin Mckay
Subject : UUCP
Date    : 94/04/19  14:13:00

Warren,

What is your non-Fido Internet address (if you have one).

TTYL. Colin.
cmckay@northx.isis.org


--- Maximus-CBCS v1.02
 * Origin: Micro80 Computer Club of Ottawa BBS (1:163/306)


Public Message 
Message # 4070 *MM1 TECH Echo*
To      : James Jones
From    : Alan Weston
Subject : Re: dial.sys contents
Date    : 94/04/21 10:35:55
Previous Reply is Message 3953   

              On Sunday, April 17th, 1994 - James Jones wrote:
 
JJ> OK...here's my dial.sys file (aside from my putting a space at the
JJ> beginning of each line, to try to avoid RiBBS reformatting it):
JJ>  Ocean Beach (14.4K);16192244878;DT*70,;38400;8N1;YES
JJ>  Delphi (2400);2886206;DT*70,;38400;8N1;YES
JJ>  Delphi (9600);2884626;DT*70,;38400;8N1;YES
JJ>  ACS Inc. BBS;14046362991;DT*70,;38400;8N1;YES
JJ> (There are another couple of lines, but this should give you the 
JJ> idea.) I say they're all 38400 bps because the modem is set up to 
JJ> always communicate with me at 38.4 no matter what the far end uses, 
JJ> and the *70, is there to kill call waiting.  With this setup, ladial 
JJ> seems to pause part way through dialing a number, and then the rest 
JJ> of the number  is echoed followed immediately by "NO DIALTONE."
JJ> --- RiBBS v2.10        
Okay, I'll look into it and see what I can do.
Thanks
Alan
 
--- RiBBS v2.10  
 * Origin: Ocean Beach BBS 619-224-4878 MM1 TECH moderator (1:202/343)
