





   ***THE MORGUE:(201)376-4462***






                    Dealing with the Rate & Route Operator

        It seems that fewer and fewer people have blue boxes these days, and
that is really too bad.  Blue boxes, while not all that great for making free
calls (since the TPC can tell when the call was made, as well as where it was
too and from), are really a lot of fun to play with.  Short of becoming a real
live TSPS operator, they are about the only way you can really play with the
network.
        For the few of you with blue boxes, here are some phrases which may
make life easier when dealing with the rate & route (R&R) operators.  To get
the R&R op, you send a KP + 141 + ST.  In some areas you may need to put
another NPA before the 141 (i.e., KP + 213 + 141 + ST), if you have no local
R&R ops.
        The R&R operator has a myriad of information, and all it takes to get
this data is mumbling cryptic phrases.  There are basically four special
phrases to give the R&R ops.  They are NUMBERS route, DIRECTORY route, OPERATOR
route, and PLACE NAME.
        Yo get an R&R an area code for a city, one can call the R&R operator
and ask for the numbers route.  For example, to find the area code for Carson
City, Nevada, we'd ask the R&R op for "Carson City, Neavda, numbers route,
please." and get the answer, "Right... 702 plus." meaning that 702 plus 7
digits gets us there.
        Sometimes directory assitance isn't just NPA + 131.  The way to get
these routings is to call R&R and ask for "Anaheim, Calafornia, directory
route, please." Of course, she'd tell us it was 714 plus, which means 714 + 131
gets us the D.A. op there.  This is sort of pointless example, but I couldn't
come up with a better one on short notice.
        Let's say you wanted to find out how to get to the inward operator for
Sacremento, California.  The first six digits of a number in that city will be
required (the NPA and an NXX).  For example, let us usem 916 756. We would call
R&R, and when the operator answered, say, "916 756, operator route, please."
The operator would say, "916 plus 001 plus."  This means that 916 + 001 + 121
will get you the inward operator for Sacramento.
        Do you know the city which corresponds to 503 640?  The R&R operator
does, and will tell you that it is Hillsboro, Oregon, if you sweetly ask for
"Place name, 503 640, please."
        For example, let's say you need the directory route for Sveg, Sweden.
Simply call R&R, and ask for, "International, Baden, Switzerland.  TSPS
directory route, please."  In response to this, you'd get, "Right... Directory
to Sveg, Sweden.  Country code 46 plus 1170."  So you'd route yourself to an
international sender, and send 46 + 1170 to get the D.A. operator in Sweden.
        Inward operator routings to various countries are obtained the same way
"International, London, England, TSPS inward route, please." and get "Country
code 44 plus 121."  Therefore, 44 plus 121 gets you inward for London.
        Inwards can get you language assitance if you don't speak the language.
Tell the foreign inward, "United Staes calling.  Language assitance in
completing a call to (caled party) at (called number)."
        R&R operators are people are people too, y'know.  So always be polite,
make sure use of 'em, and dial with care.




GF:



9: Text Philez P-Z
+-+UD:Punter
[-]33 Minutes
+-+UnltdBlk:Digital-demon             