OCCIDENTAL CHEMICAL -- DECHLORANE PLUS 515 THE FLAMETAMER 
MATERIAL SAFETY DATA SHEET
FSC: 6850 
NIIN: 00N011596 
Manufacturer's CAGE: 32618 
Part No. Indicator: A 
Part Number/Trade Name: DECHLORANE PLUS 515 THE FLAMETAMER 
===========================================================================
                            General Information
===========================================================================
Company's Name: OCCIDENTAL CHEMICAL CORPORATION 
Company's Street: 360 RAINBOW BOULEVARD SOUTH,SUITE 400 
Company's City: NIAGARA FALLS 
Company's State: NY 
Company's Country: US 
Company's Zip Code: 14302 
Company's Emerg Ph #: 716-278-7021 
Company's Info Ph #: 716-286-3081 
Record No. For Safety Entry: 001 
Tot Safety Entries This Stk#: 001 
Date MSDS Prepared: 24MAY89 
Safety Data Review Date: 01MAR90 
MSDS Serial Number: BJKKF 
===========================================================================
                     Ingredients/Identity Information
===========================================================================
Proprietary: NO 
Ingredient: DECH PLUS.PERCENT:99.90 BY VOL;99.95 BY WT.
Ingredient Sequence Number: 01 
NIOSH (RTECS) Number: IO1430000 
CAS Number: 13560-89-9 
OSHA PEL: N/K (FP N/ORNL) 
ACGIH TLV: N/K (FP N/ORNL) 
Other Recommended Limit: N/K (FP N/ORNL) 
===========================================================================
                     Physical/Chemical Characteristics
===========================================================================
Appearance And Odor: FREE-FLOWING WHITE,ODORLESS POWDER.
Boiling Point: N/A 
Melting Point: 350C,662F 
Vapor Pressure (MM Hg/70 F): SEE SUPP 
Vapor Density (Air=1): N/A 
Specific Gravity: 1.8 (WATER=1) 
Decomposition Temperature: N/K (FP N) 
Evaporation Rate And Ref: N/K (FP N/ORNL) 
Solubility In Water: INSOLUBLE 
pH: SUP DA 
===========================================================================
                      Fire and Explosion Hazard Data
===========================================================================
Flash Point: N/A 
Lower Explosive Limit: N/A 
Upper Explosive Limit: N/A 
Extinguishing Media: NON-FLAMMABLE.USE AGENT SUITABLE FOR SURROUNDING
FIRE.
Special Fire Fighting Proc: USE NIOSH/MSHA APPROVED POSITIVE PRESSURE SCBA
AND FULL PROTECTIVE EQUIPMENT.
Unusual Fire And Expl Hazrds: DECOMPOSITION BY BURNING IN OPEN FLAME MAY
YIELD HYDROGEN CHLORIDE GAS.
===========================================================================
                              Reactivity Data
===========================================================================
Cond To Avoid (Stability): AVOID TEMPERATURES ABOVE 275C,527F.
Materials To Avoid: PROLONGED HEATING IN EXCESS OF 275C,527F ACCELERATES
THERMAL DEGRADATION.
Hazardous Decomp Products: AT TEMPERATURES IN EXCESS OF 275C,527F
DEGRADATION PRODUCTS INCLUDE HYDROGEN CHLORIDE.
Conditions To Avoid (Poly): N/K (FP N/ORNL)
===========================================================================
                            Health Hazard Data
===========================================================================
LD50-LC50 Mixture: LD50 RAT ORAL >25 G/KG;LD50 (SEE SUPP) 
Route Of Entry - Inhalation: YES 
Route Of Entry - Skin: NO 
Route Of Entry - Ingestion: YES 
Health Haz Acute And Chronic: SEE SIGNS AND SYMPTOMS OF OVEREXPOSURE.
Carcinogenicity - NTP: NO 
Carcinogenicity - IARC: NO 
Carcinogenicity - OSHA: NO 
Explanation Carcinogenicity: NONE
Signs/Symptoms Of Overexp: EYES:NO OCULAR EFFECTS HAVE BEEN OBSERVED.
SKIN:NO IRRITANT EFFECTS HAVE BEEN OBSERVED.INGESTION:NOT HIGHLY TOXIC IF
SWALLOWED.INHALATION:DUST MAY CAUSE IRRITATION OF THE RESPIRATORY TRACT.
Med Cond Aggravated By Exp: N/K (FP N/ORNL)
Emergency/First Aid Proc: EYES:FLUSH W/ DIRECTED STREAM OF WATER AT LEAST
15 MIN;HOLD LIDS APART.GET IMMED MED ATTN IF IRRIT OCCURS.SKIN:WASH W/
SOAP,WATER.GET PROMPT MED ATTN IF IRRIT OCCURS.INGEST:NEVER GIVE ANYTHING
BY MOUTH TO UNCON PERSON.GIVE SEVERAL GLASSES OF WATER,THEN TICKLE BACK OF
THROAT W/ FINGER TO INDUCE VOMIT.KEEP AIRWAY CLEAR.SEEK MED ATTN
IMMED.INHAL:REMOVE FROM EXPOS,GIVE SUPPORT TREATMENT IF NEEDED.
===========================================================================
                   Precautions for Safe Handling and Use
===========================================================================
Steps If Matl Released/Spill: SCOOP & SWEEP UP ALL SPILLED PRODUCT & OTHER
CONTAMINATED MATERIAL & PLACE IN MARKED DISPOSAL CONTAINERS.CLEAN UP AREA
ON A DRY BASIS.DO NOT FLUSH TO SEWER.
Neutralizing Agent: N/K (FP N/ORNL)
Waste Disposal Method: DISPOSAL MUST BE IAW FEDERAL,STATE & LOCAL REGS (FP
N).DISPOSE OF SPILLED/WASTE PROD,OTHER CONTAM MATL IN LICENSED LANDFILL OR
BURN IN LICENSED INCIN DESIGNED TO HANDLE HYDROGEN CHLORIDE AS COMBUST
PROD.MATL NOT USED OR REPROCESSED DISP PER REGS.
Precautions-Handling/Storing: STORE IN CLEAN,DRY,WELL VENTILATED AREA AWAY
FROM HEAT.KEEP CONTR CLOSED TO PREVENT CONTAM.USE NORMAL SAFETY PRECAUTIONS
& GOOD INDUS HYGIENE PRAC.
Other Precautions: DO NOT REUSE CONTRS,RESIDUES MAY REMAIN;OBSERVE ALL
LABEL PREC.DISPOSE OF CONTR PER GOVERNMENT REGS.INSURE ADEQ VENT IN WORK
AREA.AVOID EYE CONTACT.DO NOT ALLOW TO ENTER SEWERS OR WATERWAYS.HEATING
>275C,525F CAUSES DEGRADATION,TOXIC GASES.
===========================================================================
                             Control Measures
===========================================================================
Respiratory Protection: NIOSH/MSHA APPROVED RESPIRATOR APPROPRIATE FOR
EXPOSURE OF CONCERN (FP N).
Ventilation: LOCAL AND GENERAL VENTILATION NECESSARY TO KEEP AIR
CONCENTRATION BELOW LEVEL OF CONCERN (FP N/ORNL).
Protective Gloves: RESISTANT SUCH AS COTTON. 
Eye Protection: CHEMICAL WORKERS GOGGLES (FP N). 
Other Protective Equipment: EYE WASH FACILITY SHOULD BE IN CLOSE
PROXIMITY.OBSERVE GOOD WORK PRACTICES.WEAR APPROVED DUST MASK,CLOTHING.
Work Hygienic Practices: WASH CONTAMINATED CLOTHING BEFORE REUSE.WASH
THOROUGHLY AFTER HANDLING.
Suppl. Safety & Health Data: VP:0.006 MMHG @ 200C,392F.PH:7 100 GM/L.
LD50-LC50 MIX:RABBIT DERMAL >8 G/KG;LC50 RAT INHALATION >2.25 MG/L/4 HR.
ROUTES OF ENTRY:INHALATION/SKIN/INGESTION (FP N).
===========================================================================
                            Transportation Data
===========================================================================
Trans Data Review Date:   90347 
DOT PSN Code: ZZZ 
DOT Proper Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
IMO PSN Code: ZZZ 
IMO Proper Shipping Name: NOT REGULATED FOR THIS MODE OF TRANSPORTATION
IATA PSN Code: ZZZ 
IATA Proper Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
AFI PSN Code: ZZZ 
AFI Prop. Shipping Name: NOT REGULATED BY THIS MODE OF TRANSPORTATION
Additional Trans Data: NOT REGULATE FOR TRANSPORTATION
===========================================================================
                               Disposal Data
===========================================================================
===========================================================================
                                Label Data
===========================================================================
Label Required: YES 
Label Status: G 
Common Name: DECHLORANE PLUS 515 THE FLAMETAMER 
Special Hazard Precautions: SEE SIGNS AND SYMPTOMS OF OVEREXPOSURE.
EYES:NO OCULAR EFFECTS HAVE BEEN OBSERVED.SKIN:NO IRRITANT EFFECTS HAVE
BEEN OBSERVED.INGESTION:NOT HIGHLY TOXIC IF SWALLOWED.INHALATION:DUST MAY
CAUSE IRRITATION OF THE RESPIRATORY TRACT.
Label Name: OCCIDENTAL CHEMICAL CORPORATION 
Label Street: 360 RAINBOW BOULEVARD SOUTH,SUITE 400 
Label City: NIAGARA FALLS 
Label State: NY 
Label Zip Code: 14302 
Label Country: US 
Label Emergency Number: 716-278-7021 
=======================================================================
URL for this msds http://hazard.com.  If you wish to change, add to, or
delete information in this archive please sent updates to dan@hazard.com.
